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Nr. 69/2025 

PËR ADERIMIN E REPUBLIKËS SË SHQIPËRISË NË MEMORANDUMIN 
E MIRËKUPTIMIT PËR KONTROLLIN SHTETËROR PORTUAL NË RAJONIN 
E MESDHEUT, BËRË NË MALTË, MË 11 KORRIK 1997

Në mbështetje të neneve 78, 83, pika 1, dhe 121, pika 1, të Kushtetutës, me propozimin e Këshillit të Ministrave, 

KUVENDI
I REPUBLIKËS SË SHQIPËRISË

VENDOSI:

Neni 1

Republika e Shqipërisë aderon në memorandumin e mirëkuptimit për kontrollin shtetëror portual në Rajonin e Mesdheut, bërë në Maltë, më 11 korrik 1997, sipas tekstit që i bashkëlidhet këtij ligji dhe është pjesë përbërëse e tij. 

Neni 2

Ky ligj hyn në fuqi 15 ditë pas botimit në Fletoren Zyrtare.

Miratuar në datën 4.12.2025.

Shpallur me dekretin nr. 494, datë 18.12.2025, të Presidentit të Republikës së Shqipërisë, Bajram Begaj.
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3.3.1

3.3.2

3.4

8.

9.

10.

11

28.
29.
30.
31
32.
33.

If Part Il of the Oil Record Book has not been properly completed, information on the following
guestions may be pertinent:

What was the cargo/ballast distribution in the ship on departure from the last port?

What was the cargo/ballast distribution in the ship on arrival in the current port?

. When and where was the last loading affected?
12.
13.
14.
15.
16.
17.
18.
19.
20.
21.
22.
23.
24.
25.
26.
27.

When and where the last unloading was effected?

When and where was the last discharge of dirty ballast?

When and where was the last cleaning of cargo tanks?

When and where was the last crude oil washing operation and which tanks were washed?
When and where was the last decanting of slop tanks?

What is the ullage in the slop tanks and the corresponding height of interface?

Which tanks contained the dirty ballast during the ballast voyage (if ship arrived in ballast)?
Which tanks contained the clean ballast during the ballast voyage (if ship arrived in ballast)?
In addition the following information may be pertinent:

Details of the present voyage of the ship (previous ports, next ports, trade)

Contents of oil fuel and ballast tanks

Previous and next bunkering, type of oil fuel

Availability or non-availability of reception facilities for oily wastes during the present voyage
Internal transfer of oil fuel during the present voyage

In the case of oil tankers the following additional information may be pertinent:

The trade the ship is engaged in, such as short/long distance, crude or product or alternating
crude/product, lightering service, oil/dry bulk

Which tanks clean and dirty

Repairs carried out or envisaged in cargo tanks

Miscellaneous information:

Comments in respect of condition of ship’s equipment

Comments in respect of pollution report

Other comments

Investigation ashore

Analyses of oil samples

Indicate method and results of the samples’ analyses

Further information

Additional information on the ship, obtained from oil terminal staff, tank cleaning contractors or
shore reception facilities may be pertinent.

Note: Any information under this heading is, if practicable, to be corroborated by documentation
such as signed statements, invoices, receipts, etc.

Information not covered by the foregoing
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3.5.1

3.5.2

3.53

Conclusion
Summing up of the investigator's technical conclusions

Indication of applicable provisions of Annex | of MARPOL 73/78 which the ship is suspected of
having contravened.

Did the results of the investigation warrant the filing of a deficiency report?

Section 4 Contravention of discharge provisions under Annex II to MARPOL 73/78

4.1

4.2

4.3

The provisions of sections 4 and 5 of this Annex are intended to identify information which will be
needed by a flag State Administration for the prosecution of violations of the discharge provisions
under Annex Il to MARPOL 73/78.

It is recommended that in preparing a port State control report on deficiencies, where

contravention of the discharge requirements is involved, the authorities of a coastal or port State

will be guided by the itemized list of possible evidence as shown in section 5 of this Annex. It must

be borne in mind in this connection that:

1. the report aims to provide the optimal collation of obtainable data; however, even if all the
information cannot be provided, as much information as possible must be submitted; and

2. it is important for all the information included in the report to be supported by facts which,
when considered as a whole, would lead the port or coastal State to believe a contravention
has occurred; and

3. The discharge may have been oil, in which case annex 2 to appendix Il of Annex | to MARPOL
73/78 Control Procedures applies.

In addition to the port State control report on deficiencies, a report must be completed by a port
or coastal State, on the basis of the itemized list of possible evidence. It is important that these
reports are supplemented by documents such as:

1. a statement by the observer of the pollution. In addition to the information required in 5.1 of
this Annex, the statement must include considerations which have led the observer to conclude
that none of any other possible pollution sources is in fact the source;

2. statements concerning the sampling procedures both of the slick and on board. These include
location of and time when samples were taken, identity of person(s) taking the samples and
receipts identifying the persons having custody and receiving transfer of the samples;

3. reports of analyses of samples taken of the slick and on board; the reports must include the
results of the analyses, a description of the method employed, reference to or copies of
scientific documentation attesting to the accuracy and validity of the method employed and
names of persons performing the analyses and their experience;

4. a statement by the port State control officer on board together with the port State control
officer's rank and organization;

5. statements by persons being questioned;

statements by witnesses;

7. photographs of the slick; and

o
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8. copies of relevant pages of the Cargo Record Book, log books, discharge recordings, etc.

All observations, photographs and documentation must be supported by a signed verification of
their authenticity. All certifications, authentications or verifications shall be executed in accordance
with the laws of the State which prepares them. All statements must be signed and dated by the
person making the statement and, if possible, by a witness to the signing. The names of the
persons signing statements must be printed in legible script above or below the signature.

4.4 The report referred to in 4.2 and 4.3 of this Annex must be sent to the flag State Administration. If
the coastal State observing the pollution and the port State carrying out the investigation on board
are not the same, the State carrying out the latter investigation must also send a copy of its
findings to the State observing the pollution and reguesting the investigation.

Section 5 Itemized list of possible evidence on alleged contravention of the discharge provisions of
Annex II to MARPOL 73/78

5.1 Action on sighting pollution
5.1.1  Particulars of ship or ships suspected of contravention

Name of ship

Reasons for suspecting the ship

Date and time (UTC) of observation or identification

Position of ship

Flag and port of registry

Type, size (estimated tonnage) and other descriptive data (e.g. superstructure, colour and
funnel mark)

7. Draught condition (loaded or in ballast)

8. Approximate course and speed

9. Position of slick in relating to ship (e.g. astern, port, starboard)

10. Part of the ship from which discharge was seen emanating

11. Whether discharge ceased when ship was observed or contacted by radio

O o e O 1Y B

5.1.2  Particulars of slick

Date and time (UTC) of observation if different from 5.1.1.3 of this Annex

Position of slick in longitude and latitude if different from 5.1.1.4 of this Annex

Approximate distance in nautical miles from the nearest land

Depth of water according to sea chart

Approximate overall dimension of slick (length, width and percentage thereof covered)
Physical description of slick (direction and form, e.g. continuous, in patches or in windrows)
Colour of slick

Sky conditions (bright sunshine, overcast, etc.), light fall and visibility (kms) at the time of
observation

9. Seastate

S0 o Ul g o N e




image90.jpg
5.1.3

5.14

5.1.5

5.2

5.2.1

10. Direction and speed of surface wind
11. Direction and speed of current

Identification of the observer(s)

oy Ul IO

Name of the observer

Organization with which observer is affiliated (if any)

Observer's status within the organization

Observation made from aircraft (ship) (shore) or otherwise

Name or identity of ship or aircraft from which the observation was made

Specific location of ship, aircraft, place on shore or otherwise from which observation was
made

Activity engaged in by observer when observation was made, for example: patrol, voyage,
flight (en route from ... to ...), etc.

Method of observation and documentation

Ul & W s

Visual

Conventional photographs

Remote sensing records and/or remote sensing photographs
Samples taken from slick

Any other form of observation (specify)

Note: A photograph of the discharge must preferably be in colour. The best results may be
obtained with the following three photographs:

.1 details of the slick taken almost vertically down from an altitude of less than 300 metres

with the sun behind the photographer;

.2 an overall view of the ship and “slick” showing a substance emanating from the particular

ship; and

.3 details of the ship for the purposes of identification.

Other information if radio contact can be established

O W1, 0 N =

Master informed of pollution
Explanation of master

Ship's last port of call

Ship's next port of call

Name of ship's master and owner
Ship's call sign

Investigation on board

Inspection of the certificate (CoF or NLS Certificate)

1.
2.

Name of ship
Distinctive number or letters
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5.2.2

5.2.3

5.24

5.2.5

5.2.6

Port of registry

Type of ship

Date and place of issue

Date and place of endorsement

)

Inspection of P and A Manual

List of Annex Il substances the ship is permitted to carry
Limitations as to tanks in which these substances may be carried
Ship equipped with an efficient stripping system

Residue guantities established at survey

ol

Inspection of Cargo Record Book

Sufficient pages of the Cargo Record Book should be copied to cover a full
loading/unloading/ballasting and tank cleaning cycle of the ship. A copy of the tank diagram should
also be taken.

Inspection of log book

Last port, date of departure, draught forward and aft;

Current port, date of arrival, draught forward and aft ;

Ship's position at or near the time the incident was reported ;

Spot check if times entered in the Cargo Record Book in respect of discharges correspond with
sufficient distance from the nearest land, the required ship’s speed and with sufficient water
depth.

B W

Inspection of other documentation on board

Other documentation relevant for evidence (if necessary make copies) such as:
.1 cargo documents of cargo presently or recently carried, together with relevant information
on required unloading temperature, viscosity and/or melting point;
.2 records of temperature of substances during unloading ;
.3 records of monitoring equipment if fitted.

Inspection of ship

Ship's equipment in accordance with the P and A Manual;

Samples taken; state location on board;

Sources of considerable leakage;

Cargo residues on surface of segregated or dedicated clean ballast ;
Condition of pump room bilges;

Condition of monitoring system;

Slop tank contents (estimate quantity of water and residues).

N o W IS
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5.2.7 Statements of persons concerned

If the Cargo Record Book has not been properly completed, information on the following questions
may be pertinent:

Was there a discharge (accidental or intentional) at the time indicated on the incident report?
Which tanks are going to be loaded in the port?

Which tanks needed cleaning at sea? Had the tanks been prewashed?

When and where were these cleaned?

Residues of which substances were involved?

What was done with the tank washing slops?

Was the slop tank, or cargo tank used as a slop tank, discharged at sea?

When and where was the discharge effected?

. What are the contents of the slop tank or cargo tank used as slop tank?

10 Which tanks contained the dirty ballast during the ballast voyage (if ship arrived in ballast)?
11.Which tanks contained the clean ballast during the ballast voyage (if ship arrived in ballast)?
12.Details of the present voyage of the ship (previous ports, next ports, trade)

13.Difficulties experienced with discharge to shore reception facilities

14.Difficulties experienced with efficient stripping operations

15.Which tanks are clean or dirty on arrival?

16.Repairs carried out or envisaged in cargo tanks

17.Miscellaneous information

18.Comments in respect of condition of ship’s equipment

19.Comments in respect of pollution report

20.0ther comments.

CENOU A BN R

5.3 Investigation ashore
5.3.1  Analyses of samples

Indicate method and results of the samples’ analyses
5.3.2  Further information

Additional information on the ship, obtained from terminal staff, tank cleaning contractors or
shore reception facilities may be pertinent

Note: Any information under this heading is, if practicable, to be corroborated by documentation
such as signed statements, invoices, receipts, etc.

5.3.3 Information from previous unloading port terminal

1. Confirmation that the ship unloaded, stripped or prewashed in accordance with its P and A
Manual

2. The nature of difficulties if any

3. Restrictions by authorities under which the ship was permitted to sail
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4. Restrictions in respect of shore reception facilities
5.4 Information not covered by the foregoing

5.5 Conclusion

1. Summing up of the investigator's conclusions;

2. Indication of applicable provisions of Annex Il to MARPOL 73/78 which the ship is suspected of
having contravened ;

3. Did the results of the investigation warrant the filing of a deficiency report?
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ANNEX 3

FACTS REGARDED AS "CLEAR GROUNDS"

1. The Authorities will regard as "clear grounds" inter alia the following:

10.
11.

12.

a report or notification by another Authority;

during examination of the certificates and documents referred to in Annex 11 of the
Memorandum, inaccuracies have been revealed or the documents have not been properly
kept, updated, or they have been falsely maintained;

indications that the relevant crew members are unable to communicate appropriately
with each other, or with other persons on board, or that the ship is unable to
communicate with the shore-based authorities either in a common language of those
authorities;

a certificate has been fraudulently obtained or the holder of a certificate is not the person
to whom that certificate was originally issued;

the ship has a master, officer or rating holding a certificate issued by a country which has
not ratified the STCW Convention;

evidence of cargo and other operations not being conducted safely or in accordance with
the IMO guidelines;

failure of the master of an oil tanker to produce the record of the oil discharge monitoring
and control system for the last ballast voyage;

absence of an up to date muster list, or crew members not aware of their duties in the
event of fire or an order to abandon the ship;

the emission of false distress alerts not followed by proper cancellation procedures;

the absence of principal equipment or arrangements required by the conventions;
evidence from the Port State Control Officer's general impressions and observations that
serious hull or structural deterioration or deficiencies exist that may place at risk the
structural, watertight or weather tight integrity of the ship;

information or evidence that the master or crew is not familiar with essential shipboard

operations relating to the safety of ships or the prevention of pollution, or that such
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13.

14.

15.

16.

17.

operations have not been carried out;

the absence of a table of shipboard working arrangements or records of hours of work or
rest of seafarers;

the ship has changed flag for the purpose of avoiding compliance with the MLC or the ship
flies the flag of a State that has not ratified the MLC, 2006;

there is a complaint alleging that specific working and living conditions on the ship do not
conform to the requirements of the MLC, 2006 or following investigation of an on shore
complaint;

the working and living conditions on the ship do not conform to the requirements of the
MLG;

a report or complaint by the master, a crew member, or any person or
organization with a legitimate interest in the safe operation of the ship shipboard
living and working conditions or the prevention of pollution, unless the Authority
concerned deems the report or complaint to be manifestly unfounded. The identity of the
person lodging the report or the complaint must not be revealed to the master or the

shipowner of the ship concerned.

Following are examples of clear grounds for the control of ships on security aspects:

gl W OB

ISSC is not valid or it has expired.

The ship is at a lower security level than the port.

Drills related to the security of the ship have not been carried out.

Records for the last 10 ship/port or ship/ship interfaces are incomplete.

Evidence or observation that key members of the ship’s personnel cannot communicate
with each other.

Evidence from observations that serious deficiencies exist in security arrangements.
Information from third parties such as a report or a complaint concerning security related
information.

The ship holds a subsequent, consecutively issued Interim International Ship Security
Certificate (ISSC) and in the professional judgement of the inspector one of the purposes

of the ship or company in requesting such a certificate is to avoid full compliance with
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SOLAS 74 Chapter XI-2 and Part A of the ISPS Code, beyond the period of the initial Interim
Certificate. ISPS Code Part A specifies the circumstances when an Interim Certificate may

be issued.

If clear grounds as described above are established, the PSCO shall immediately inform the
competent security authority (unless the PSCO is also an Officer Duly Authorized for Security).
The competent security authority shall then decide on what further control measures are
necessary taking into account the security level in accordance with Regulation 9 of SOLAS 74,
Chapter XI.
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ANNEX 4

INFORMATION SYSTEM ON INSPECTIONS

To assist Authorities in their selection of foreign flag ships to be inspected in their ports it is
necessary to have at the disposal of Authorities up to date information of inspection of an
individual foreign flag ship in one of the other regional ports.

For that purpose the Authorities undertake to provide an Information Centre, preferably by
means of computerizing data transmission, with information on ships inspected in the national
ports, basing themselves on the information set out in Annex 5 to the Memorandum. The
insertion of information into the inspection files should preferably be realized by means of
direct, computerized input on a daily basis.

For the purpose of exchanging rapid information, the information system shall embrace a
communication facility which allows for a direct, computerized exchange of messages
between individual Authorities, including the notifications as referred to in section 3.8 of the
Memorandum and the exchange of information on operational violations as referred in
Section 5 of the Memorandum.

The information as in paragraph 2 and 3 above shall be handled in a standardized form and in
accordance with standardization as set out in the guide for users of the information system
provided by the Information Centre.

The Information Centre will organize the processing of information as in paragraph 2 above so
as to ensure that inspection data are easily accessible both for purposes of consultation and
updating in accordance with procedures as set out in the guide for users of the information
system provided by the Information Centre.

Information for administrative purpose, such as statistical information, will be provided by the
Secretariat under the guidance of the Committee. This will be based on data provided by the
Information Centre.

The information system indicated in the foregoing paragraphs will be implemented as long as
the Memorandum takes effect.

Studies to monitor and, where necessary, to improve the quality of the system will be carried
out on a continuous basis.

Whenever deficiencies are found which lead to the delay or detention of a ship, the port State
Authority will send a copy of the report, as referred to in Annex 5 to the Memorandum, to the
flag Administration concerned.




image98.jpg
ANNEX 5

PUBLICATION OF INFORMATION FOR PSC

Contents

» Report of Inspection in Accordance with the Med MoU on PSC "Form A/1" and "Form A/2"

» Report of Inspection in Accordance with the Med MoU on PSC "Form B"

» NOTIFICATION OF DETENTION OF SHIP

» NOTIFICATION OF RELEASE OF SHIP

» EXCHANGE OF MESSAGES BY REGION AUTHORITIES IN ACCORDANCE WITH
SECTION 3.8 OF THE MEMORANDUM
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REPORT OF INSPECTION IN ACCORDANCE WITH THE

m\ MEDITERRANEAN MEMORANDUM OF UNDERSTANDING FORM A/1
e ON PORT STATE CONTROL'

(Reporting authority) Copy to: - Master

(Name of Office} - head office

(address} - PSCO

(telephone} if ship is detained, copy to:

(fax) - flag State

(e-mail} - recognized organization, if applicable

HIP PARTICULARS

12

1. Name of ship............ 2. Flagofship ...

Type of ship ......... 4. call sigh e

IMO number 6. Grosstonnage ...

Deadweight (where applicable

3
5
7. Date keel laid / major conversion commenced ........
8
9

Full particulars of company (identical to particulars as in the SMC)**?

IMO Company number: ...... I TV vt B T T S P S
Address: ...
City: ...... COUNEINS s oomconssssmocsmms sy spaon secsams esse

10. Name and signature of master to certify that the information under 9 is correct:

Signature ...

11. Date of boarding ship 12. Place of inspection

13. If vessel is detained: Date of issue of detention notice: ........... ....Duration of Detention:.......

14. Date of report: ...

15. Type of inspection: O Initial inspection O More detailed Inspection O Expanded inspection O (CLCH:

L This inspection report has been issued solely for the purpose of informingthe master and other port States that an inspection by the port State, mentioned in the heading, has taken place. This inspection report cannot be construed
as a seaworthiness certificate in excess of the certificates the ship is required to carry.

2 Non-IsM ships: Master to supply and sign under 10. for correct full particulars of company.
3 Masters, Shipowners and/or Operators are advised that detailed information on the inspection may be subject to publication {(www.medmou.org

4 Concentrated Inspection Campaign, a separate questionnaire should be filed up and recorded into THETIS-Med.
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Annex 5 to the Mediterranean MoU

FORM A/2

16. Follow-Up of inspection(s) :
Nr. Visit date Inspection Team Observations
1

2

17. Operational controls { if any):

OO OO oo s enimm s e s s e e O  CommUNcation EOUIPIMENT .............oooeioorie oo emsmmss cmsos e emmss oninns O ‘Abandonship:drl

R O Ol filtering @QUIPMENt ..........coooom s eciee oo ion e s e s s O Emergency fire pump

O DEMAEE CONIOL c.cocvivuis i sienieiicisinimminises sostin i s st siess O EMERZENCY BENEIATOT ......ce e corveesee e servemres e emessem et s ses et s sene O Emergency steering
18. Relevant certificate(s)
b. Issuing c. Dateof d. Date of e. Information on Last intermediate, periodical, or annual survey

Authority issue expiry Date of survey Surveying Authority Country

a. Title

4
=]

W o ~N oW NP
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FORM A/3

19. Classification society (ies) responsible for issuance of class certificates:
Issued on: .. Expired on: ..o
Issued on: .. EXpired on: e
20. Recognized Organization {s) responsible for issuance of certificates on behalf of the flag State:
21. Ship related inspection action taken:
OO Flag State administration informed O Inspection done at sea [0 Observations to inspection
O Coastal State informed O Inspection suspended O Excluded AFS grounds
O Recognized Organization informed O Dismissed on AFS grounds 0 MARPOL investigation of contravention of discharge provision
OO Next port of call informed O Vessel expelled on security O The flag State has been requested an action plan within a deadline
O 1Lo informed [0 Vessel expelled on other grounds O Overriding Factor
O Union representative informed [T Other @UROIILY INFOIMEU ....couueveceveeee st cessssees sesess s sss e sess s s st sssees e sbs s bas et sens st nn s s et s
22. Deficiencies O no O yes (see attached FORM B)
23. Supporting documentation O no O yes (see annex)
PORT STATE PARTICULARS

District office

Address

Telephone

Fax

E-mail

Name(s):

This report must be retained on board for a period of at least two years and must be readily available for consultation by Port State Control Officers at all times.

(duly authorized PSCO of reporting authority})
Signature
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REPORT OF INSPECTION IN ACCORDANCE WITH THE
MEDITERRANEAN MEMORANDUM OF UNDERSTANDING FORM B
ON PORT STATE CONTROL

(Reporting authority} Copy to: - Master
(address) - head office
(telephone}) - PSCO

(fax} if ship is detained, copy to:
(e-mail) - flag State

- recognized organization, if applicable

1. Name of ship. 2. IMO number. 3. Date of report.. 4. Place of inspection.

Deficiencies found and follow up actions™

Code Defective item Nature of defect ! Convention ref.? Ground.for {AT) Due Date Additional comments RO AD ISM
detention
O O o O
O O o O
O O o o0
O O o O
O O o o0
O O o O
O O o O
O O o O
O O o O
O O o o
O O o O
O O o O
O O o O
O O o O
O O o o0
O O o O
O O o O

Name(s):
(duly authorized PSCO of reporting authority)

Signature(s)

ek
Masters, Ship owners and/or Operators are advised that detailed information on the inspection may be subject to publication {www.medmou.org)
L This inspection was not a full survey and deficiencies listed may not be exhaustive. In the event of a detention, it is recommended that a full survey is carried out and all deficiencies are rectified before an application for re
inspection is made.

2 To b I
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ﬂ\ PORT STATE CONTROL
e NOTIFICATION OF DETENTION OF SHIP'

Flag State / Consulate

Classification society/recognized organization
Fax no.

E-mail

Number of pages, incl. this

Dear Sir / Madam,

[Ship’s name, flag, IMO No.] — Detention of ship

The oo Maritime Authority have on [date] carried out an inspection of
the above ship at [Port, country].

The ship is detained at [time of detention] hours due to the following detainable deficiencies:

9 .
10.

Enclosed please find a copy of the Report of inspection forms A & B.

For further inquiries, please contact: [ Name and contact details ]

Yours faithfully,

* As per IMO-MSC/Circ.1011 and MEPC/Circ.383
INCERT AT THE BACK OF THE PRESENT DOCUMENT THE DEDICATED APPEAL PROCEDURE

Revision 2




image104.jpg
Jﬁ\ PORT STATE CONTROL
- NOTIFICATION OF RELEASE OF SHIP

Flag State / Consulate

Classification society/recognized organization
Fax no.

E-mail

Number of pages, incl. this

Dear Sir / Madam,

[Ship’s name, flag, IMO No.] — Release of ship

The i Maritime Authority have on [date] carried out a re-inspection of the

above ship at [Port, country].

The ship was released at [time of release] hours.

[Insertion of free text, if any]

Enclosed please find a copy of the Report of inspection forms A & B.

Yours faithfully,

* As per IMO-MSC/Circ.1011 and MEPC/Circ.383
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EXCHANGE OF MESSAGES BY REGION AUTHORITIES IN ACCORDANCE WITH
SECTION 3.8 OF THE MEMORANDUM

1

In the case of deficiencies not fully rectified or only provisionally repaired, a message shall be
sent to the competent Authority of the region State where the next port of call of the ship is
situated.

The exchange of messages, as in paragraph 1 above, shall take effect through the use of the
communication facilities incorporated in the information system as described in Annex 4 and/or
by facsimile on the form contained in the Appendix to this Annex.

Each message as in paragraph 1 above, shall contain the following information:

» date:

from (country):

port:

to (country):

port:

a statement reading deficiencies to be rectified:
name of ship:

IMO identification number (if available):
type of ship:

flag of ship:

call sign:

gross tonnage:

year of build:

issuing Authority of relevant certificate(s):
date of departure:

estimated place and time of arrival:

nature of deficiencies:

action taken:

suggested action at next port of call:

name and facsimile number of sender.

VVVVVVVVVVVVVVVVYVVY
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ANNEX 6

QUALITAITVE CRITERIA FOR ADHERENCE TO THE MED MOU

Maritime Authority of a State may adhere as a full member, provided that all of the following
gualitative criteria have been met:

Such Maritime Authority shall explicitly subscribe to the commitments under the Memorandum
with a view to contributing to the common endeavour to eliminate the operation of substandard
ships;

Such Maritime Authority shall take all necessary measures to encourage the ratification of all
relevant instruments in force. Port State Control shall not be applied by such Maritime Authority to
those instruments it has not yet ratified.

Such Maritime Authorities shall have sufficient capacity, logistically and substantially, to
appropriately enforce compliance with international maritime standards regarding maritime safety,
pollution prevention and living and working conditions on board with regard to ships entitled to fly
its flag, which shall include the employment of properly qualified inspectors acting under the
responsibility of its Administration, to be demonstrated to the satisfaction of the Committee
referred to in 6.1 of the Memorandum;

Such Maritime Authority shall have sufficient capacity, logistically and substantially, to comply in full
with all provisions and activities specified in the Memorandum in order to enhance its commitment,
which shall include the employment of properly qualified port State control officers acting under the
responsibility of its Administration, to be demonstrated to the satisfaction of the Committee
referred to in 6.1 of the Memorandum;

Such Maritime Authority shall, as of its effective date of membership, establish an online connection
to the information system referred to in Annex 4;

Such Maritime Authority shall sign a financial agreement for paying its share in the operating cost of
the Memorandum and shall, as of its effective date pay its financial contribution to the budget as
approved by the Committee referred to in 6.1 of the Memorandum.
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ANNEX 7

PORT STATE CONTROL OFFICER CRITERIA AND REQUIREMENTS

Contents
Section 1 Qualification Criteria for Port State Control Officers

Section 2 Requirements for the Identity Card for Port State Control Inspectors
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Section 1 QUALIFICATION CRITERIA FOR PORT STATE CONTROL OFFICERS

1. In pursuance of the provisions of 3.5 of the Memorandum, the port State control officer must be
properly qualified and authorized by the Authority to carry out port State control inspections
[without prejudice to national provisions].

2, A properly gualified port State control officer must have completed a minimum of one year's
service as a flag State surveyor dealing with surveys and certification in accordance with the
relevant instruments and be in possession of:

1. a certificate of competency as master, enabling that person to take command of a ship of
1,600 tons gross tonnage or more (see STCW, Regulation 1I/2), or

2. a certificate of competency as chief engineer, enabling that person to take up that task on board
a ship whose main power plant has a power equal or superior to 3,000 kW (see STCW,
Regulation 111/2), or

3. has passed an examination recognized by the Authority as a naval architect, mechanical
engineer or an engineer related to the maritime fields and worked in that capacity for at least
5 years.

The port State control officers mentioned under 2.1 and 2.2 above must have served for a period of
not less than five years at sea as officer in the deck or engine department.

3. Alternatively, a port State control officer is deemed to be properly qualified if that person:

1. holds a relevant university degree or an equivalent training, and

has been trained and qualified at a school for ship safety inspectors, and

3. has served at least 2 years as a flag State surveyor dealing with surveys and
certification in accordance with the relevant instruments.

I

4., A properly qualified port State control officer must be able to communicate orally and in writing
with seafarers in the language most commonly spoken at sea.

5. A properly qualified port State control officer must have appropriate knowledge of the provisions
of the relevant instruments and of the relevant procedures on port State control.

6. A properly gualified port State control officer must remain updated with the new relevant
instruments and regulations. In achieving the goal of retaining and updating their knowledge the
PSCO should use the Distance Learning Programs available.

7. Port State control officers not fulfilling the above criteria are also accepted if they are employed
for port State control by the Authorities before 1 July 1996.
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Section 2 REQUIREMENTS FOR THE IDENTITY CARD FOR PORT STATECONTROL INSPECTORS
1. The identity card shall contain at least the following information:

name and issuing Authority;

full name of the holder of the identity card

an up to date picture of the holder of the identity card;

the signature of the holder of the identity card;

a statement to the effect that the holder of the identity card is authorized to carry out
inspections in accordance with the national legislation.

Ui O3 =

2. If the main language used on the identity card is not English, it must include a translation into that
language.

3, The format of the identity card is left to the discretion of the competent Authorities.
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ANNEX 8
APPEAL AND REVIEW PROCEDURES

Appeal Procedure

Section 3.13 of the Med MoU memorandum states that "the owner or the operator of a
ship will have the right of appeal against a detention decision to higher administrative
Authority or to the Court of competent jurisdiction, according to the law in each
country. However, an appeal shall not cause the detention to be suspended.”

Owners or operators are advised to use the official Authority’s procedure if they wish to
appeal against a detention order. The basic appeal procedures in the Med MoU member
States are listed in the document called: Appeal procedures in Med MoU member States
(as published on the website www.medmou.org).

Review Procedure

In case an owner or operator declines to use the Authority’s official appeal procedure but
still wishes to complain about a detention decision, such a complaint should be sent to
the flag State or the Recognised Organisation (if authorized to act for the flag State).

The flag State or Recognised Organisation may then ask the port State to reconsider its
decision to detain the ship.

In such cases the port State should investigate the decision and inform the flag State or
the Recognised Organisation of the outcome. If the port State agrees to reserve its
decision it should also inform the Med MoU database manager and the Med MoU
Secretariat.

If the flag State or the Recognised Organisation disagrees with the outcome of the
investigation as mentioned above, a request for review may be sent within 90 days, from
the date of detention to the Med MoU Secretariat. Such a request should be
accompanied by all information relevant to the detention in electronic format
{submission by E-mail to: secretariat@medmou.org) and in English language.

The Secretariat will set up a "Review Panel: comprising of the Secretariat as Coordinator
and 3 MoU Authorities requested on an alphabetically rotating basis, excluding the port
and flag State. The Secretariat will also inform the port State of the request of review
and invite the port State to submit relevant information in electronic format.

The Review Panel will consider the procedural and technical aspects of the inspection
based on the information provided by the flag State and / or the Recognised Organisation
and the port State. The Review Panel members return their opinions to the Secretariat.
Should additional information been required, the Secretariat will arrange this information
to be provided to all Review Panel members. The detail of correspondence is kept as an
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internal matter. The Review Panel findings represent a majority opinion

The Secretariat will prepare a summary of the opinions of the Review Panel and will
inform the flag State or the Recognised Organisation, as appropriate, the port State and
the MoU advisory Board.

If the view of the Review Panel supports the flag State or the Recognised Organisation’s
complaint, the port State will be requested to reconsider its decision again.

The findings of the Review Panel are not binding but could provide justification for the
port State to amend its inspection data already inserted in the database and to inform
the database manager and the Secretariat accordingly. The Secretariat will inform the
flag State or Recognised Organisation, as appropriate on the action (not) taken by the
Port State.

The findings of Review Panel could not be used as a ground for claiming a financial
compensation.
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ANNEX 9
SELECTION CRITERIA (TARGET FACTOR)

The calculation of the Target Factor is divided into two parts:
1. Generic Factor, based on elements of the ships profile.
2. History Factor, based on the ships inspection history in the Med MoU

Generic Factor

The Generic Factor for an individual ship is calculated by adding together the relevant
elements of its profile:
e Targeted flag
Targeted ship type
Non IACS member classification society
Ships age

The Generic Factor is updated when the particulars of the ship change or the status of its
existing flag change.

History Factor

The History Factor is applied to the Generic Factor to reflect the actual condition of the
ship found following PSC inspections.

The History Factor is calculated by applying the elements below to each Med MoU
inspection of the ship carried out:

e Inspection interval

e Detained

e Number of deficiencies

e Outstanding deficiencies

The Overall Target Factor is calculated by adding the Generic and History Factor but it
cannot be less than the Generic Factor.

Regardless of the target factor value the following ships shall be considered as overriding
priority for inspection:

1. Ships which have been reported as overriding priority by pilots or port authorities
in accordance with section 1.5 of the Memorandum;

2. Ships carrying dangerous or polluting goods, which have failed to report all
relevant information concerning the ship's particulars, the ship’s movements and
concerning the dangerous or polluting goods being carried to the competent
authority of the port and coastal State;

3. Ships which have been the subject of a report or notification by another
Authority;

4. Ships which have been the subject of a report or complaint by the master, a crew

member, or any person or organization with a legitimate interest in the safe
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operation of the ship, shipboard living and working conditions or the prevention
of pollution, unless the Authority concerned deems the report or complaint to be
manifestly unfounded; the identity of the person lodging the report or complaint
must not be revealed to the master or the shipowner of the ship concerned;
5. Ships which have been:
i.  involved in a collision, grounding or stranding on their way to the
port,

ii. accused of an alleged violation of the provisions on discharge of
harmful substances or effluents,

iii.  maneuvered in an erratic or unsafe manner whereby routing
measures, adopted by the IMO, or safe navigation practices and
procedures have not been followed, or

iv.  otherwise operated in such a manner as to pose a danger to
persons, property or the environment;

6. Ships which have been suspended or withdrawn from their class for safety
reasons in the course of the preceding 6 months;
7. Ships which cannot be identified in the THETIS-Med' information system.

The Authorities will give priority for inspection to the ships with the higher Target Factor
as indicated by the THETIS-Med' system. The criteria and their weight are indicated in
table 1 of this annex. The Target Factor of the ship will be the sum of all applicable
criteria points. Full implementation of the targeting System will become applicable when
statistical data for all criteria is available in the THETIS-Med' system. The following
elements are relevant for the targeting factor:

.1 Ships visiting a port of a State, the Authority of which is a signatory to the
Memorandum, for the first time or after an absence of 12 months or more.

.2 Ships not inspected by any Authority within the previous 6 months;

.3 Ships whose statutory certificates on the ship’s construction and equipment,
issued in accordance with the Conventions, and the classification certificates,
have been issued by a non IACS organization;

.4 Ships flying the flag of a State appearing in the blacklist as published in the annual
report of the MoU;

.5 Ships which have been permitted by the Authority to leave a port of its State on
certain conditions:

i. deficiency to be rectified before departure;
ii. deficiency to be rectified at the next port;
iii. deficiencies to be rectified within 14 days;
iv. deficiencies for which other conditions have been specified;
v. if ship related action has been taken and all deficiencies have been
rectified;

.6 Ships for which deficiencies have been recorded during a previous inspection,
according to the number of deficiencies;

.7 Ships which have been detained in a previous port;

.8 Ships flying the flag of a non-party to a relevant instrument;

iPSCC23/16

be THETIS-Med
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.9 Other ships above 13 years old.

TABLE 1

CRITERIA

TARGET FACTOR

Ship Age

0 - 5years: 0 point

6 - 10 years: 5 points

11-15 years: 10 points

16 - 20 years: 10 + 1 point for each year
exceeding 15 years

>20 vyears: 15 + 2 points for each year
exceeding 20 years

Ship type

4 points for ships with type codes 13, 30, 40,
55, 60, 61, 70,71
and of 15 years of age and over 0 points for all
others

Ship flag - Excess of average detention, based
upon 3 year rolling average figure

+1 point for each percentage
point in excess (decimal number rounded up)

0.6 points for each deficiency found in last 4

Deficiencies initial inspections or follow up with new
deficiency (decimal number rounded up)
Depending on number of detentions
in last 4 inspections:
1 detention - 15 points

Detentions

2 detentions - 30 points
3 detentions - 60 points
4 detentions - 100 points

Classification Society
IACS

-non

10 points

Outstanding deficiencies
(A deficiency recorded in the THETIS-Med' in
the last inspection and not marked as rectified

2 points for each outstanding deficiency

{Codel0))
Time since last inspection:
6-12 months 3 points
12 - 24 months 6 points
Over 24 months or never inspected in Med 50 points

MoU region (including new ships)

Calculation method

The target factor is the sum of the TFV Values
Calculated daily

Priority level
Target Factor
101 -
41-100
11-40
0-10

Priority 1 (very high)
Priority 2 (high)
Priority 3 (medium)
Priority 4 (low)
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ANNEX 10
REFUSAL OF ACCESS

General Provisions

In accordance with section 3.8.2 of the Memorandum the Mediterranean MoU States
must refuse access to their ports to ships which have:
1. proceeded to sea without complying with the corrective measures laid down by
the detaining port (jumped detention);
2. not called at the indicated repair yard;

The ban may only be lifted following a reinspection of the ship at the company’s expense
at an agreed port by PSCO’s of the banning State and if evidence is provided to its
satisfaction that the vessel fully complies with the applicable requirements of the
International Conventions.

A port State may permit the access of a ship in the event of force majeure or overriding
safety considerations or to reduce or minimize the risk of pollution or to have deficiencies
rectified.

Procedures for the following cases as well as suggested communication documents are
described below:

1. Allowing a ship to sail to a repair yard;

2. Actions if a ship fails to arrive at an agreed repair yard;

3. Actions if a ship fails to comply with the detention order (jumped detention).

Procedure For Allowing A Ship To Sail To An Agreed Repair Yard

The flag State or Recognized Organization acting on behalf of the flag State must confirm
in writing that the ship is permitted to proceed to the nearest available and appropriate
repair port and advise any conditions for the voyage (see letter “Request For Agreement
To Proceed To A Repair Yard”). The designated repair yard must be acceptable by the flag
state / RO and the PSC authority. The conditions for release must be acceptable to the
port State that may impose additional conditions.

The flag State or recognized organization acting on behalf of the flag State must also issue
single voyage certificates or preferably endorse existing certificates. The voyage will be in
ballast and exclude any commercial operations. Exceptionally, cargo already on board
may be carried to the repair port, or specified intermediate ports, when it is safe to do so.
These ports should be included in the conditions of release (see letter “Conditions Of
Release from Detention to a Repair Port”) and be informed if they would accept the
vessel.

The company and / or Master must provide to the PSC Authority written confirmation of a
repair yard contract or supply of equipment as appropriate.
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The agreed repair yard will be in a port in which follow up action will be taken and before
releasing the ship the PSCO should obtain confirmation in writing from the relevant port
State authority that the ship will be accepted and that they will adhere to the MoU
communication procedure (see letter “Request For Agreement To Proceed To A Repair
Yard”)

The master must be informed in writing of the conditions of release. The master must also
be advised that the ship may be banned if it does not comply with these conditions or
does not call at the repair port (see letter “Conditions Of Release from Detention to a
Repair Port).

The master must be informed in writing that, as a condition of release, the detaining port
must be notified by the port State control authority of the repair port in writing
immediately that the ship has arrived at the agreed repair yard (see letter “Conditions Of
Release from Detention to a Repair Port). If a notification is not send the detaining port
may proceed with the issuance of a Refusal of Access order.

The PSC inspection form is to make clear to which port the ship is allowed to sail and its
ETA.

The port State control authority of the repair port, the flag State and the recognized
organization should be informed of the departure of the vessel and its ETA at the repair
port (see letter “Conditions Of Release from Detention to a Repair Port)

Procedure If A Ship Fails To Call At An Agreed Repair Yard

If a ship fails to call at the agreed repair yard or fails to arrive at the prearranged time the
ship is liable for banning. The decision to apply a ban is for the detaining port State,
following confirmation that the ship has not called at the agreed repair yard or fails to
comply with the conditions of release (including the notification of arrival) or has not
otherwise complied with the detention order. Before issuing the Refusal of Access order
the detaining State may reguest consultations with the flag State Administration of the
ship.

When a ban is applied, the Maritime Authority of the banning State will advise the ISM
Company that the ban is in place. This letter will be copied to the flag State, recognized
organization(s), classification society(ies), Med MoU members, Med MoU Secretariat, the
THETIS-Med' manager, Secretariats of cooperating MoU’s and USCG. The database
manager must be informed through the information system.

Notification of a banned ship will appear on the ship’s identification screen on the
THETIS-Med' information system and the list of banned ships on the Med MoU website
will be updated simultaneously.

In the case of a ship banned for not complying with the conditions for a safe, single voyage
to a repair yard a formal request by the ISM company for the ban to be lifted must be
made to the banning State. The ban may only be lifted following a re inspection of the ship
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at the company’s expense at an agreed port by PSCO’s of the banning State and if
evidence is provided to its satisfaction that the vessel fully complies with the applicable
reguirements of the International Conventions.

If the agreed port of re inspection is in the Med MoU region, the port State authority of
that port may, with the agreement of the banning port State, authorise the ship to
proceed thereto, for the sole purpose of verifying that the ship meets the conditions
specified in paragraph 4. When the banning State and the ISM company agree to re
inspect in a port outside the Med MoU region, the company will consult with that port
State to agree access and if so the company will send written confirmation to the banning
State. The decision to lift the ban shall remain with the banning State.

All costs related to the re inspection of a banned ship will be borne by the ISM company.
If the re inspection has no satisfactory results the ban will not be lifted.

If the ship is in a port outside the jurisdiction of the PSCO carrying out the re inspection
and the PSCO believes the ship is in a detainable condition then PSCO has to inform the
port State where the ship lies so that it may consider action to detain the ship. If the ship
does not comply with the requirements the ban will not be lifted.

In order to have the ban lifted, the company must address a formal request to the port
State authority of the Member State that imposed the ban. This request must be
accompanied by:

1. a document from the flag State administration showing that the ship fully
conforms to all the provisions of the applicable international conventions. The
document may be in the form of an official statement but it must be issued by the
flag administration and not a recognized organization.

2. a document from the classification society(ies) classing the ship that the ship
conforms to the class standards stipulated by that society(ies). The classification
society(ies) must also provide evidence that an on board visit has taken place prior
to issue of the document, if appropriate

If the re inspection provides evidence to the satisfaction of the banning State that the ship
fully complies with all the reguirements of the Conventions the ban will be lifted. The
company will be informed of the lifting of the ban by the banning State. This letter will be
copied to the flag State, recognized organization(s), classification society(ies), Med
MoU members, Med MoU Secretariat, THETIS-Med' manager, Secretariats of cooperating
MoU’s and USCG.

The THETIS-Med' will remove the notification from ship’s identification screen. The ship
will be removed from the banned list on the Med MoU website simultaneously.

The company has a right of appeal against the banning in accordance with the port States
own legislation.
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PORT STATE CONTROL

REQUEST FOR AGREEMENT TO PROCEED TO A REPAIR YARD

From: (PSC office of (port)) Sax:
To: (Port State Authority of repair yard)
(Flag State Authority)

cc:  (Recognized organization issuing the relevant certificates)

Ship Name IMO No Flag oo

Call sign Year of keel laid

Type of Ship oo Callsign o

Gross Tonnage __

Recognised Organization(s) __..................... Classification Society(16S) ..o

The above named vessel is detained in (port)  but cannot rectify all deficiencies. The vessel has requested that the
following deficiencies are repaired in (port ).

Deficiencies that cannot be repaired Suggested action:
in the present port (including action at next port)

Before releasing the vessel this Authority requests:

1. the PSC Authority for the port of [name] to confirm by fax or email if the above mentioned ship is permitted to call in
that port and that a follow up inspection will be carried out;
2 the Flag State Authority (if necessary through its recognized organization) to confirm by fax that the above mentioned
ship is permitted to proceed to (port) and any conditions for the voyage.
Reporting AUthOTItY e OFfICe: e
Fax:
Email:
Tel:
Date:

Name & Signature
(duly authorized Port State Control Officer)




image119.jpg
ANNEX 11
LIST OF CERTIFICATES TO BE VERIFIED

During an inspection the PSCO will as a minimum and to the extent applicable examine the following

documents:

005 1S

N R

10.
11.
12.
13.

14.
15.
16.
17.
18.
19.

20.
21.
22,
23.
24.

25.

26.

International Tonnage Certificate (1969) (ITC, Art.7);

Certificate of Registry or other document of nationality (UNCLOS);

Certificates as to the ship's hull strength and machinery installations issued by the classification
society in question (only to be required if the ship maintains its classwith a classification society);
Reports of previous port State control inspections;

Passenger Ship Safety Certificate (SOLAS 1988 Amend./Cl/Reg.12, SOLAS Protocol 1988/Cl/Reg.12);
Cargo Ship Safety Construction Certificate (SOLAS/Cl/Reg.12, SOLAS Protocol 1988/Cl/Reg.12);

Cargo Ship Safety Equipment Certificate (SOLAS 1988 Amend./Cl/Reg.12, SOLAS Protocol
1988/Ci/Reg. 12);

Cargo Ship Safety Radio Certificate (SOLAS 1988 Amend./Ci/Reg.12, SOLAS Protocol 1988/Cl/Reg.12);
Cargo Ship Safety Certificate (SOLAS Protocol 1988/Ci/Reg. 12);

Special Purpose Ship Safety Certificate (SPS Code, C1/Art.1.7.4, Res. A.791 (19));

For ro-ro passenger ships, information on the A/A-max ratio (SOLAS 1995 Amend./Cli-1/Reg.8-1);
Damage control plans and booklets (SOLAS 2006 Amend./ClI-1/Reg.19, 20, 23);

Stability Booklet and information (SOLAS 2008 Amend/Cil-1/Reg.5, SOLAS/CIi-1/Reg.22, LLP8S,
Reg.10);

Manoeuvring Booklet and information (SOLAS 1981 Amend./Cll-1/Reg.28.2);

Unattended Machinery spaces (UMS) evidence (SOLAS 1981 Amend./Cli-I/Reg.46.3);

Exemption Certificate and any list of cargoes (SOLAS/CII-2/Reg.10.7.1.4);

Fire control plan (SOLAS 2000 Amend./ClI-2/Reg.15.2.4);

Fire safety operational booklet (SOLAS 2000 Amend./Cli-2/Reg.16.3.1);

Dangerous goods special list or manifest, or detailed stowage plan (SOLAS 2000 Amend./Cli-
2/Reg.19);

Doc. of compliance Dangerous Goods (SOLAS 2001 Amend./Cli-2/Reg.19.4);

Ship’s log book with respect to the records of drills, including security drills, and the log for records
of inspection and maintenance of lifesaving appliances and arrangements and fire fighting
appliances and arrangements (SOLAS 2006 Amend./Clli/Reg.37,19.3, 19.4, 20);

Minimum Safe Manning Document (SOLAS 2000 Amend./CV/Reg.14.2);

SAR coordination plan for passenger ships trading on fixed routes (SOLAS 1995 Amend./CV/Reg.15,
7.2);

LRIT Conformance Test Report (SOLAS/CV/Reg.19.1);

Copy of the Document of compliance issued by the testing facility, stating the date of compliance
and the applicable performance standards of VDR (voyage data recorder)

(SOLAS/CV/Req.18.8);

AlS test report (SOLAS 2010 Amend./CV/Reg.18.9);
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27.
28.
29.
30.
31
32.
33.

34,

35.

36.

37.
38.

39.

40.
41.
42.
43.
44,

45.

46.

47.

48.

49.
50.

51.
52.

For passenger ships, List of operational limitations (SOLAS 2001 Amend./CV/Reg.30.2);

Cargo Securing Manual (SOLAS 2002 Amend./CVi/Reg.5.6);

Bulk Carrier Booklet (SOLAS 1996 Amend./CVI/Reg.7.3);

Loading/Unloading Plan for bulk carriers (SOLAS 1996 Amend./CVi/Reg.7.3);

Document of authorization for the carriage of grain (SOLAS 1991 Amend./CVI/Reg.9);

Material Safety Data Sheets (MSDs) (SOLAS 2009 Amend./CVi/Reg.5-1);

INF (International Code for the Safe Carriage of Packaged Irradiated Nuclear Fuel, Plutonium and
High-Level Radioactive Wastes on Board Ships) Certificate of Fitness (SOLAS 1999
Amend./CVil/Reg.16, INFC 1.3);

Copy of Document of Compliance issued in accordance with the International Management Code
for the Safe Operation of Ships and for Pollution Prevention (DoC) ISM Code (SOLAS 1994
Amend./CiX/Reg.4.1);

Safety Management Certificate issued in accordance with the International Management Code for
the Safe Operation of Ships and for Pollution Prevention (SMC) (SOLAS 1994 Amend./CiX/Reg.4.2,
4.3);

High Speed Craft Safety Certificate and Permit to Operate High Speed Craft (SOLAS 1994
Amend./CX/Reg.3.2, HSCC 1.8.1, 2);

Continuous Synopsis Record (SOLAS 2005 Amend./CXI-1/Reg.5);

International Certificate of Fitness for the Carriage of Liquefied Gases in Bulk, or the Certificate of
Fitness for the Carriage of Liquefied Gases in Bulk, whichever is appropriate (GCC-4/Cl/N1.6.4,
IGCC/CI/N1.5.4);

International Certificate of Fitness for the Carriage of Dangerous Chemicals in Bulk, or the
Certificate of Fitness for the Carriage of Dangerous Chemicals in Bulk, whichever is appropriate
(BCC-10/Cl/N1.6.3, IBCC/CI/N1.5.4, BCH/I/1.6.1);

International Oil Pollution Prevention Certificate (MARPOL/ANI/Reg.7.1);

Survey Report Files (in case of bulk carriers or oil tankers) (SOLAS XI-1 reg.2, 2011 ESPcode);

Oil Record Book, parts | and || (MARPOL/ANI/R17, Reg.36);

Shipboard Marine pollution emergency plan for Noxious Liquid Substances (MARPOL/ANII/Reg.17);

{Interim) Statement of compliance Condition Assessment Scheme (CAS) (MARPOL/ANI/Reg.20.6,
21.6.1);

For oil tankers, the record of oil discharge monitoring and control system for the lastballast voyage
(MARPOL/ANI/Regq.31.2);

Shipboard Oil Pollution Emergency Plan (SOPEP) (MARPOL/ANI/Reg.37.1);

STS Operation Plan and Records of STS Operations (MARPOL ANI/Reg.41);

International Pollution Prevention Certificate for the Carriage of Noxious LiquidSubstances in Bulk
(NLS) (MARPOL/ANII/Reg.9.1);

Cargo Record Book (MARPOL/ANII/Reg.15, MARPOL/ANII-Appendix2);

Procedures and Arrangements Manual (chemical tankers and NLS tankers) (MARPOL/ANII/Reg.14.1
+ P&A manual);

International Sewage Pollution Prevention Certificate (ISPPC) (MARPOL/ANIV/Reg.5.1);

Garbage Management Plan (MARPOL/ANV/Appendix 1);
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53.
54.
55.
56.
57.
58.
59.
60.
61.
62.
63.
64.
65.
66.
67.

68.

69.
70.

71.

72.

73.

74.
75.

76.

77.
78.
79.
80.
81.
82.
83.

Garbage Record Book (MARPOL/ANV/Appendix Ii};

International Air Pollution Prevention Certificate (IAPPC) (MARPOL/ANVI/Reg.6.1);

Logbook for fuel oil change-over (MARPOL/ANVI/Reg.14.5);

Type approval certificate of incinerator (MARPOL/ANVI/Reg.16.6.1 + Appendix IV(1));

Bunker delivery notes (MARPOL/ANVI/Reg.18.5+ Appendix V);

International Energy Efficiency Certificate (MARPOL/ANVI/Reg.6);

Ship Energy Efficiency Management Plan (SEEMP) (MARPOL/ANVI/Reg.22);

EEDI Technical File (MARPOL/ANVI/Reg. 20);

Statement of Compliance — Fuel Oil Consumption Reporting (MARPOL/ANVI/Reg.6);

Engine International Air Pollution Prevention Certificate (EIAPPC) (NoxTC2008/2.1.1.1);

Technical files (NoxTC2008/2.3.6);

Record book of engine parameters (NoxTC2008/6.2.2.7.1);

International Load Line Certificate (1966) (LLP'88 Art.16.1);

International Load Line Exemption Certificate (LLP’88 Art.16.2);

Certificates issued in accordance with STCW Convention (STCW95/Art. Vi, RI/2, STCW code/Sect. A-
1/2);

Maritime Labour Certificate and Declaration of Maritime Labour Compliance part land Il (MLC and
DMLC part | and 1) (MLC, 2006/Reg.5.1/ standard A5.1.3);

Medical certificates (MLC, 2006/ Reg. 1.2/Standard A1.2);

Table of shipboard working arrangements (MLC, 2006/ Reg.2.3/ standard A2.3, 10 and STCW95/A-
Vill/1.5);

Records of hours of work or rest of seafarers (MLC, 2006/Reg. 2.3/standard A2.3, 12 and
STCW95/A-Vill/1.5);

Certificate  or documentary evidence of financial security for repatriation (MLC,
2006/Reg2.5/standard A2.5.2);

Certificate or documentary evidence of financial security relating to shipowners liability (MLC,
2006/Reg.4.2/standard A4.2.1);

Mobile Offshore Drilling Unit Safety Certificate MODU Code/lI/Section 6),

Certificate of insurance or any other financial security in respect of civil liability foroil pollution
damage (CLC69P92/AVII.2);

Certificate of insurance or any other financial security in respect of civil liability for Bunker oil
pollution damage (BUNKERS 2001/Art.7.2);

International Ship Security Certificate (ISSC) (ISPSC/PA/19.2.1);

Record of AFS (AFS/Annex 4/Reg.2(1));

International Anti-Fouling System Certificate (IAFS Certificate) (AFS/Annex 4/Reg.2(1));
Declaration on AFS (AFS/Annex 4/Reg.5(1));

International Ballast Water Management Certificate IBWMC) (BWMC Art 9.1(a));

Ballast Water Record Book (BWRB) BWMC Art 9.1 (b));

Certificate of insurance or other financial security in respect of liability for theremoval of wrecks
(Nairobi WRC 2007 / Art. 12.2)
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MEMORANDUM MIREKUPTIMI PiiR KONTROLLIN SHTETEROR PORTUAL
Ni RAJONIN E MESDHEUT

Autoritetet Detare t&!
Algjerisé

Kroacisg?

Qipros

Egjiptit

Izraelit

Jordanisé?®

Libanit

Maltés

Marokut

Tunizisé

Turqisé

Autoritetit Palestinez*

né vijim t& referuara si “Autoritetet”

Duke njohur nevojén pér té rritur siguring detare dhe mbrojtjien e mjedisit detar dhe
réndésing e pérmirésimit t& kushteve t& jetesés dhe punés né bordin e anijeve;

Duke kujtuar Deklaratén e miratuar mé 28 néntor 1995 me rastin ¢ Konferencés Euro-
Mesdhetare né Barcelong, duke krijuar njé partneritet Euro-Mesdhetar dhe duke pérfshirg,
ndér t& tjera, bashk&punimin né siguriné detare dhe parandalimin e ndotjes né pellgun e
Mesdheut;

Duke theksuar me vlerésim progresin e arritur né kéto fusha, vegandrisht nga Organizata
Ndérkombétare Detare (IMO) dhe Organizata Ndérkombétare e Punés (ILO),

Duke theksuar edhe kontributin g8 ka dhe 8 mund t& jepet nga Komuniteti Evropian né
pérmbushjen e objektivave t8 lartpérmendura;

Duke pasur parasysh se pérgjegjésia kryesore pér zbatimin efektiv t& standardeve t8
pércaktuara né instrumentet ndérkombétare i mbetet autoriteteve t& shtetit, flamurin e t& cilit
ka t& drejté t& mbajé njé anije;

Duke pranuar megjithaté se kérkohet veprim efektiv nga shtetet portuale pér t& parandaluar
funksionimin ¢ anijeve nén standarde;

! Autoritetet Detare jané administratat kombétare detare t& pércaktuara pér zbatimin e kétij Memorandumi.

2 Kroacia aderoi né Memorandum, duke filluar nga 1 janari 2024.

3 Jordania iu bashkua Memorandumit t¢ Mirékuptimit Mesdhetar (Med MoU) né vitin 1999 Amendamenti Nr.
(2

4 Anétarésimi i Autoritetit Palestinez u diskutua nga komiteti né takimin e tij té paré dhe u theksua komunikimi
nga Autoriteti Detar i Izraelit pér informacione mbi disa rregullime té brendshme procedurale qé do té pengonin
nénshkrimin e Memorandumit t& Mirékuptimit Mesdhetar nga Autoriteti Palestinez. Né mungesé té
delegacioneve té Izraelit dhe Autoritetit Palestinez, komiteti ra dakord t& shtyjé shqyrtimin e géshtjes derisa té
dy Autoritetet t& paragiten né mbledhjen e komitetit. Megjithaté, komiteti theksoi se megenése delegacioni 1
Autoritetit Palestinez nuk mund t& nénshkruante Memorandumin e Mirékuptimit Mesdhetar brenda periudhés sé
pércaktuar pér nénshkrimin e tij (d.m.th. 12 korrik 1997 deri mé 23 shkurt 1998), ¢éshtja e ngritur nga Autoriteti
Detar i Izraelit mund té trajtohet né kohén e duhur sipas procedurave té pérshkruara né nenin 8 t&
Memorandumit { Amendamenti Nr. (1)}.




image2.jpg
Duke njohur gjithashtu nevojén pér t& shmangur shtrembérimin ¢ konkurrencés ndérmjet
porteve;

Té bindur pér domosdoshméring, pér kéto géllime, t& njé sistemi t& pérmirésuar dhe t&
harmonizuar t& kontrollit shtetéror portual dhe t& forcimit t& bashk&punimit dhe shkémbimit
t& informacionit;

Kang arritur mirékuptimin ¢ méposhtém:

Seksioni 1 Angazhimet

1.1

1.2

1.3

1.4

1.5

Cdo Autoritet do t& zbatojé dispozitat e kétij Memorandumi dhe Shtojcave t& tij, t&
cilat pérb&jné pjesé integrale t& Memorandumit, dhe do t& ndérmarré t& gjitha hapat e
nevojshém pér t& ratifikuar instrumentet pérkatése pér qéllimet e kétij Memorandumi.

Cdo Autoritet do t& mbajé njé sistem efektiv t& Kontrollit Shtetéror Portual me
synimin pér t& garantuar qg, pa diskriminim pérsa i pérket flamurit, anijet tregtare t&
huaja q& lundrojné n& njé port t& shtetit t& tij, ose t& ankoruara jashté nj& porti t& tillg,
t& jené né& pérputhje me standardet ¢ pércaktuara né instrumentet pérkatése té
pércaktuara né nenin 2. Cdo Autoritet mund t& kryejé gjithashtu kontrolle mbi anijet
né instalimet né det t& hapur.

Cdo Autoritet do t& arrijé, brenda njé periudhe 3 vjegare nga hyrja né fuqi e
Memorandumit, njé total vjetor inspektimesh qé& korrespondon me 15% t& numrit t&
parashikuar t& anijeve tregtare t& huaja individuale, né vijim t& referuara si “anije”, t&
cilat kang hyré né portet ¢ shtetit t& tij gjaté njé periudhe t& fundit pérfagésuese prej 12
muajsh. Komiteti i krijuar n& pérputhje me nenin 6.1 do t& monitorojé aktivitetin e
pérgjithshém t& inspektimit dhe efektivitetin e tij né t& gjithé rajonin. Komiteti
gjithashtu do t& rregullojé shkallén e synuar t& inspektimit bazuar n& pérvojén e fituar
dhe progresin e béré n& zbatimin ¢ Memorandumit t& Mirékuptimit.

Cdo Autoritet do t& konsultohet, bashképunojé dhe shk&mbejé informacion me
Autoritetet e tjera pér t& zhvilluar mé tej g&llimet e Memorandumit.

Cdo Autoritet, ose ¢do organ tjetér, sipas rastit, do t& vendosé njé proceduré t&
pérshtatshme pér shérbimet pilot dhe autoritetet portuale & t& informojné menjéhers
Autoritetin kompetent t& Shtetit portual, sa heré q& ata mésojné gjaté kryerjes sé&
detyrave t& tyre normale se ka mangési q& mund t8 cenojné siguring e anijes, ose qé
mund t& pérbéjné njé kércénim pér démtimin e mjedisit detar.
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Seksioni 2  Instrumentet pérkatése

2.1

2.2

2.3

2.4

2.5

Pér géllimet ¢ Memorandumit, “instrumentet pérkatése” jané né fuqi s& bashku me
Protokollet dhe amendamentet e kétyre instrumenteve dhe kodet pérkatése t& statusit
t& detyrueshém, sig¢ specifikohet né (Shtojcén 1)

N& lidhje me Konventén e Transportit Tregtar (Standardet Minimale) t& vitit 1976
(Konventa 147 e Organizatés Ndérkombétare t8 Punds - ILO), ¢do Autoritet do t&
zbatojé udhézimet n& Shtojcén 1 “Inspektimi i kushteve t& punés né bordin e anijes:
Udhézimet pér procedurén”.

Cdo Autoritet do t& zbatojé ato instrumente pérkatése qé jand né fuqi dhe né t& cilat
shteti i tij &shté palé. N& rastin e ndryshimeve n& njé instrument pérkatés, ¢do
Autoritet do t& zbatojé ato ndryshime q& jané né fuqi dhe q& shteti i tij ka pranuar. Njé
instrument i ndryshuar né ké&té ményré do t& konsiderohet mé pas si “instrumenti
pérkatés” pér até Autoritet.

Kur inspektohet njé anije q& mban flamurin ¢ njé shteti g8 nuk &shté palé né njé
Konventé ose njé “instrument pérkatés” i ndryshuar pér gé&llime t& kontrollit shtetéror
portual, autoritetet q& jané palé n& ké&t& Konventé ose “instrument pérkatds” té
ndryshuar duhet t8 garantojné g8 trajtimi i dhéné& pér njé anije t& till¢ dhe ekuipazhin e
saj nuk &shté mé i favorshém sesa ai q& u jepet anijeve q& mbajné flamurin e njé shteti
q& &shté palé né até Konventé ose “instrument pérkatés”.

N& rastin e anijeve nén 500 ton tonazh bruto, Autoritetet do t& zbatojné ato kérkesa t&
instrumenteve pérkatése qé& jané t& zbatueshme dhe né masén g& njé instrument
pérkatés nuk zbatohet, do t& ndérmarré veprime té tilla g8 mund t& jené t& nevojshme
pér t& garantuar q& ato anije nuk jand haptazi t& rrezikshme pér siguring, shéndetin ose
mjedisin, duke pasur parasysh, veganérisht Shtojcén 1.

Seksioni 3  Procedurat e inspektimit, Korrigjimit dhe Ndalimit

3.1.1

3.1.2

3.21

3.2.2

Né& zbatimin ¢ Memorandumit, autoritetet do t& kryejné inspektime t& cilat do t&
konsistojné n& njé vizité né bordin ¢ njé anijeje pér t& kontrolluar vlefshméring e
certifikatave dhe dokumenteve t& tjera t& réndésishme pér géllimet ¢ Memorandumit,
si dhe gjendjen e anijes, pajisjet dhe ekuipazhin e saj, si dhe kushtet e jetesss dhe
punés s& ekuipazhit.

Autoriteti do t8 garantojé q& inspektori, si minimum, do t& kontrollojé certifikatat dhe
dokumentet e renditura né Shtojeén 1, deri né masén e zbatueshme dhe t& bindet pér
kushtet e pérgjithshme t& anijes, duke pérfshiré sallén e motorit dhe akomodimet dhe
kushtet higjienike.

Kurdoherg q& ka arsye t& qarta pér t& besuar se gjendja e njé anijeje ose e pajisjeve
ose ekuipazhit t& saj nuk plotéson né thelb kérkesat ¢ njé instrumenti pérkatés, do t&
kryhet njé inspektim mé i detajuar, duke pérfshiré kontrollin e métejshém t&
pérputhshmé&risé me kérkesat operacionale né bord.

Ekzistojné arsye t& qarta kur inspektori gjen prova té cilat, né gjykimin e tij
profesional, garantojné njé inspektim mé t& detajuar t& anijes, pajisjeve ose
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3.2.3

3.2.4

3.3

3.4

3.51

3.5.2

3.5.3

ekuipazhit. Autoritetet do t& konsiderojné si baz& t& qarté, ndér t& tjera, ato t&
pércaktuara né Shtojcén 3.

Asgjé né kéto procedura nuk duhet t& interpretohet si kufizim i kompetencave t&
Autoriteteve pér t& marré masa brenda juridiksionit t8 tyre né lidhje me ¢do ¢&shtje
me t& cilén lidhen instrumentet pérkatése.

Do t& zbatohen gjithashtu procedurat dhe udhézimet pérkatése pér kontrollin ¢ anijeve
t& specifikuara né Shtojcén 1.

N& pérzgjedhjen e anijeve pér inspektim, Autoritetet do t'u japin pérparési anijeve t&
méposhtme:

Anijet & vizitojné njé port t& njé shteti, Autoriteti i t& cilit &shté nénshkrues i
Memorandumit, pér heré t& paré ose pas njé mungese prej 12 muajsh ose mé shumg;

Anijet & jané lejuar t& largohen nga porti i njé shteti; Autoriteti i t& cilit &shté
nénshkrues i Memorandumit, me kusht g8 manggsité e vérejtura duhet t& korrigjohen
brenda njé periudhe t& caktuar, pas skadimit t& késaj periudhe;

Anijet t& cilat jan& raportuar nga pilotét ose autoritetet portuale se kané mangési qé
mund t& cénojné lundrimin e tyre t& sigurt;

Anijet, certifikatat statutore t& t& cilave pér ndértimin dhe pajisjet e anijes, nuk jané
l&shuar né pérputhje me instrumentet pérkatése.

Anijet q& transportojné mallra té rrezikshme ose ndotése, t8 cilat nuk kang raportuar t&
gjithé informacionin pérkatés né lidhje me t& dhénat e anijes, 1&vizjet e anijes dhe né
lidhje me mallrat e rrezikshme ose ndotése & transportohen tek autoriteti kompetent i
portit dhe shtetit bregdetar;

Anijet t& cilat jan& pezulluar nga shoqéria klasifikuese e tyre pér arsye sigurie gjaté
gjashté muajve t& fundit.

Autoritetet do t& pérpigen t& inspektojné anijet t& cilat nuk kané gend t& inspektuara
brenda 6 muajve t& méparshém nga Autoritete t& tjera, pérveg rasteve kur ka arsye t&
qarta pér inspektim. Ké&to procedura nuk jang t8 zbatueshme pér anijet e listuara ng
paragrafin 3.3 t& cilat mund t& inspektohen sa heré q& Autoriteti ¢ g¢gmon t&
pérshtatshme.

Inspektimet do t& kryhen vetém nga njé person, i autorizuar sipas rregullavenga
Autoriteti i tij pér t& kryer inspektime shtetérore portuale dhe pérgjegjés ndaj atij
Autoriteti, i cili plotéson kérkesat e paragrafit 3.5.3 dhe kriteret ¢ kualifikimit t&
specifikuara né Shtojcén 7.

Inspektori q& kryen kontrollin shtetéror portual, mund t& asistohet nga njé person me
ekspertizén e kérkuar kur njé ekspertizé e tillé nuk mund t& sigurohet nga Autoriteti i
tij.

Inspektori q& kryen kontrollin shtetéror portual dhe personi q& ¢ ndihmon até, nuk do
t& kené asnjé interes tregtar as né portin ¢ inspektimit, as né anijet ¢ inspektuara, as
inspektori nuk duhet t& pundsohet apo kryejé puné n&é emér t& organizatave
jogeveritare q& 18shojné certifikatat statutore dhe t& klasifikimit ose q& kryejné
kontrollet e nevojshme pér 18shimin e kétyre certifikatave pér anijet.
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3.5.4

3.6.1

3.6.2

3.6.3

3.6.4

3.6.5

3.6.6

3.7

Secili inspektor duhet t& mbajé njé dokument personal né formén e kartés s& identitetit
t& 18shuar nga autoriteti i tij, q& specifikon se inspektori &shté i autorizuar pér t& kryer
inspektime. Njé model i zakonshém pér njé karté t8 tillé identiteti i bashkélidhet
Shtojeés 7.

Pas pérfundimit t& njé inspektimi, kapitenit t& anijes do t'i jepet nga inspektori njé
dokument né formén e specifikuar né Shtojcén 5 t& ké&tij Memorandumi Mirékuptimi,
duke dhéné rezultatet e inspektimit dhe detajet e ¢do vendimi t& marré nga inspektori
dhe t& veprimit korrigjues qé& duhet t& ndérmerret nga kapiteni, pronari ose operatori.

Autoriteti duhet t& bindet q& ¢do manggsi e konfirmuar ose zbuluar nga inspektimi
&shté korrigjuar.

N& rastin ¢ mangésive q& jané haptazi t& rrezikshme pér siguring, shéndetin ose
mjedisin, Autoriteti do t& ndalojé anijen ose operacionin gjaté t& cilit jan& zbuluar
mangésité. Urdhri i ndalimit ose ndalimi i operacionit nuk do t& hiqget derisa t& hiqet
rreziku, pérveg né kushtet e parashikuara né paragrafin 3.8.1 mé& poshtg.

Gjaté ushtrimit t& gjykimit t& tij profesional nése njé anije duhet t& ndalohet apo jo,
inspektori do t& udh&hiqget nga kriteret e pércaktuara né Shtojcén 1.

Kur arsyeja pér ndalim &shté rezultat i démtimit aksidental t& pésuar gjaté udhétimit t&
anijes né njé port ose gjaté operacioneve t& ngarkesave, nuk do t& l&shohet asnjé
urdhér ndalimi, me kusht q&:

. kérkesat ¢ Rregullores I/11(c) t& Konventss Ndérkombétare pér Siguring e Jetés né

Det (SOLAS) t& jen& marré né konsideraté né lidhje me njoftimin ¢ Administratés sé
flamurit, kontrollorit t& eméruar ose organizatés s& njohur pérgjegjése pér 1&shimin e
certifikatés pérkatése;

. para hyrjes né port ose menjéheré pasi ka ndodhur njé dém, kapiteni ose zotéruesi i

anijes i ka paraqitur autoritetit t& kontrollit shtetéror portual detaje mbi rrethanat e
aksidentit dhe démin e pé&suar dhe informacionin pér njoftimin e kérkuar t&
Administratés sé¢ flamurit;

. anija po ndérmerr veprimet e duhura korrigjuese, sipas bindjes s& Autoritetit, dhe

. Autoriteti ka siguruar, pasi &shté njoftuar pér pérfundimin e veprimit korrigjues, qé

manggsité, t& cilat ishin haptazi t& rrezikshme pér siguring, shéndetin ose mjedisin,
jané trajtuar sipas bindjes s& Autoritetit.

N& rrethana té jashtézakonshme kur, si rezultat i njé inspektimi mé t& detajuar, gjendja
e pérgjithshme e njé anijeje dhe pajisjeve t8 saj, duke marré parasysh edhe detarét dhe
kushtet e tyre t& jetesés dhe t& punds, rezulton t& jeté haptazi nén standarde, Autoriteti
mund t& pezullojé inspektimin. Pezullimi i inspektimit mund t& vazhdojé derisa palét
pérgjegjése t& kené ndérmarré hapat e nevojshém pér t& garantuar qé anija t& jeté né
pérputhje me kérkesat ¢ instrumenteve pérkatése. Para pezullimit t& njé inspektimi,
Autoriteti duhet t8 keté& regjistruar mangési t& ndalueshme né disa fusha. Né& njoftimin
e ndalimit palét pérgjegjése do t& informohen se inspektimi &shté pezulluar derisa
Autoriteti t& jeté informuar se anija pérmbush t& gjitha kérkesat pérkatése.

N& rast se njé anije ndalohet, Autoriteti do t& informojé menjéheré administratén e
shtetit, flamurin e t& cilit anija ka t& drejté t& mbajé dhe konsullin ose, né mungesé t&
tij, pérfaqésuesin e tij diplomatik mé t& afért pér veprimin e ndérmarré. Kur &shté e
nevojshme, do t& informohet edhe organizata pérgjegjése pér 1&shimin e certifikatave.
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3.8.1

3.8.2

3.8.3

3.9

3.10

3.11

3.12

Kur mangésité e pérmendura né paragrafin 3.6.3 nuk mund t& korrigjohen né portin e
inspektimit, Autoriteti mund t& lejojé anijen t& vazhdojé né njé port tjetér, ose né
kantierin mé& t& afért t& riparimit, duke iu nénshtruar kushteve t& pérshtatshme t&
pércaktuara nga ai Autoritet, me qéllim pér t& garantuar q& anija mund t& vazhdojé
késhtu pa rrezik pér siguring, shéndetin ose mjedisin. N& rrethana té tilla, Autoriteti do
t& njoftojé Autoritetin kompetent t& Shtetit t& rajonit ku ndodhet porti tjetér i thirrjes
ose kantieri i riparimit, palét e pérmendura né paragrafin 3.7 dhe ¢do autoritet tjetér
sipas rastit. Njoftimi p&r Autoritetet do t& béhet né pérputhje me Shtojcén 5. Autoriteti
qé merr njé njoftim t& tillé do t& informojé Autoritetin njoftues pér veprimet e
ndérmarra.

Autoritetet do t& marrin masa pér t& garantuar g& anijeve t8 pérmendura né paragrafin
3.8.1, t& cilat ose shkojné né det pa respektuar kushtet e pércaktuara nga Autoriteti qé
ndaloi anijen, ose q& nuk hyjné né portin ose kantierin e réné dakord pér t& ndérmarré
riparime, do t'u refuzohet hyrja né ¢do port brenda kuadrit t& kétij Memorandumi,
derisa pronari ose operatori dhe shteti i flamurit t& njoftojné Autoritetin e Shtetit, ku
anija u konstatua me defekt, ose Autoritetin & merr anijen, & anija p&rmbush t&
gjitha kérkesat e zbatueshme t8 instrumenteve pérkatése. N& rastin e fundit, Autoriteti
marrds do t& njoftojé t& gjitha Autoritetet e tjera pér kété pajtueshméri.

N& rast t8 jashtézakonshém t& “forcés madhore”, mund t& lejohet hyrja né njé port t&
caktuar, pér t& minimizuar rrezikun e jetés ose ndotjes.

Dispozitat ¢ nenit 3.7 dhe 3.8 nuk cénojné kérkesat e instrumenteve, ose procedurave
pérkatése t& vendosura nga organizatat ndérkombétare, né lidhje me procedurat e
njoftimit dhe raportimit pér kontrollin shtetéror portual.

Gjaté ushtrimit t& kontrollit sipas Memorandumit, Autoritetet do t& b&jné t& gjitha
pérpjekjet ¢ mundshme pér t& shmangur ndalimin ose vonimin e padrejté t& njé
anijeje. Asgjé né Memorandum nuk cénon t& drejtat ¢ krijuara nga dispozitat e
instrumenteve pérkatése né lidhje me kompensimin pér ndalimin ose vonesén e
panevojshme.

N& rast se kapiteni, pronari ose agjenti i anijes njofton Autoritetet e kontrollit shtetéror
portual para ose pas mbérritjes s& anijes né port, pér ¢do démtim, avari ose mangési t&
anijes, makinerive dhe pajisjeve t8 saj, t& cilat synohet t& riparohen ose korrigjohen
para se anija t& lundrojé nga ai port, ndalimi duhet t& regjistrohet vetém nése
konstatohen manggsi & justifikojné ndalimin, pasi kapiteni t& keté dhéné njoftimin se
anija ishte gati pér inspektorét. E njéjta proceduré zbatohet kur autoritetet ¢ kontrollit
shtetéror portual, njoftohen se anija &shté planifikuar t& kontrollohet né port né lidhje
me kérkesat ¢ flamurit, statutit ose té klasit.

N& rrethana t& jashtézakonshme, kur njé anije né rrugén e saj pér né njé kantier t&
caktuar riparimi duhet t& hyjé né njé port pér riparime t& pérkohshme pér arsye
sigurie, ajo mund t& lejohet né até port. T8 gjitha operacionet tregtare jané t& ndaluara,
pérveg shkarkimit t& ngarkesés sé& saj, nése kérkohet pér arsye sigurie. Anija mund t&
lejohet t& vazhdojé né kantierin e specifikuar t& riparimit, vetém nése shteti i flamurit
& anijes ka l&shuar certifikata statutore pér anijen, q& kufizojné vlefshméring e tyre né
até lundrim specifik dhe shteti portual &shté i bindur se njé anije e tillé nuk do t&
pérbgjé rrezik t& panevojshém pér siguring e anijes, ose mjedisin, ose t& shkaktojé
véshtirési t& panevojshme pér ekuipazhin.
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3.13 Pronari ose operatori i njé anijeje do t& keté t& drejtén e ankimimit kundér vendimit t&
ndalimit né Autoritetin mé t& larté administrativ, ose né Gjykatén e juridiksionit
kompetent, sipas ligjit né ¢do vend. Megjithaté, ankesa nuk shkakton pezullimin e
ndalimit.

3.14 Nése njé inspektim zbulon mangési qé garantojné ndalimin ¢ njé anijeje, t& gjitha
kostot né lidhje me inspektimet pas t& parit, do t& mbulohen nga pronari i anijes ose
operatori. Ndalimi nuk do t& higet derisa t& jets kryer pagesa e ploté ose t& jeté dhéné
njé garanci ¢ mjaftueshme pér rimbursimin e shpenzimeve.

Seksioni 4  Sigurimi i informacionit

4.1 Cdo Autoritet do t& raportojé pér inspektimet e tij sipas Memorandumit dhe rezultatet
e tyre, né pérputhje me procedurat e specifikuara né Shtojcén 4.

4.2 Autoritetet do t'i japin informacionin e méposhtém Sekretariatit t8 Memorandumit:

(a) Numri i inspektoréve q& punojné né emér t& tyre né inspektimet shtetérore
portuale. Kur inspektimet punojné me kohé t& pjesshme, totali korrigjohet né njé
numdr inspektorésh t& punésuar me kohé t& plotg;

(b) Numri i anijeve individuale q& hyjné n& portet e tyre né njé vit pérfaqésues para
Memorandumit;

(¢) Tarifat pér inspektimet, nése ka.

Ky informacion do t& pérditésohet t& paktén ¢do tre vjet.

Seksioni S Shkeljet operative

Autoritetet, me kérkesén e njé autoriteti tjetér, do t& pérpiqen t& sigurojné prova né lidhje me
shkeljet e dyshuara t& kérkesave pér ¢éshtjet e funksionimit t& Rregullit 10 t& Rregullores
Ndérkombétare pér Parandalimin e Pérplasjeve né Det t& vitit 1972 dhe t& Konventés
Ndérkombétare pér Parandalimin ¢ Ndotjes nga Anijet t& vitit 1973, t& ndryshuar nga
Protokolli i vitit 1978, né lidhje me t& N& rast t& shkeljeve t8 dyshuara q& pérfshijng
shkarkimin e substancave t& démshme, njé Autoritet, me kérkesén e njé Autoriteti tjetér, do t&
vizitojé né port anijen ¢ dyshuar pér njé shkelje t& tillé pér t& marré informacion dhe, kur
&shté e pérshtatshme, pér t& marré njé mostér t& ¢do substance ndotése t& dyshuar. N& rastet e
pérmendura né kété nen, Autoriteti kérkues duhet t& deklarojé se shteti i flamurit t& anijes
&shté njoftuar tashmé pér shkeljen e pretenduar.

Seksioni 6  Organizimi

6.1 Do t& krijohet nj& Komitet i pérbéré nga njé pérfagésues i secilit prej Autoriteteve qé
jang palé né Memorandum. Njé pérfagésues i Organizatés Ndérkombétare Detare, i
Organizatés Ndérkombétare t& Punés dhe i Komisionit Evropian do t& ftohet t& marré
pjesé pa voté né punén ¢ Komitetit. Pérfaqésuesve t& autoriteteve detare t& shteteve t&
tjera bregdetare mesdhetare dhe, né pérputhje me dispozitat e nenit 8, ¢gdo organizate
ose autoriteti tjetér q& Komiteti mund ta gjykojé t& pérshtatshme, mund t'u jepet
statusi i vézhguesit pa voté.
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6.2
6.3

6.4

6.5

6.6

6.7

Komiteti do t& mblidhet njé& heré né vit dhe né ato raste t& tjera g8 mund t& vendosé.
Komiteti do t&:
kryejé detyrat specifike q& i jang caktuar sipas Memorandumit.

promovojé me t& gjitha mjetet e nevojshme, duke pérfshiré seminare pér
kontrollorét, harmonizimin e procedurave dhe praktikave né lidhje me inspektimin,
korrigjimin, zbulimin dhe zbatimin e paragrafit 2.4.

zhvillojé dhe rishikojé udh&zimet pér kryerjen e inspektimeve sipas Memorandumit.

zhvillojé dhe rishikojé procedurat, duke pérfshiré ato q& lidhen me shkémbimin e
informacionit.

mbajé nén shqyrtim ¢éshtje t& tjera né lidhje me funksionimin dhe efektivitetin e
Memorandumit.

promovojé me t& gjitha mjetet ¢ nevojshme harmonizimin e funksionimit dhe
efektivitetit t& ké&tij Memorandumi me ato t& marréveshjeve t& ngjashme pér Rajonet e
tjera.

miratojé buxhetin dhe do t& vendosé kontributet e secilés palé né Memorandum.

Pérveg rasteve kur parashikohet ndryshe (né nenin 7), Komisioni do t& marré
vendimet e tij duke vepruar me shumicé t& thjeshté.

Njé& Sekretariat i siguruar nga Autoriteti Detar i Egjiptit, do t& ngrihet dhe do t& keté
zyrén e tij né Aleksandri-Egjipt.

Sekretariati, duke vepruar nén drejtimin e Komitetit dhe brenda kufijve t8 burimeve t&
véna né dispozicion té tij, do t&:

pérgatité takime, qarkullojé dokumente dhe ofrojé njé ndihmé t8 tille & mund t&
kérkohet pér t& mundésuar Komitetin qé& t& kryejé funksionet e tij.

lehtésojé shkémbimin e informacionit, kryerjen e procedurave t& pérshkruara ng
Shtojcén 4 dhe pérgatitjen e raporteve, sipas nevojés, pér géllimet ¢ Memorandumit.

kryejé puné té tjera q& mund t& jené t& nevojshme pér t& garantuar funksionimin
efektiv t& Memorandumit dhe pér t& rishikuar Memorandumin periodikisht ng
kohé&zgjatje 5-vjegare.

Njé& Marréveshje pér tremujorin kryesor t& Sekretariatit duhet t& vendoset ndérmjet
Memorandumit t& Mirékuptimit Mesdhetar t& pérfaqésuar nga Kryetari dhe Qeveria e
Egjiptit.

Seksioni 7 Amendamentet

71

7.2

Cdo Autoritet, i cili ¢ ka pranuar Memorandumin, mund t& propozojé ndryshime né
Memorandum.

N& rastin e ndryshimeve t& propozuara né nenet ¢ Memorandumit, do t& zbatohet
procedura e méposhtme:
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7.3

(a) Amendamenti i propozuar do t& dorézohet népérmjet Sekretariatit pér shqyrtim
nga Komiteti.

(b) Amendamentet do t& miratohen me dy t& tretat ¢ shumicés sé pérfaqésuesve t&
Autoriteteve t& pranishme dhe g& votojné né Komitet.

Nése njé amendament miratohet, do t'u komunikohet nga Sekretariati Autoriteteve pér
pranim.

Ndryshimet e paragrafit 1 t& nenit 2 miratohen me dy t& tretat e shumicés sé&
pérfagésuesve t& autoriteteve t& pranishme dhe votuese, té cilat jan& palé nég
Konventén e re t& propozuar pér t'u pérfshiré si “instrument pérkatés”.

(¢) Njé amendament do t& konsiderohet se &shté pranuar ose né fund t& njé periudhe
gjashtémujore pas miratimit nga pérfagésuesit ¢ Autoriteteve né Komitet, ose né fund
t& ¢do periudhe tjetér t& pércaktuar unanimisht nga pérfaqésuesit e Autoriteteve né
Komitet né& momentin ¢ miratimit, pérve¢ nése brenda periudhds pérkatése njé
kundérshtim i komunikohet Sekretariatit nga njé Autoritet.

(d) Nj& amendament do t& hyjé né& fuqi 60 dité pasi t& jeté pranuar, ose né fund t& njé
periudhe tjetér t& pércaktuar unanimisht nga pérfaqésuesit e Autoriteteve né Komitet.

Né& rastin e amendamenteve t& propozuara né Shtojcat ¢ Memorandumit, do t&
zbatohet procedura e méposhtme:

(a) amendamenti i propozuar do t& dorézohet népérmjet Sekretariatit pér shqyrtim nga
Autoritetet.

(b) amendamenti do t& konsiderohet se &shté pranuar né fund t& nj& periudhe prej tre
muajsh nga data kur &shté komunikuar nga Sekretariati, pérveg nése njé Autoritet
kérkon me shkrim q& amendamenti t& shqyrtohet nga Komiteti. N& rastin e fundit do
& zbatohet procedura e specifikuar né paragrafin 7.2.

(c) amendamenti do t& hyjé n& fuqi 60 dit&, pasi t& jeté pranuar, ose né fund t& ¢do
periudhe t& pércaktuar unanimisht nga Autoritetet.

Seksioni 8  Dispozitat administrative

8.1

8.2

8.3

8.4

Memorandumi nuk cenon t8 drejtat dhe detyrimet sipas ndonjé marréveshjeje
ndérkombétare.

Njé Autoritet Detar i njé Shteti, i cili pérmbush kriteret ¢ specifikuara né Shtojcén 6,
mund t'i p&mbahet Memorandumit me pranimin e shumic8s s& thjeshté t&
pérfagésuesve t& Autoriteteve t& pranishém dhe & votojné né Komitet.

Memorandumi mbetet i hapur pér nénshkrim, né seling e Sekretariatit t& Komitetit nga
11 korriku 1997 deri mé& 23 shkurt 1998. Autoritetet Detare & plotésojné kérkesat e
specifikuara né Shtojcén 6, mund t& b&hen palé t& Memorandumit duke:

a) nénshkruar pa asnjé rezervé pér pranimin, ose duke
b) nénshkruar me nénshkrim q& i nénshtrohet pranimit, i pasuar nga pranimi.

Pranimi ose aderimi do t& b&het me njé komunikim me shkrim nga Autoritetet Detare
drejtuar Sekretariatit.
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8.5 Sekretariati do t& informojé Autoritetet Detare q& kané nénshkruar Memorandumin
pér ¢do nénshkrim ose komunikim me shkrim, ose pér pranimin ose aderimin dhe pér
datén né t& cilén ka ndodhur njé rast i tillg.

8.6 Ky Memorandum do t& hyjé né fuqi pér ¢do Autoritet né datén & i njoftohet
Sekretariatit sipas rregullave.

8.7 Cdo Autoritet Detar ose Organizaté qé déshiron t& marré pjesé si vézhgues, do t'i
paragesé me shkrim Komitetit njé aplikim dhe do t& pranohet si vézhgues me
pélgimin unanim t& pérfaqésuesve t& Autoriteteve t& pranishém dhe q& votojné né
mbledhjen ¢ Komitetit.

8.8  Cdo autoritet mund t& térhiget nga Memorandumi duke ¢ njoftuar Komitetin me
shkrim 60 dité para.

8.9  Versionet né anglisht, fréngjisht dhe arabisht jan& njélloj autentiké. Teksti n& anglisht
&shté versioni zyrtar i Memorandumit né rast mosmarréveshjeje.

Seksioni 9  Programet e trajnimit dhe seminaret

Autoritetet do t& pérpigen t& krijojné programe dhe seminare t& pérshtatshme trajnimi.

Seksioni 10 Mekanizmi Financiar
Shpenzimet pér drejtimin e Sekretariatit dhe Qendrés sé& Informacionit financohen nga:
- Kontributi financiar i secilés palé né Memorandum.
- Nése &shté e mundur, dhurata dhe subvencione nga vendet ose organizatat donatore.

Kontributet financiare pér shpenzimet pér drejtimin e Sekretariatit dhe Qendrés sé
Informacionit t& Paléve né Memorandum duhet t& paguhen, né pérputhje me vendimet dhe
procedurat e miratuara nga Komiteti.

Nénshkruar né Malté, né gjuhén angleze, né datén t& njémbédhjeté korrik t& vitit njémijé e
néntéqind e nént&dhjeté e shtaté.
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SHTOJCAT E MEMORANDUMIT

Shtojca 1 Procedurat e Kontrollit Shtetéror Portual

Shtojca 2 Procedurat pér hetim sipas MARPOL 73/78

Shtojca 3 Fakte t& konsideruara si “Arsye t& Qarta”

Shtojca 4 Sistemi informativ pér inspektimet

Shtojca § Publikimi i informacionit pér Kontrollin Shtetéror Portual

Shtojca 6 Kriteret cildsore pér respektimin ¢ Memorandumit t&€ Mirékuptimit
Mesdhetar

Shtojca 7 Kriteret dhe kérkesat e Zyrtarit t& Kontrollit Shtetéror Portual

Shtojca 8 Procedurat ¢ ankimimit dhe rishikimit

Shtojca 9 Kriteret e pérzgjedhjes (faktori i synuar)

Shtojca 10 Refuzimi i Hyrjes

Shtojca 11 Lista e Certifikatave & do t& Verifikohen
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SHTOJCA 1

PROCEDURAT E KONTROLLIT SHTETEROR PORTUAL

Pérmbajtja
Seksioni 1 Té pérgjithshme
1.1 Udh&zime & duhen respektuar né inspektimin e anijeve t& huaja.
1.2 Parimet & rregullojné korrigjimin e manggsive ose ndalimin e njé anijeje.
1.3 Zbatimi i klauzol&s “jo mé trajtim favorizues”.
1.4 Inspektim mé i detajuar
Seksioni 2 Standardet minimale té personelit dhe certifikimi

2.1 Hyrje

2.2 Kontrolli i personelit
2.3 Kontrolli i certifikimit
2.4 Ndalimi

Seksioni 3  Konventa Detare e Punés e vitit 2006 (MLC 2006), ose Konventa e
Transportit Tregtar (Standardet Minimale) e vitit 1976 (Nr. 147) dhe
Protokolli ILO 147 i vitit 1966, nése éshté e zbatueshme

Seksioni 4  Udhézime pér kontrollorét qé duhen respektuar né inspektimin e anijeve
té ngarkesave nén 500 toné tonazh bruto dhe anijeve té ndértimit
tradicional

Seksioni 1 Té pérgjithshme

1.1 Udhézime g€ duhen respektuar né inspektimin e anijeve té huaja.

1.1.1 Instrumentet pérkatése t& pérmendura né nenin 2.1 t& Memorandumit, jané si mé
posht&:

1) Konventa Ndérkombétare pér Linjat ¢ Ngarkesés, 1966 (LOAD LINE 66),

2) Protokolli i vitit 1988 né lidhje me Konventén Ndérkombétare pér Linjat e Ngarkesés,
1966 (LOAD LINE Prot 88);

3) Konventa Ndérkombétare pér Siguriné e Jetés né Det, 1974 (SOLAS 74),

4) Protokolli i vitit 1988 n& lidhje me Konventén Ndérkombétare pér Siguring e Jetés né
Det, 1974 (SOLAS Prot 88);

5) Konventa Ndérkombétare pér Parandalimin e Ndotjes nga Anijet, 1973, ¢ ndryshuar
nga Protokolli i vitit 1978 né lidhje me t&, dhe i ndryshuar mé tej nga Protokolli i vitit
1997 (MARPOL),
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6)
7

8)
9)

Konventa Ndérkombétare pér Standardet ¢ Trajnimit, Certifikimit dhe Mbajtjes sé&
Vrojtimit pér Detarét, 1978 (STCW 78),

Konventa mbi Rregulloret Ndérkombétare pér Parandalimin e Pérplasjeve né Det,
1972 (COLREG 72);

Konventa Ndérkombétare pér Matjen e Tonazhit t& Anijeve, 1969 (TONNAGE 69),
Konventa e Punés Detare, 2006 (MLC 20006);

10)Konventa ¢ Transportit Tregtar (Standardet Minimale), 1976 (Konventa e ILO-s

nr.147) (ILO 147);

11) Protokolli i vitit 1992 pér ndryshimin ¢ Konvent&s Ndérkombétare mbi Pérgjegjésiné

Civile pér Démtimin e Ndotjes nga Nafta, 1969 (CLC PROT 1992),

12) Konventa Ndérkombétare pér Kontrollin e Sistemeve t& Démshme Kundér Ndotjes né

Anije, 2001 (AFS 2001);

13) Konventa Ndérkombétare pér Pérgjegjésing Civile pér Démtimin e Ndotjes nga Nafta

t& Rezervuarit t& Karburantit né Anije, 2001,

14) Konventa Ndérkombétare pér Kontrollin dhe Menaxhimin e Ujit dhe Sedimenteve t&

Balastit t& Anijeve (BWM).

15)Konventa Ndérkombétare e Nairobit pér Eliminimin ¢ Mbetjeve (Nairobi WRC

1.1.2

1.2

1.3

2007).

Udhézimet ¢ pérmendura né nenin 3.1 t& Memorandumit, u referohen dispozitave
pérkatése sa vijon:

Procedurat pér Kontrollin Shtetéror Portual, 2011 (Rezoluta IMO A.1052(27)),
Parimet e Personelit t& Sigurt (Rezoluta IMO A.1047 (27).

Dispozitat e Kodit Ndérkombétar t& Mallrave t& Rrezikshme Detare.

Publikimi i ILO-s “Inspektimi i Kushteve t& Punés né Bordin ¢ Anijes: Udh&zime
pér procedurén”.

e Procedurat e pércaktuara né Shtojeén ¢ Memorandumit.

Parimet q& rregullojné korrigjimin e mangésive ose ndalimin e njé anijeje.

N& marrjen e njé vendimi né lidhje me korrigjimin ¢ njé mangésie ose ndalimi t& njé
anijeje, Zyrtari i Kontrollit Shtetéror Portual do t& marré parasysh rezultatet e
inspektimit mé t& detajuar t& kryer né pérputhje me nenin 3 t&¢ Memorandumit. Zyrtari
i Kontrollit Shtetéror Portual do t& ushtrojé gjykimin e tij profesional né pércaktimin
nése do ta ndalojé anijen derisa t& korrigjohen mangésité, ose do ta lejojé até t&
lundrojé me disa mangési pa rrezik t& paarsyeshém pér siguring, shéndetin ose
mjedisin, duke pasur parasysh rrethanat ¢ veganta t& udhétimit t& synuar. Pérsa u
pérket standardeve minimale t& personelit dhe dispozitave t& Konventss s& Punés
Detare, 2006 (MLC 2006) dhe/ose Konventés ILO nr.147, do t& respektohen
procedurat e veganta t& pércaktuara né nenet 3 dhe 4 t& késaj Shtojce.

Zbatimi i klauzolés “jo mé trajtim favorizues”.

N& zbatim t& nenit 2.4 t& Memorandumit, duhet t& respektohen sa vijon. Anijet &
kang t& drejté t& mbajné flamurin e njé shteti, i cili nuk &shté palé né njé instrument
pérkatés t& listuar né nenin 2 t& Memorandumit dhe si rrjedhojé, nuk pajiset me
certifikata, q& pérfagésojné prova “prima facie” t& kushteve t& kénagshme né bord, do
t& marrin informacion mé t& detajuar ose sipas rastit, njé inspektim t& zgjeruar. N&
kryerjen e njé inspektimi t& tillg, Zyrtari i Kontrollit Shtetéror Portual duhet t& ndjeké
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1.4

t& nj&jtat udhézime si¢ parashikohen pér anijet pér t& cilat zbatohen instrumentet
pérkatése.

Nése anija ose ckuipazhi ka ndonjé formé& alternative t& certifikimit, Zyrtari i
Kontrollit Shtetéror Portual, n& kryerjen e ké&tij inspektimi, mund t& marré parasysh
formén dhe pérmbajtjen e kétij dokumentacioni. Kushtet né njé anije t& tillé dhe
pajisjet e saj dhe certifikimi i ekuipazhit, numri dhe pérbérja e tij duhet t& jené né
pérputhje me géllimet e dispozitave t& nj& instrumenti pérkatés, pémdryshe anija do t'i
nénshtrohet kufizimeve t& tilla q& jan& t& nevojshme pér t& marré njé nivel t&
krahasueshém sigurie dhe mbrojtjeje t& mjedisit detar.

Inspektimi mé i Detajuar.

N& masén g8 ka arsye t& qarta pér njé inspektim mé t& detajuar né lidhje me dispozitat
e Konventés SOLAS, Protokollit t& saj, Konventés s& Linjave t& Ngarkesés,
Konventss mbi Rregulloret e Pérplasjes dhe MARPOL 73/78, gjaté kryerjes s& kétij
inspektimi,Zyrtari i Kontrollit Shtetéror Portual do t& marré marré parasysh
konsideratat ¢ dhéna né udhézimet pér “Pérgatitien dhe llojin ¢ njé inspektimi t&
Kontrollit Shtetéror Portual”, dispozitat ¢ Kodit Ndérkombétar t& Mallrave t&
Rrezikshme Detare né botimin e tij t& fundit, dhe Dispozitat e nenit 3 t& késaj Shtojce
né lidhje me kushtet e jetesés dhe punés né& bordin e anijeve.

Seksioni 2 Standardet minimale té personelit dhe certifikimi

2.1

2.2

2.2.1

Hyrje

Parimi udhézues pér inspektimin shtetéror portual t& personelit t& njé anijeje t& huaj
duhet t& jeté vendosja e konformitetit me kérkesat e shtetit t& flamurit pér personel t&
sigurt. Kur kjo &shté né dyshim, duhet t& konsultohet shteti i flamurit. Kérkesa t& tilla
pér personel t& sigurt burojné nga:

o Konventa Ndérkombétare pér Siguriné e Jetés né Det (SOLAS) 1974.

o Konventa e Transportit Tregtar (Standardet Minimale) 1976 (Konventa 147 e
Organizatés Ndérkombétare t& Punés), e cila ndér t& tjera i referohet Konventés nr.
53 t& Organizatés Ndérkombétare t& Punés, nenet 3 dhe 4;

e Konventa e Punés Detare 2006 (MLC 2006);

o Konventa Ndérkombétare pér Standardet ¢ Trajnimit, Certifikimit dhe Mbajtjes sé&
Vrojtimit pér Detarét (STCW) 1978;

o Parimet ¢ Menaxhimit t& Sigurt (Rezoluta ¢ Organizatés Ndérkombétare Detare A.
1047(27), e ndryshuar

Ndalimi, si veprim i Shtetit portual, do t& ndérmerret vetém mbi bazat e pércaktuara

né instrumentet pérkatése dhe do t& pérdoret né lidhje me késhillat nga Shteti i

flamurit. Kur njé pérgjigje ¢ tillé nuk vjen menjéheré dhe shkalla e mungesés sé

personelit &shté e tillé g& e bén anijen haptazi t& pasigurt pér udhétimin ose shérbimin

e synuar, ndalimi mund t& jeté mjeti i vetém.

Kontrolli i Personelit
Nése njé anije udhshiget né pérputhje me njé dokument t& personelit t8 sigurt ose

dokument ekuivalent t& 1&shuar nga Shteti i flamurit, Zyrtari i Kontrollit Shtetéror
Portual duhet t& pranojé qé anija &shté e drejtuar né ményré t8 sigurt, pérveg rastit kur
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2.3

2.3.1

2.3.2

dokumenti &shté 1&shuar qarté, pa marré parasysh parimet e pérfshira né instrumentet
pérkatése dhe né Udhézimet ¢ Organizatés Ndérkombétare Detare pér Zbatimin e
Parimeve t& Personelit t& Sigurt. N& kété rast t& fundit, Zyrtari i Kontrollit Shtetéror
Portual duhet t& veprojé sipas procedurave t& pércaktuara né paragrafin 2.2.3

Nése numri ose pérbérja aktuale ¢ ekuipazhit nuk konfirmon dokumentin e personelit,
Shteti i portit duhet t'i kérkojé Shtetit t& flamurit k&shilla, nése anija mund t& lundrojé
ose jo me numrin aktual t8 ekuipazhit dhe pérbérjen e saj. Njé kérkesé e tillé duhet t&
béhet sa mé shpejt qé t& jeté e mundur.

Pérgjigja nése ka, nga Shteti i flamurit, duhet t& konfirmohet me shkrim. Nése numri
dhe pérbérja aktuale e ekuipazhit nuk &shté né pérputhje me dokumentin e personelit
t& sigurt ose Shteti i flamurit nuk ké&shillon q& anija mund t& lundrojé, anija mund t&
konsiderohet pér ndalim pasi kriteret e pércaktuara né paragrafin 2.4 t& ké&saj shtojce
& jené marré né konsideraté sipas rregullave.

Nése anija nuk mban njé dokument t& personelit t& sigurt ose ekuivalent, Shteti i portit
duhet t'i kérkojé Shtetit t& flamurit t& specifikojé numrin e kérkuar t& ekuipazhit dhe
pérbérjen e tij dhe t& 18shojé njé dokument sa mé shpejt t& jeté ¢ mundur. N& rast se
numri aktual ose pérbérja ¢ ekuipazhit nuk konfirmon specifikimet e marra nga Shteti
i flamurit, zbatohet procedura ¢ parashikuar né paragrafin 2.2.2. Né&se Shteti i flamurit
nuk i pérgjigjet kérkesss, kjo do t& konsiderohet si bazé e qarté pér njé inspektim mé
t& detajuar pér t& garantuarqé numri dhe pérbérja e ekuipazhit t& jeté né pérputhje me
parimet e pércaktuara né paragrafin 2.1. Anija do t& lejohet t& vazhdojé vetém nése
&shté e sigurt pér ta béré ké&té, duke marré parasysh kriteret e ndalimit sipas paragrafit
2.4. N& ¢do rast t& tillg, standardet minimale q& do t& zbatohen nuk do t& jené mé
rigoroze se ato q& zbatohen pér anijet q& mbajné flamurin e shtetit t& portit. Mungesa
e njé dokumenti t& personelit t& sigurt do t& raportohet si mangési.

Kontrolli i Certifikimit

Kontrolli i pérgjithshém i certifikimit mbi anijet duhet t& kryhet n& pérputhje me
procedurat ¢ pércaktuara né Nenin 10 dhe n& Rregulloren 1/4 t& Konventés
Ndérkombétare pér Standardet e Trajnimit, Certifikimit dhe Rojes pér Detarét
(STCW).

Kontrolli i certifikimit mbi anijet ¢ angazhuara né transportin ¢ ngarkesave t&
rrezikshme t8 18ngshme me shumicé, duhet t& jeté mé i rrepté. Zyrtari i Kontrollit
Shtetéror Portual duhet t& bindet q8 zyrtarét pérgjegjés pér trajtimin dhe operimin e
ngarkesave t& ken& prova t& dokumentuara se kané pasur trajnimin ¢ duhur dhe
pérvojé.

Asnjé pérjashtim nga mbartja e provave té tilla dokumentuese nuk duhet t& pranohet.
Kur konstatohet njé mangési, kapiteni i anijes duhet t& informohet dhe mangésia t&
korrigjohet. N& lidhje me trajnimin e duhur, referohet kapitulli V i Konventés
Ndérkombétare pér Standardet ¢ Trajnimit, Certifikimit dhe Vrojtimit pér Detarét
STCW, Rezolutat 10, 11 dhe 12 t& miratuara nga Konferenca Ndé&rkombétare pér
Trajnimin dhe Certifikimin e Detaréve, e vitit 1978 dhe né nenet pérkatése t& Kodit
Ndérkombétar pér Ndértimin dhe Pajisjet ¢ Anijeve q& transportojné Kimikate t&
Rrezikshme me Shumicé dhe Kodin Ndérkombétar pér Ndértimin dhe Pajisjen e
Anijeve g& transportojné Gazra t& Léngshém me Shumicé.
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Ndalimi

Para ndalimit t& njé anijeje sipas paragrafit 2.2 ose 2.3 t& késaj Shtojce, duhet t&
merren parasysh rrethanat ¢ méposhtme:

Kohézgjatja dhe natyra ¢ udhé&timit ose shérbimit t& synuar;

Nése mungesa pérbén apo jo rrezik pér anijen, personat né bord ose mjedisin;
Nése mund t& vézhgohen apo jo periudhat e duhura t& pushimit t& ekuipazhit;
Madhésia dhe 1loji i anijes dhe pajisjeve té ofruara;

Natyra e ngarkesave

S R, S0 b (e

Mungesa e njé oficeri t8 kuvertés ose inxhinierit qé kérkohet t& certifikohet, nuk duhet
t& jeté arsye pér ndalim kur mungesa &shté né& pérputhje me ndonjé dispozité t&
jashtézakonshme t& miratuar nga shteti i flamurit.

Seksioni 3  Konventa e Punés Detare, 2006 (MLC 2006) ose Konventa e Transportit

3.1

3.1.1

3.2

3.21

B )

Tregtar (Standardet Minimale), 1976 (Nr. 147) dhe Protokolli ILO 147,
1966, nése éshté e zbatueshme

Konventa ¢ Punés Detare, 2006 (MLC, 2006), nése &shté e zbatueshme

N& ushtrimin e kontrollit t8 MLC, 2006, Zyrtari i Kontrollit Shtetéror Portual do t&
vendosé, né bazé t& arsyeve té qarta té renditura né Shtojcén 3 dhe gjykimit t& tij/saj
profesional, nése anija do t& marré njé inspektim mé t& detajuar. Té gjitha ankesat &
nuk jané haptazi t& pabazuara né lidhje me kushtet né bord, do t& hetohen térésisht dhe
do t& ndérmerren veprime sipas gjykimit t& tij/saj, pér t& pércaktuar nése kushtet né
bord shkaktojnd rrezik pér sigurind ose shéndetin e marinaréve, c¢ka kérkon
korrigjimin ¢ kushteve dhe, nése &shté e nevojshme, mund ta ndalojé anijen derisa t&
ndérmerren veprimet ¢ duhura korrigjuese t& raportimit pér ndalimet.

Procedurat e raportimit pér ndalimet, jepen né Shtojcén 5.

[Zbatimi i procedurave t& Kontrolli Shtetéror Portual & jané specifike pér Konventén
¢ Punés Detare, 2006, mund t& gjendet né botimin ¢ Organizatés Ndérkombétare t&
Pungs “Udhé&zues pér zyrtarét ¢ kontrollit shtetéror portual & kryejné inspektime
sipas Konventés s& Punés Detare 2006

Konventa e Transportit Tregtar (Standardet Minimale), 1976 (Organizata
Ndérkombétare ¢ Punés 147) dhe Protokolli i Organizatés Ndérkombétare t& Punés
147, 1996, nése éshté e zbatueshme.

Inspektimet né bordin e anijeve sipas Konventés s& Transportit Tregtar (Standardet
Minimale) 1976 (Konventa ¢ Organizatés Ndérkombétare t& Punés Nr. 147) do t&
lidhen me:

Konventén pér Moshén Minimale, 1973 (Nr.138); ose Konventén pér Moshén
Minimale (Det) (E rishikuar, 1936 (Nr.58), ose Konventén pér Moshén Minimale
(Det), 1920 (Nr.7);

Konventén e Ekzaminimit Mjeké&sor (Detarét), 1946 (Nr.73),

Konventén pér Parandalimin e Aksidenteve (Detarét), 1970 (Nr.134) (Nenet 4 dhe 7);
Konventén e Akomodimit t& Ekuipazheve (E rishikuar), 1949 (N1.92),

Konventén e Ushqimit dhe Kateringut (Ekuipazhet e Anijeve), 1946 (Nr.68) (Neni 5);
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3.4

3.5

3.6

Konventén pér Certifikatat ¢ Kompetencés s& Oficeréve/Zyrtaréve, 1936 (Nr.53)
(Nenet 3 e 4).

Inspektimi né lidhje me certifikatat ¢ kompetencés trajtohet né nenin 2 t& késaj
Shtojce. N& ushtrimin e kontrollit t& Konventave t& listuara mé sipér nga (1) deri né
(6), Zyrtari i Kontrollit Shtetéror Portual do t& vendosé né bazé t& arsyeve t& qarta t&
renditura n& Shtojcén 3 dhe duke pasur parasysh pérshtypjen e tij t& pérgjithshme mbi
anijen, do t& duhet t& ushtrojé gjykimin e tij profesional pér t& vendosur nése anija do
t& marré nj& inspektim mé t8 detajuar. T¢ gjitha ankesat né lidhje me kushtet ng bordin
e anijes duhet t& hetohen térésisht dhe t& ndérmerren veprime sipas nevojés nga
rrethanat. Ai do t& ushtrojé gjithashtu gjykimin e tij profesional pér t& pércaktuar nése
kushtet n& bord sjellin rrezik pér siguring ose shéndetin e ekuipazhit g8 kérkon
korrigjimin ¢ kushteve dhe, nése &shté e nevojshme, mund ta ndalojé anijen derisa t&
ndérmerren veprimet ¢ duhura korrigjuese. Procedurat e raportimit pér ndalimet, jepen
né Shtojcén 5.

Pér aq kohé& sa ka arsye t& qarta pér njé inspektim mé t& detajuar né lidhje me
dispozitat ¢ Konvent&s Nr.147 t& Organizatés Ndérkombétare t& Punés, gjaté kryerjes
s& njé inspektimi, Zyrtari i Kontrollit Shtetéror Portual do t& marré parasysh
paragrafin ¢ méparshém n& ké&t& nen dhe konsideratat ¢ dhéna né& publikimin e
Organizatés Ndérkombétare t& Punés “Inspektimi i kushteve t& punés né bordin e
anijes: Udh&zime pér procedurén”.

Konventat pérkatése né kuadrin e dispozitave t& paragrafit 3.5, jan&:

1. Konventa ¢ Marréveshjes pér Nenet e Detaréve, 1926 (Nr. 22),
Konventa ¢ Riatdhesimit t& Detaréve 1926 (Nr. 23);

3. Konventa pér pérgjegjésiné e¢ pronaréve t& anijeve (Detarét ¢ Sémuré dhe t&
Lénduar), 1936 (Nr.55); ose Konventa ¢ Sigurimit t& Sémundjeve (Detit), 1936
(Nr. 56); ose Konventa pér Kujdesin Mjeké&sor dhe Pérfitimet ¢ Sémundjeve, 1969
(Nr. 130);

4. Konventa pér Liring e Asociimit dhe Mbrojtjen e t& Drejtés pér Organizim, 1948

(Nr.87);

Konventa pér t& Drejtén pér Organizim dhe Marréveshje Kolektive, 1949 (Nr. 98);

Konventa ¢ Dokumenteve t& Identitetit t& Detaréve, 1958 (Nr. 108);

Konventa ¢ Pérfagésuesve t& Punétoréve, 1971 (Nr. 135);

Konventa pér Mbrojtjen e Shéndetit dhe Kujdesit Mjekésor (Detarét), 1987

(Nr.164);

9. Konventa e Riatdhesimit t& Detaréve (E rishikuar), 1987 (Nr. 166).

PO L 28 1

Nése Zyrtari i Kontrollit Shtetéror Portual merr njé ankesé se standardet e pércaktuara
né Konventat ¢ renditura né paragrafin 3.4 nuk jan& p&rmbushur, ¢éshtja duhet t&
raportohet né pérfagésingé mé t& afért detare, konsullore ose diplomatike t& shtetit t&
flamurit pér veprime t& métejshme. Nése ¢mohet ¢ nevojshme, Autoriteti pérkatés
mund t8 pérgatisé njé raport pér shtetin e flamurit, nése &shté e mundur me prova, me
njé kopje pér Organizatén Ndérkombétare t& Punés.

Ato pjesé t& botimit t& Organizatés Ndérkombétare t& Punés “Inspektimi i Kushteve t&
Punés né Bordin e Anijes: Udh&zime pér proceduré” t& cilat lidhen me:
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1. Procedurat e kontrollit pér anijet me flamur kombétar;
2. Formimin profesional;

3. Certifikatat e kompetencés sé zyrtarit;

4. Orarin ¢ punés dhe personelit;

Nuk duhet t& konsiderohen si dispozita pérkatése pér inspektimin e anijeve, por si
informacion vetém pér Zyrtarét e Kontrollit Shtetéror Portual.

Seksioni 4  Udhézimet pér kontrollorét qé duhen respektuar né inspektimin e anijeve

4.1

4.1.1

4.1.2

4.1.3

4.2

4.2.1

4.2.2

4.2.3

té ngarkesave nén 3500 toné tonazhi bruto dhe anijet e ndértimit
tradicional

Anije mallrash mesdhetare nén 500 toné tonazh bruto

ME poshté jepet njé udhézues pér zbatimin e nenit 2.5 t& Memorandumit né lidhje me
anijet e ngarkesave mesdhetare nén 500 toné& tonazh bruto.

Autoritetet q& kan& pranuar dhe zbatuar “Rregulloret Mesdhetare t& Sigurisé sé
Anijeve t& Mallrave” né anijet e tyre, né masén qé njé instrument pérkatés nuk &shté i
zbatuesh8m pér njé anije nén 500 ton& tonazh bruto; udh&higen nga rregulloret né
fjalé.

Autoritetet q& nuk mund t& zbatojné dispozitat e paragrafit 4.1.2 mé sipér, né masén
qé njé instrument pérkatés nuk &shté i zbatueshdm pér njé anije nén madhé&sing e
Konventss, detyra e Zyrtarit t& Kontrollit Shtetéror Portual do t& jeté gé t& vlerésojé
nése anija &shté e njé standardi t& pranueshém t& lidhur me siguring, shéndetin apo
mjedisin. N& kryerjen e kétij vler&simi, Zyrtari i Kontrollit Shtetéror Portual do t&
marré parasysh faktoré t& tillé si koh&zgjatja dhe natyra ¢ udhé&timit ose shérbimit t&
synuar, madhésia dhe 110ji i anijes, pajisjet e ofruara dhe natyra e ngarkesés.

Anije té Ndértimit Tradicional

MEé poshté jepet njé udhézues pér zbatimin e nenit 2.5 té¢ Memorandumit né
lidhje me anijet e ndértimit tradicional

N& masén q& njé instrument pérkatés nuk &shté i zbatueshém pér njé anije t& ndértimit
tradicional, detyra ¢ Zyrtarit t& Kontrollit Shtetéror Portual do t& jeté q& t& vlerésojé
nése anija shté e njé standardi t& pranueshém né lidhje me siguring, shéndetin ose
mjedisin. N& kryerjen e kétij vler&simi, Zyrtari i Kontrollit Shtetéror Portual do t&
marré parasysh faktoré t& tillé si koh&zgjatja dhe natyra ¢ udhé&timit ose shérbimit t&
synuar, madhésia dhe 1loji i anijes, pajisjet e ofruara dhe natyra e ngarkesés.

N& ushtrimin e funksioneve t& tij sipas paragrafit 2.2, Zyrtari i Kontrollit Shtetéror
Portual duhet t& udh&hiqet nga ¢do certifikaté dhe dokument tjetér i l&shuar nga Shteti
i flamurit. Zyrtari i Kontrollit Shtetéror Portual, duke pasur parasysh kéto certifikata
dhe dokumente dhe nén pérshtypjen e tij t& pérgjithshme pér anijen, do t& ushtrojé
gjykimin e tij profesional pér t& vendosur nése dhe né ¢faré aspekti, anija do t& marré
njé inspektim mé t& detajuar, duke marré parasysh faktorét e pérmendur né paragrafin
2.2. Kur kryen njé inspektim mé t& detajuar, Zyrtari i Kontrollit Shtetéror Portual ng
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masén & ¢ gmon t& nevojshme, do t'u kushtojé vémendje pikave t& renditura ng
paragrafin 2.4. Lista nuk merret parasysh.

Artikuj me réndési té pérgjithshme

4.2.4.1 Zérat q& lidhen me kushtet ¢ caktimit t& linjave t8 ngarkesés:

1. Integriteti i ngusht& i motit t& kuvertave t& ekspozuara (ose t& papérshkueshme nga
uji, sipas rastit);

Celésat dhe pajisjet mbyllése;

Mbylljet e ngushta ndaj hapjeve né superstruktura;

Marréveshjet e lirimit;

Daljet ansore;

Ventilatorét dhe gypat e ajrit;

Informacioni i stabilitetit.

SO Wi N

4.2.4.2 Artikyj t& tjeré q& lidhen me siguring e jet8s né det:

1. Pajisjet pér shpétimin e jetés;

2. Aparatet kundér zjarrit;

3. Kushtet e pérgjithshme strukturore (d.m.th. byk, kuvert&, mbulesa t& kapakut etj.);
4. Makinerité kryesore dhe instalimet elektrike;

5. Pajisjet e lundrimit, duke pérfshiré instalimet radio.

4.2.4.3 Artikujt g8 lidhen me parandalimin e ndotjes nga anijet:

4.2.5

6. Mjete pér kontrollin e shkarkimit t& vajit dhe pérzierjeve vajore, p.sh., ndarja e ujit
vajor ose mjete t& tjera ekuivalente (rezervuar(et)) pér mbajtjen e vajit, pérzierjeve
vajore, mbetjeve t& vajit;

7. Prania e vajit né avullimin e motorit.

N& rastin e manggsive q& konsiderohen pér siguring, shéndetin ose mjedisin, Zyrtari i
Kontrollit Shtetéror Portual do t& ndérmarré veprime t& tilla, t& cilat mund t&
pérfshijné ndalimin sipas nevojés, duke pasur parasysh faktorét e pé&rmendur ng
paragrafin 2.2, pér t& garantuar g8 mungesa t& korrigjohet ose & anija, nése lejohet t&
vazhdojé né njé port tjetér, nuk paraqet rrezik t& qarté pér siguring, shéndetin ose
mjedisin.
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SHTOJCA 2

PROCEDURAT PER HETIMET SIPAS MARPOL 73/78

Pérmbajtja

Seksioni 1 Procedurat pér kérkesat e shkarkimit sipas Shtojcave I dhe II té
MARPOL 73/78

Seksioni 2  Kundérshtimi i dispozitave té shkarkimit sipas Shtojcés I t¢ MARPOL
73/78

Seksioni 3  Lista e detajuar e provave té mundshme mbi shkeljen e pretenduar té
dispozitave té shkarkimit té Shtojcés I t¢ MARPOL 73/78

3.1 Veprimi pér shikimin e ndotjes nga nafta

3.2 Hetimi né bord

3.3 Hetimi né& breg

3.4 Informacioni q& nuk mbulohet nga sa mé sipér
3.5 Pérfundime

Seksioni 4  Shkelje e dispozitave té shkarkimit sipas Shtojcés II t¢ MARPOL 73/78

Seksioni 5  Lista e detajuar e provave té mundshme mbi shkeljen e pretenduar té
dispozitave té shkarkimit té Shtojcés II té¢ MARPOL 73/78

5.1 Veprimi pér shikimin e ndotjes

5.2 Hetimi né bord

5.3 Hetimi né breg

5.4 Informacioni q& nuk mbulohet nga sa mé sipér
5.5 Pérfundime




image21.jpg
Seksioni 1 Procedurat pér kérkesat e shkarkimit sipas Shtojcave I dhe II té

MARPOL
73/78
1.1 Duke vepruar né bazé t& njé raporti ose njoftimi pér njé shkelje t& pretenduar t&

1.2

1.3

kérkesave t& shkarkimit sipas Shtojecave I dhe II t& MARPOL 73/78, Zyrtari i
Kontrollit Shtetéror Portual do t& udh&higet nga procedurat ¢ pércaktuara né nenet 2
dhe 3 t& ké&saj Shtojce né lidhje me hetimet pér shkeljen e pretenduar t& dispozitave t&
shkarkimit t& Shtojcés It8 MARPOL 73/78 dhe n& nenet 4 dhe 5 t& késaj Shtojce né
lidhje me hetimet pér shkeljen e pretenduar t& dispozitave t& shkarkimit t& Shtojeés II
t& MARPOL 73/78.

Kur ushtron kontroll mbi shkeljet e pretenduara t& kérkesave t8 shkarkimit sipas
shtojcave I dhe II t& MARPOL 73/78, Zyrtari i Kontrollit Shtetéror Portual do t'i
kushtojé vémendje dispozitave 4.3.1 dhe 4.3.2 t& Rezolutés A. 1052(27) t&
Organizatés Ndérkombétare Detare, t& ndryshuar dhe Shtojcés 3 t& s& njéjtés
Rezoluté, dhe udhézimeve t& Administratés Shtetérore té Portit, bazuar né kéto
dispozita.

N& rast se hetimi i tij zbulon manggsi q& jang haptazi t& rrezikshme pér siguring,
shéndetin ose mjedisin, Zyrtari i Kontrollit Shtetéror Portual do t& zbatojé dispozitat e
3.6.3 t& Memorandumit.

Seksioni 2 Shkelja e dispozitave té shkarkimit sipas Shtojcés I t¢ MARPOL 73/78

2.1

2.2

2.3

Dispozitat ¢ neneve 2 dhe 3 t& k&saj Shtojce synojné t& identifikojné informacionin qé
shpesh i nevojitet njé administrate shtetérore t& flamurit pér ndjekjen penale t&
shkeljeve t& tilla t& mundshme.

Rekomandohet q& né pérgatitien e njé raporti t8 kontrollit shtetéror portual pér
mangésité, ku pérfshihet shkelje ¢ kérkesave t& shkarkimit, autoritetet e shtetit
bregdetar ose portual t& udh&higen nga lista ¢ detajuar e provave t& mundshme, sig
specifikohet né nenin 3 t& k&saj shtojce. N¢& lidhje me kété duhet pasur parasysh se:

1. Raporti synon t& garantojé renditjen optimale t& t& dhénave t& arritshme;
megjithaté, edhe nése i gjithé informacioni nuk mund t& jepet, duhet t& dorézohet
sa mé shumé informacion & t& jeté e mundur,

2. Eshts e réndésishme qé t& gjitha informacionet e pérfshira né raport t& mbéshteten
nga fakte t& cilat, kur konsiderohen né térési, do ta shtynin portin ose shtetin
bregdetar t& besonte se ka ndodhur njé shkelje.

Pérveg raportit t& kontrollit shtetéror portual pér manggsité, njé raport duhet t&
plotésohet nga njé shtet port ose bregdetar, mbi bazén e listés s& detajuar t& provave t&
mundshme. Fshté e réndésishme qé kéto raporte t& plotdsohen me dokumente té& tilla
si:

1. Njé deklaraté nga vézhguesi i ndotjes. Pérveg informacionit t& kérkuar né pikén
3.1 t& ké&saj Shtojce, deklarata duhet t& pérfshijé konkluzione g8 e ¢ojné
vézhguesin né pérfundimin se asnjé nga burimet e tjera t& mundshme t& ndotjes
nuk é&shté né fakt burimi;
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2. Deklaratat né lidhje me procedurat e marrjes s& mostrave si té njollave t8 naftés ng
det ashtu edhe né bord. Ké&to duhet t& pérfshijng vendndodhjen dhe kohén kur jang
marré mostrat, identitetin ¢ personave (& marrin mostrat dhe faturat q&
identifikojné personat q& kané pérgjegjésiné dhe marrin transferimin e mostrave;

3. raportet ¢ analizave t& mostrave t& marra t& njollave t& naftés n& det dhe né bord,
raportet duhet t& pérfshijné rezultatet e analizave, njé pérshkrim t& metodés sé&
pérdorur, referencé ose kopje t& dokumentacionit shkencor q& vérteton saktésing
dhe vlefshméring e metodés s& pérdorur dhe emrat e personave & kryejné analizat
dhe pérvojén e tyre;

4. njé deklaraté nga Zyrtari i Kontrollit Shtetéror Portual né bord s& bashku me

gradén dhe organizimin e Zyrtarit t& Kontrollit Shtetéror Portual;

deklaratat e personave t& pyetur;

deklaratat ¢ déshmitaréve;

fotografi t& njollave t& naftés;

Kopje t& fageve pérkatése t& Librave t& Regjistrimit t& Naftés, regjistrave,

regjistrimeve t& shkarkimeve et;.

PO L BN

Té gjitha vézhgimet, fotografité dhe dokumentacioni duhet t& mbéshteten nga njé
verifikim i nénshkruar i autenticitetit t& tyre. T& gjitha vértetimet, autentikimet ose
verifikimet do t& ekzekutohen né& pérputhje me ligjet e shtetit q& i pérgatit ato. T&
gjitha deklaratat duhet t& nénshkruhen dhe datohen nga personi qé bén deklaratén dhe,
nése &shté ¢ mundur, nga njé déshmitar i nénshkrimit. Emrat ¢ personave qg
nénshkruajné deklaratat duhet t& shtypen me shkrim t& lexueshém sipér ose poshté
nénshkrimit.

2.4  Raporti i pérmendur n& paragrafét 2.2 dhe 2.3 t8 késaj shtojce duhet t'i dérgohet
Administratés sé Shtetit t& Flamurit. Nése shteti bregdetar 8 vézhgon ndotjen dhe
shteti portual g& kryen hetimin né bord nuk jané t& nj&jté, shteti q& kryen hetimin e
fundit duhet t'i dérgojé gjithashtu njé kopje t& konstatimeve té tij shtetit g& vézhgon
ndotjen dhe kérkon hetimin.

Seksioni 3 Lista e detajuar e provave té¢ mundshme mbi shkeljen e pretenduar
té

dispozitave té shkarkimit té Shtojcés I t¢ MARPOL 73/78
3.1 Veprimi pér shikimin e ndotjes nga nafta
3.1.1 T& dhénat ¢ anijes ose anijeve t& dyshuara pér shkelje

Emri i anijes

Arsyet pér t& dyshuar né anije

Data dhe ora (Koha Universale ¢ Koordinuar) ¢ vézhgimit ose identifikimit
Pozicioni i anijes

Flamuri dhe porti i regjistrit

Lloji (p.sh. cisterng, anije mallrash, anije pasagjerésh, anije peshkimi), madhé&sia
(tonazhi i vler&suar) dhe t& dhéna té tjera pérshkruese (p.sh. ngjyra e mbistrukturés
dhe shenja e oxhakut)

7. Gjendja e thellésisé s& lundrimit (me ngarkesé ose me balaste)

8. Kursi dhe shpejtésia e pérafért

OF o s i 97 b
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3.1.2

3.1.3

3.1.4

9.

10.
11.

Pozicioni i njollave t& naftés n& lidhje me anijen (p.sh. bordi I majté, bordi i
djatht&)

Njé pjesé e anijes nga e cila &shté paré shkarkimi anésor

Nése shkarkimi ndaloi kur anija u vézhgua, ose u kontaktua me radio

T& vegantat e njollave t& naftés né det

1.

=

14.
15.
16.

Data dhe ora (Koha Universale e Koordinuar) e vézhgimit nése jané t& ndryshme
nga paragrafi 3.1.1.3 i k&saj Shtojce;

Pozicioni i njollave t& naftés né& gjatési dhe gjerési gjeografike nése &shté i
ndryshém nga paragrafi 3.1.1.4 i késaj Shtojce;

Distanca e pérafért né milje detare nga pika e referimit mé e afért;

Dimensioni i pérgjithshém i pérafért i njollés s& naftés (koh&zgjatja, gjerésia dhe
pérqindja e saj ¢ mbuluar me naftg),

Pérshkrimi fizik i njollave t& naftés (drejtimi dhe forma p.sh. e vazhdueshme, ng
copa ose né vargje t& gjaté);

Paraqitja e njollave t& naftés (specifikoni kategorité),

Kategoria A: Mezi e dukshme né kushtet mé t& favorshme t& drités;

Kategoria B: E dukshme si shkélqim argjendi né sipérfaqgen e ujit;

Kategoria C: Mund t& vérehet gjurma e paré e ngjyrés;

. Kategoria D: Shirit t& ndritshém t& ngjyrave,

. Kategoria E: Ngjyrat fillojné t& zbehen;

. Kategoria F: Ngjyrat jané shumé mé t& erréta;

. Kushtet e giellit (diell i shndritshém, vrandsira etj.), rénia e drités dhe dukshméria

(n& kilometra) né momentin ¢ vézhgimit;
Shteti detar;

Drejtimi dhe shpejtésia e erés sipérfagésore;
Drejtimi dhe shpejtésia e rrymés.

Identifikimi i vézhguesit(ve)

AR S

Emri i vézhguesit;

Organizata me té cilén vézhguesi &shté i lidhur (nése ka);

Statusi i vézhguesit brenda organizatés;

Vézhgimi i kryer nga avioni/anija/bregu/ndryshe;

Emri ose identiteti i anijes ose avionit nga i cili &shté kryer vézhgimi,
Vendndodhja specifike e anijes, avionit, vendit né breg ose né ndonjé ményré
tjetdr nga i cili &shté kryer vézhgimi;

Veprimtaria ¢ kryer nga vézhguesi kur kryhej vézhgimi, p.sh.: patrullg, lundrim,
fluturim (gjaté rrugés nga .... né ....), etj.

Meényra e vézhgimit dhe dokumentimi

N N =

Pamore;

Fotografi konvencionale;

Té dhénat me sensoré né distancé dhe/ose fotografi me sensoré né distancg;
Mostrat ¢ marra nga njolla e naftés;

Cdo formé tjetér vézhgimi (specifikoni);
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3.1.5

3.2

3.21

3.2.2

3.2.3

Shénim: Njé fotografi e shkarkimit preferohet t& jeté me ngjyra. Fotografité mund t&
japin informacionin ¢ méposhtém: q& njé material né sipérfaqen e detit &shté nafta; q&
sasia ¢ naftés s& shkarkuar pérbén shkelje t& Konventés, q& nafta &ht& duke u
shkarkuar ose &shté shkarkuar nga njé anije e caktuar; dhe identitetin ¢ anijes.

Pérvoja ka treguar se sa mé sipér mund t& merren me tre fotografité e méposhtme:

1. detajet e njollés s& naftés t& marra pothuajse vertikalisht poshté nga njé lartési prej
mé pak se 300 metra me diellin pas fotografit;

2. njé pamje e pérgjithshme e anijes dhe “njollés s& shké&lqyeshme™ & specifikon
naftén g& buron nga njé anije e caktuar; dhe

3. detajet e anijes pér géllime identifikimi.

Informacione t& tjera nése mund t& vendoset kontakti me radio

Kapiteni i informuar pér ndotjen
Shpjegimi i Kapitenit

Porti i fundit i thirrjes s& anijes

Porti tjetér i thirrjes sé anijes

Emri i kapitenit dhe pronarit t& anijes
Shenja e thirrjes s& anijes

ANE DN

Hetimi né bord
Inspektimi i Certifikatés Ndérkombétare t& Parandalimit t& Ndotjes s& Naftés

Emri i anijes

Numri ose shkronjat dalluese
Porti i regjistrit

Lloji i anijes

Data dhe vendi i 1&shimit
Data dhe vendi i miratimit

AN R DN

Shénim: Nése anijes nuk i 8shté 1&shuar njé Certifikaté Ndérkombétare ¢ Parandalimit
t& Ndotjes s& Naftés (IOPP), duhet t& jepet sa mé& shumé nga informacioni i kérkuar.

Inspektimi i Suplementit t& Certifikatés Ndérkombétare t& Parandalimit t& Ndotjes s&
Naftés (IOPP)

1. Paragrafét ¢ zbatueshém t& neneve 2, 3, 4, 5 dhe 6 t& shtojcss sé& Certifikatés
Ndérkombétare t8 Parandalimit t& Ndotjes s& Naftés (cisterna jonaftémbajtése)

2. Paragrafét e zbatueshém t& neneve 2, 3, 4, 5, 6, 7, 8, 9 dhe 10 t& suplementit t&
Certifikatés Ndérkombétare t& Parandalimit t& Ndotjes s& Naftés (cisterna
naftémbajtése)

Shénim: Nése anija nuk ka njé Certifikaté Ndérkombétare t& Parandalimit t& Ndotjes
s& Naftés, duhet t& jepet njé pérshkrim i pajisjeve dhe materialeve né bord, t&

projektuara pér t& parandaluar ndotjen detare.

Inspektimi i Librit t& Regjistrimit t8 Naftss
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1.

2

Fage e mjaftueshme t& Librit t& Regjistrimit t& Naft&s - Pjesa I duhet t& kopjohet
pér t& mbuluar njé periudhé prej 30 ditésh para incidentit t& raportuar

Faget e mjaftueshme t& Librit t& Regjistrimit t& Naftés - Pjesa II (nése n& bord)
duhet t& kopjohen pér t& mbuluar njé cikél t& ploté ngarkimi/shkarkimi/gaké&llimi
dhe pastrimi t& rezervuarit t& anijes. Duhet t& merret gjithashtu njé kopje e
diagramit t& rezervuarit.

3.2.4 Inspektimi i regjistrit

3.2.5

3.2.6

3.2.7

O =

Porti i fundit, data e nisjes, zhytja e anijes para dhe pas

Porti aktual, data e mbérritjes, zhytja e anijes para dhe pas

Pozicioni i anijes né ose afér kohds kur u raportua incidenti

Kontrolli né vend nése pozicionet e pérmendura né librin ¢ ditarit p&rputhen me
pozicionet e shénuara né Librin ¢ Regjistrimeve t& Naftés. (ORB)

Inspektimi i dokumentacionit tjetér né bord

Dokumentacion tjetér i pérshtatshém pér prova (nése &shté e nevojshme béni kopje)

si:
1.
2.

fletét e fundit t& ulazhit;
t& dhénat e pajisjeve t& monitorimit dhe kontrollit.

Inspektimi i anijes

1.

Nk W

SN

Pajisjet e anijes né pérputhje me suplementin ¢ Certifikatés Ndérkombétare t&
Parandalimit t& Ndotjes s& Naftés;

Mostrat ¢ marra. Vendndodhja né bord,

Gjurmét e naftés né aférsi té pikave t& shkarkimit né det;

Gjendja e motorrit dhe pérmbajtja e bishtave;

Gjendja e ndarésit t& ujit nga nafta (seperatori), pajisjet ¢ filtrimit dhe alarmit,
mjetet ¢ ndalimit ose monitorimit;

Mbajtéset e llumit(sludge) dhe/ose rezervuaréve mbajtés;

Burimet e rrjedhjeve t& mundshme;

Pér cisternat e naftés, provat e méposhtme shtesé mund t& jené t& pérshtatshme:
Nafté né sipérfagen e balasteve t& pastér t& veguar ose t& dedikuar

Gjendja e ujrave t& ndotur t& sallés s8 pompés

Gjendja e sistemit t& larjes s& naftés s& papérpunuar

Gjendja e sistemit t& gazit inert

Gjendja e sistemit t& monitorimit dhe kontrollit

Pé&rmbajtja e rezervuarit (llogaritni sasing e ujit dhe naftés)

o aoe o

Deklaratat ¢ personave t& interesuar

Nése Pjesa I e Librit t& Regjistrimit t& Naftés nuk &shté plotésuar si¢ duhet,
informacioni pér pyetjet ¢ méposhtme mund té8 jets me vend:

1.

2.

A ka pasur njé shkarkim (aksidental apo t& géllimshém) né& kohén e treguar né
raportin e incidentit?
A kontrollohet automatikisht shkarkimi i ujrave t& ndotura?
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3.3

3.3.1

Al

9.
10.

11.
12.
13.
14.
15.

16.
17.
18.

19.

20.
21.

22.
23.
24.

25.
26.
27.

28.
29.
30.
31.
32.
33.

Nése po, né cilén oré &shté véné n& funksion pér heré t& fundit ky sistem dhe né
cilén oré &shté véné pér heré t& fundit ky sistem né modalitetin manual?

Nése jo, cila ishte data dhe ora e shkarkimit t& fundit t& derdhjes?

Cila ishte data e asgjésimit t& fundit t& mbetjeve dhe si u krye asgjésimi?

A &shté e zakonshme t& kryhet shkarkimi i ujit t& kullimit direkt n& det, apo t&
ruhet fillimisht n& njé rezervuar grumbullimi? Identifikoni rezervuarin e
grumbullimit

A jané pérdorur kohét e fundit rezervuarét ¢ karburantit t& naftés si rezervuarg
balasti?

Nése Pjesa II e Librit t& Regjistrimit t& Naftés nuk &shté plotésuar si¢ duhet,
informacioni pér pyetjet ¢ méposhtme mund t8 jeté me vend:

Cila ishte shpérndarja e ngarkesés/balasteve né anije né nisje nga porti i fundit?
Cila ishte shpérndarja e ngarkesés/balasteve né anije me mbérritjen né portin
aktual?

Kur dhe ku &shté cénuar ngarkimi i fundit?

Kur dhe ku &shté kryer shkarkimi i fundit?

Kur ka gené shkarkimi i fundit i balasteve t& pista?

Kur dhe ku ishte pastrimi i fundit i rezervuaréve t& mallrave?

Kur dhe ku ka gené& operacioni i fundit i larjes s& naftés bruto dhe cilat depozita
jang laré?

Kur dhe ku ka gené dekantimi i fundit i rezervuaréve t& slopeve?

Sa &shté ulazhi né rezervuarét e slopeve dhe lartésia pérkatése e matjes?

Cilét rezervuaré pérmbanin balastin ¢ ndotur gjaté udhé&timit me balaste (nése
anija arrinte me balaste)?

Cilét rezervuaré pérmbanin balaste t& pastér gjaté udhétimit me balaste(nése anija
arrinte me balaste)?

Pérveg késaj, informacioni i méposhtém mund t& jeté me vend:

Detajet e lundrimit aktual t& anijes (portet ¢ méparshme, portet e ardhshme,
udhétimi)

Pé&rmbajtja e karburantit t& naftés dhe rezervuaréve té balastit.

Rezervuari i méparshém dhe i ardhshém i karburantit, 1loji i karburantit t& naftés
Disponueshméria ose mosdisponueshméria e kompanive t& terheqjes pér mbetjet e
vajore gjaté lundrimit aktual

Transferimi i brendshém i karburantit gjaté lundrimit aktual

N& rastin e cistenave, informacioni shtesé i méposhtém mund t& jeté me vend:
Udhétimi né t& cilén angazhohet anija, si p.sh. né distanca t& shkurtra/té gjata,
bruto ose produkt, ose bruto/produkt i alternuar, ngarkesa te ndezshme,
vajore/ngarkesa t& thata

Cilét rezervuaré jané t& pastér dhe cilét t& ndotur?

Riparimet e kryera ose t& parashikuara né depozita mallrash

Informacione t& ndryshme:

Komente né lidhje me gjendjen e pajisjeve t& anijes

Komentet né lidhje me raportin ¢ ndotjes

Komentet e tjera

Hetimi né breg

Analizat e mostrave té naftés

Specifikoni metodén dhe rezultatet e analizave t& mostrave
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3.3.2

3.4

3.5

3.51

3.5.2

3.5.3

Informacione t8 métejshme

Informacione shtesé mbi anijen, t& marra nga stafi i terminalit t& naftés, kontraktorét e
pastrimit t& rezervuaréve ose objektet e pritjes né breg mund t& jené t& pérshtatshme.

Shénim: Cdo informacion nén ké&té titull, nése &shté ¢ mundur, duhet t& vértetohet me
dokumentacion t& tillé si deklarata t& nénshkruara, fatura, déftesa, etj.

Informacion q& nuk mbulohet nga sa mé sipér
Pérfundim
Pérmbledhja e konkluzioneve teknike t& hetuesit

Tregimi i dispozitave t& zbatueshme t& Shtojcés It& MARPOL 73/78 t& cilat dyshohet
se anija i ka shkelur.

A garantuan rezultatet ¢ hetimit paraqitjen e njé raporti t& mangésive?

Seksioni 4  Shkelja e dispozitave té shkarkimit sipas Shtojcés IT té¢ MARPOL 73/78

4.1

4.2

4.3

Dispozitat ¢ neneve 4 dhe 5 t& k&saj Shtojce synojné t& identifikojné informacionin qé
do t'i nevojitet njé administrate shtetérore t& flamurit pér ndjekjen penale t& shkeljeve
t& dispozitave t& shkarkimit sipas Shtojcés II t&€ MARPOL 73/78.

Rekomandohet & né& pérgatitjen e njé raporti t& Kontrollit Shtetéror Portual mbi
mangésité, ku pérfshihet shkelja e kérkesave t& shkarkimit, autoritetet e njé shteti
bregdetar ose portual do t& udhshiqen nga lista e detajuar e provave t& mundshme si¢
specifikohet né seksionin 5 t& késaj Shtojce. N& lidhje me kété duhet pasur parasysh
se:

1. raporti synon t& garantojé renditjen optimale t& t& dhénave t& bindshme;
megjithaté, edhe nése i gjithé informacioni nuk mund t& jepet, duhet t& dorézohet
sa mé shumé informacion & t& jeté e mundur; dhe

2. &shté e réndésishme qé i gjithé informacioni i p&rfshiré né raport t& mbéshtetet nga
fakte t& cilat, kur konsiderohen si njé e téré, do ta shtynin portin ose shtetin
bregdetar t& besonte se ka ndodhur njé shkelje; dhe

3. Shkarkimi mund t& keté qené nafté, né rastin e t& cilit zbatohet aneksi 2 i shtojcés
1It& aneksit I t& procedurave té kontrollit MARPOL 73/78.

Pérveg raportit t& Kontrollit Shtetéror Portual pér manggsité, njé raport duhet t&
plotésohet nga njé shtet port ose bregdetar, mbi bazén e listés s& detajuar t& provave t&
mundshme. Fshté e réndésishme qé kéto raporte t& plotésohen me dokumente t& tilla
si:

1. njé deklaraté nga vézhguesi i ndotjes. Pérveg informacionit t8 kérkuar né pikén 5.1
t& késaj Shtojce, deklarata duhet t& pérfshijé konsiderata t& cilat e kan& guar
vézhguesin né pérfundimin se asnjé nga burimet e tjera t& mundshme t& ndotjes
nuk éshté né fakt burimi;

2. Deklaratat né lidhje me procedurat ¢ marrjes s8 mostrave si t& njollave t& naftés né
det ashtu edhe né bord. Ké&to pérfshijné vendndodhjen dhe kohén e marrjes sé
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4.4

mostrave, identitetin e personit(ve) & marrin mostrat dhe faturat q& identifikojné
personat qé kang kujdestariné dhe marrin transferimin ¢ mostrave;
3. raportet ¢ analizave t& mostrave t& marra nga njollat ¢ naftés n& det dhe né bord;
raportet duhet t& pérfshijné rezultatet e analizave, njé pérshkrim t& metodés sé&
pérdorur, referencé ose kopje t& dokumentacionit shkencor q& vérteton saktésing
dhe vlefshméring e metodés s& pérdorur dhe emrat e personave gé kryejné analizat
dhe pérvojén e tyre;
njé deklaraté nga Zyrtari i Kontrollit Shtetéror Portual né bord s& bashku me
gradén dhe organizatén e Zyrtarit t& Kontrollit Shtetéror Portual;
deklaratat e personave t& pyetur;
deklaratat ¢ déshmitaréve;
fotografi t& njollave t& naftés né det; dhe
kopje t& faqeve pérkatése t& Librit t& Regjistrimit t& Transportit, regjistrave,
regjistrimeve té shkarkimeve et;.

=

® A

Té gjitha vézhgimet, fotografité dhe dokumentacioni duhet t& mbéshteten nga njé
verifikim i nénshkruar i origjinalitetit t& tyre. T& gjitha vértetimet, origjinalitetet ose
verifikimet do t& ekzekutohen né& pérputhje me ligjet e shtetit q& i pérgatit ato. T&
gjitha deklaratat duhet t& nénshkruhen dhe datohen nga personi qé bén deklaratén dhe,
nése &shté ¢ mundur, nga njé déshmitar i nénshkrimit. Emrat ¢ personave q&
nénshkruajné deklaratat duhet t& shtypen me shkrim t8 lexueshém sipér ose poshté
nénshkrimit.

Raporti i pérmendur né paragrafét 4.2 dhe 4.3 t& késaj Shtojce duhet t'i dérgohet
Administratés sé& Shtetit t& Flamurit. Nése shteti bregdetar 8 vézhgon ndotjen dhe
shteti portual g& kryen hetimin né bord nuk jané t& nj&jté, shteti q& kryen hetimin e
fundit duhet t'i dérgojé gjithashtu njé kopje t& konstatimeve té tij shtetit g& vézhgon
ndotjen dhe kérkon hetimin.

Seksioni 5  Lista e detajuar e provave té mundshme mbi shkeljen e pretenduar té

51

511

dispozitave té shkarkimit té Shtojcés II té¢ MARPOL 73/78
Veprimi pér shikimin e ndotjes
T& dhénat ¢ anijes ose anijeve t& dyshuara pér shkelje

Emri i anijes

Arsyet pér t& dyshuar né anije

Data dhe ora (Koha Universale ¢ Koordinuar) e vézhgimit ose identifikimit

Pozicioni i anijes

Flamuri dhe porti i regjistrit

Lloji, madhé&sia (tonazhi i vlerésuar) dhe t& dhéna t& tjera pérshkruese (p.sh.

superstruktura, ngjyra dhe shenja e hinkés)

Gjendja e thellésisé s& lundrimit (me ngarkesé ose me ¢akéll)

8. Kursi dhe shpejtésia e pérafért

9. Pozicioni i njollave t& naftés n& det né lidhje me anijen (p.sh. né anén ¢ pasme,
portin, n& anén e djatht&)

10. Nj& pjesé ¢ anijes, nga e cila u pa shkarkimi

11. Nése shkarkimi pushoi kur anija u vézhgua ose u kontaktua me radio

AN R DN

bl
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5.1.2 Té vecantat e njollés sé naftés

1.

Il

T
8.

9.

Data dhe ora (Koha Universale e Koordinuar) e vézhgimit nése jané t& ndryshme
nga paragrafi 5.1.1.3 i k&saj Shtojce

Pozicioni i njollés s& naftés né gjatési dhe gjerési gjeografike ndse &shté i
ndryshém nga paragrafi 5.1.1.4 i k&saj Shtojce

Distanca ¢ pérafért né milje detare nga toka mé e afért

Thell&sia e ujit sipas grafikut detar

Matja e pérafért i pérgjithshém i njollés s& naftés (kohézgjatja, gjerésia dhe
pérqindja e mbuluar)

Pérshkrimi fizik i njollave t& naftés (drejtimi dhe forma p.sh. e vazhdueshme, ng
copa ose né vargje t& gjaté)

Ngjyra e njollés s& naftés

Kushtet e giellit (diell i shndritshém, vranésira etj.), rénia e drités dhe dukshméria
(n& kilometra) né momentin ¢ vézhgimit

Gjendja detare

10. Drejtimi dhe shpejtésia e erés sipérfaqésore
11. Drejtimi dhe shpejtésia e rrymés

5.1.3 Identifikimi i vézhguesit(ve)

N RGN

A

Emri i vézhguesit

Organizata me t& cilén vézhguesi &shté i lidhur (nése ka)

Statusi i vézhguesit brenda organizatés

Vézhgimi i kryer nga avioni (anija) (bregu), ose ndryshe

Emri ose identiteti i anijes ose avionit, nga i cili shté kryer vézhgimi
Vendndodhja specifike e anijes, avionit, vendit né breg ose né ndonjé ményré
tjetér nga i cili &shté& kryer vézhgimi

Veprimtaria ¢ kryer nga vézhguesi kur &shté kryer vézhgimi, p.sh.: patrullg,
lundrim, fluturim (gjaté rrugés nga ... né ...), etj.

5.1.4 Ményra e vézhgimit dhe dokumentimi

G . G D

Vizuale

Fotografi konvencionale

Regjistrime me sensoré né distancé dhe/ose fotografi me sensoré né distancé
Mostrat ¢ marra nga njolla e naftés né det

Cdo formé tjetér vézhgimi (specifikoni)

Shénim: Njé fotografi e shkarkimit preferohet t& jeté me ngjyra. Rezultatet mé t8 mira
mund t& merren me tre fotografité e méposhtme:

1.

2

3.

detaje t& njollés s& naftés né det t& marra pothuajse vertikalisht poshté nga njé
lart&si prej mé pak se 300 metra me diellin pas fotografit;

njé pamje e pérgjithshme e anijes dhe “e njollés s& naftés né det” q& specifikon njé
substancé qé buron nga anija e caktuar; dhe

detajet e anijes pér géllime identifikimi.

5.1.5 Informacione t& tjera nése mund t& vendoset kontakt radio

1.

Kapiteni i informuar pér ndotjen
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5.2

5.2.1

5.2.2

523

524

5.2.5

AR

Shpjegimi i kapitenit

Porti i fundit i thirrjes s& anijes

Porti tjetér i thirrjes sé anijes

Emri i kapitenit dhe pronarit t& anijes
Shenja e thirrjes s& anijes

Hetimi né bord

Inspektimi i certifikatés (Certifikata ¢ Pérshtatshmérisé n& Cisterna Kimike ose
Certifikata ¢ Substancave t& Léngshme t& Démshme)

AN R DN =

Emri i anijes

Numri ose shkronjat dalluese
Porti i regjistrit

Lloji i anijes

Data dhe vendi i 1&shimit
Data dhe vendi i miratimit

Inspektimi i Manualit P dhe A

1.
2.

3.
4.

Lista e substancave t& Shtojcés II & anija lejohet t& mbajé

Kufizimet né lidhje me rezervuarét né t& cilét mund t& transportohen kéto
substanca

Anije e pajisur me njé sistem efikas zhveshjeje

Sasité e mbetjeve t& pércaktuara né survejim

Inspektimi i Librit t& Regjistrimit t& Ngarkesés

Faget e mjaftueshme t& Librit t& Regjistrimit t& Ngarkesave duhet t& kopjohen pér t&
mbuluar njé cikél t& ploté ngarkimi/shkarkimi/balastimi dhe pastrimi t& rezervuarit t&
anijes. Duhet t& merret gjithashtu njé kopje e diagramit t& rezervuarit.

Inspektimi i regjistrit

D =

Porti i fundit, data e nisjes, thellésia e lundrimit para dhe pas;

Porti aktual, data e mbérritjes, thellsia e lundrimit para dhe pas;

Pozicioni i anijes né ose afér koh&s kur u raportua incidenti;

Kontrollimi n& vend nése kohét e regjistruara né Librin e Regjistrimit t&
Ngarkesés né lidhje me shkarkimet korrespondojné me distancén e mjaftueshme
nga toka mé e afért, shpejtésing e kérkuar t8 anijes dhe me thellési t& mjaftueshme
uji.

Inspektimi i dokumentacionit tjetér né bord

Dokumentacion tjetér i pérshtatshém pér prova (nése &shté e nevojshme t& b&hen
kopje) & tilla si:

1.

dokumentet e ngarkesave t& ngarkesave t& transportuara aktualisht ose s& fundmi,
s& bashku me informacionin pérkatés mbi temperaturén e kérkuar t& shkarkimit,
viskozitetin dhe/ose pikén e shkrirjes;

regjistrimet ¢ temperaturés sé substancave gjaté shkarkimit;




image31.jpg
5.2.6

5.2.7

g

Nk

20

10.
11.
12.

13.
14.

15

53

53.1

53.2

3. & dhénat e pajisjeve monitoruese nése ka té tilla.
Inspektimi i anijes

Pajisjet e anijes né pérputhje me Manualin P dhe A;

Mostrat e marra; vendndodhja né bord,

Burimet e rrjedhjeve t& konsiderueshme;

Mbetjet e ngarkesave né sipérfagen e balastit t& pastér t& veguar ose t& dedikuar;
Gjendja e ujrave t& ndotura (bilgeve) t& sallés s& pompés;

Gjendja e sistemit t& monitorimit;

Pérmbajtja e rezervuarit (llogaritni sasiné e ujit dhe mbetjet).

SR BN =

Deklaratat e personave té interesuar

Nése Libri i Regjistrimit t& Ngarkesave nuk &shté plotésuar si¢ duhet, informacioni
pér pyetjet e méposhtme mund t& jeté me vend:

A ka pasur njé shkarkim (aksidental apo t& qéllimsh&m) n& kohén e treguar né raportin
e incidentit?

Cilét rezervuaré do t8 ngarkohen né port?

Cilét rezervuaré kishin nevojé pér pastrim né det? A ishin laré paraprakisht
rezervuarét?

Kur dhe ku jang pastruar k&ta?

Mbetjet e cilave substanca u pérfshing?

Cfaré u b& me mbetjet ¢ rezervuaréve?

A u shkarkua né& det rezervuari i mbetjeve, ose rezervuari i ngarkesave q& pérdorej si
rezervuar i mbetjeve?

Kur dhe ku &shté kryer shkarkimi?

Cila &shté pérmbajtja e rezervuarit t& mbetjeve ose rezervuarit t& ngarkesave qé
pérdoret si rezervuar mbetjesh?

Cilét rezervuaré pérmbanin balastet e ndotura gjaté lundrimit me balaste (nése anija
arrinte me balaste)?

Cilét rezervuaré p&rmbanin balaste t& pastéra gjaté lundrimit me balaste (nése anija
arrinte me balaste)?

Detajet e lundrimit aktual t& anijes (portet e m&parshme, portet ¢ ardhshme, udhé&timi)

Véshtirésité e pérjetuara me shkarkimin né objektet e pritjes né breg

Véshtirésité e pérjetuara me operacionet efikase t& zhveshjes

. Cilét rezervuaré jané t& pastér ose t& pisét né momentin ¢ mbérritjes?
16.
17.
18.
19.
20.

Riparimet e kryera ose t& parashikuara né rezervuarét ¢ ngarkesave
Informacione t& ndryshme

Komentet né lidhje me gjendjen e pajisjeve t& anijes

Komentet né lidhje me raportin ¢ ndotjes

Komente t& tjera.

Hetimi né breg

Analizat ¢ mostrave

Specifikoni metodén dhe rezultatet e analizave t& mostrave

Informacione t8 métejshme
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53.3

5.4

5.5

Informacionet shtesé mbi anijen, t& marra nga stafi i terminalit, kontraktorét e
pastrimit t& rezervuaréve ose objektet e pritjes né breg mund t& jené t& réndésishme.
Shénim: Cdo informacion nén ké&té titull, nése &shté ¢ mundur, duhet t& vértetohet me
dokumentacion t& tillé si deklarata t& nénshkruara, fatura, déftesa, etj.

Informacion nga terminali i mé&parsh&ém i portit t& shkarkimit

1.

2.
3.
4.

Konfirmimi & anija &shté shkarkuar, pastruar ose paralaré né pérputhje me
manualin e saj P dhe A

Natyra e véshtirésive nése ka

Kufizimet nga autoritetet sipas t& cilave anija lejohej t& lundronte

Kufizimet né& lidhje me kompanité e grumbullimit t& mbetjeve vajore né breg

Informacioni qé nuk mbulohet nga sa mé sipér

Pérfundim

Pé&rmbledhja e pérfundimeve t& hetuesit;

Tregimi i dispozitave t& zbatueshme t& Shtojeés II t& MARPOL 73/78, t& cilat anija
dyshohet se i ka shkelur;

A garantuan rezultatet ¢ hetimit paraqitjen e njé raporti t& mangésive?
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SHTOJCA 3

FAKTET E KONSIDERUARA ST “ARSYE Tii QARTA”

1. Autoritetet do t8 konsiderojné si “arsye t& qarta” ndér té tjera sa vijon:

1.
2

10.
11.

12.

13.

14.

15.

16.

17.

njé raport ose njoftim nga njé autoritet tjetér,

gjaté ekzaminimit t& certifikatave dhe dokumenteve t8 pérmendura né Shtojcén 11 t&
Memorandumit, jané zbuluar pasaktési ose dokumentet nuk jané mbajtur, pérditésuar
ose jané mbajtur né ményré té rreme;

indikacionet q& anétarét pérkatés t& ekuipazhit nuk jané né gjendje t& komunikojné si¢
duhet me njéri-tjetrin, ose me persona t& tjeré né bord, ose se anija nuk &shté né
gjendje t& komunikojé me autoritetet me bazé né breg as né njé gjuhs t& pérbashkét t&
kétyre autoriteteve;

certifikata &shté marré me mashtrim ose mbajtési i certifikatés nuk &shté personi t&
cilit 1 &shté l&shuar fillimisht ajo certifikaté;

anija ka njé kapiten, oficer ose detar q& mban njé certifikaté t& l&shuar nga njé vend qé
nuk e ka ratifikuar Konventén Ndérkombétare pér Standardet ¢ Trajnimit, Certifikimit
dhe Vrojtimit pér Detarét;

déshmi t& mallrave dhe operacioneve t& tjera q& nuk kryhen né ményré t& sigurté ose
né pérputhje me udhézimet ¢ Organizatés Ndérkombétare Detare;

déshtimi 1 kapitenit t& njé cisterne nafte pér t& prodhuar t& dhénat e sistemit t&
monitorimit dhe kontrollit t& shkarkimit t& naftés pér lundrimin e fundit t& gakéllit;
mungesa ¢ njé liste t& pérditésuar t& personelit, ose anétarét ¢ ekuipazhit nuk jang t&
vetddijshém pér detyrat e tyre né rast zjarri ose urdhri pér té braktisur anijen;

emetimi i sinjalizimeve t& rreme t& shqetésimit g8 nuk ndigen nga procedurat e duhura
t& anulimit;

mungesa ¢ pajisjeve ose aranzhimeve kryesore t& kérkuara nga konventat;

déshmi nga pérshtypjet dhe vézhgimet e pérgjithshme t& Zyrtari t& Kontrollit
Shtetéror Portual se ekzistojné pérkeqésime serioze t& trupit, ose strukturore, ose
mangési g8 mund t& véné né rrezik integritetin strukturor, t& papérshkueshém nga uji
ose ndaj motit t& anijes;

informacion ose déshmi se kapiteni ose ekuipazhi nuk jané& t& familjarizuar me
operacionet thelb&sore t& anijes né lidhje me siguriné e anijeve ose parandalimin e
ndotjes, ose q& operacione t& tilla nuk jané kryer;

mungesa ¢ njé tabele t& aranzhimeve t8 punés sé anijeve ose t& shénimeve t& oréve t&
punés ose pushimit t& detaréve;

anija ka ndryshuar flamurin me gé8llim t& shmangies s& pérputhshmérisé me
Konventén e Punés Detare ose anija mban flamurin e njé shteti q& nuk ¢ ka ratifikuar
Konventa ¢ Punés Detare, 2006,

ka nj& ankesé & pretendon se kushtet specifike t& punés dhe t8 jetesés né anije nuk
jané n& pérputhje me kérkesat ¢ Konventés s& Punés Detare, 2006 ose pas hetimit t&
njé ankese né breg;

kushtet e punds dhe té& jetesés né anije nuk jan& n& pérputhje me kérkesat ¢ Konventss
s& Punés Detare;

njé raport ose ankesé nga kapiteni, njé anétar i ekuipazhit, ose ¢do person ose
organizaté me njé interes legjitim né funksionimin e sigurt t& kushteve t& jetesés dhe
t& punés né bordin e anijes ose parandalimin e ndotjes, pérveg rasteve kur Autoriteti
né fjalé e gjykon raportin ose ankesén t& jeté haptazi i pabazuar. Identiteti i personit q&
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paraqget raportin ose ankesén nuk duhet t'i zbulohet kapitenit ose pronarit t& anijes né
fjalé.

2. M& poshté jang shembuj t& arsyeve t& qarta pér kontrollin e anijeve né aspektet e sigurisé:

el ol s

o

Certifikata Ndérkombétare e Sigurisé s& Anijeve nuk &shté e vlefshme ose ka skaduar.
Anija &shté né njé nivel sigurie mé t& ulét se porti.

Stérvitjet né lidhje me siguring e anijes nuk jané kryer.

Regjistrimet pér 10 ndérfaqet e fundit anije/port ose anije/anije jané t& paplotésuara.
Déshmi ose vézhgim & andtarét kryesoré t& personelit t& anijes nuk mund t&
komunikojn& me njéri-tjetrin.

Déshmi nga vézhgimet se ekzistojné mangési serioze né pajisjet dhe aparaturat e
sigurisé.

Informacion nga palét e treta, t& tilla si njé raport ose njé ankesé né lidhje me
informacionin e lidhur me siguring.

Anija mban njé Certifikaté Ndérkombétare t& Sigurisé s& Anijes (ISSC) t&
mévonshme, t& l&shuar né ményré t& njépasnjéshme dhe sipas gjykimit profesional t&
inspektorit, njé nga qéllimet e anijes ose kompanisé né kérkimin e njé certifikate t&
tillé &shté t& shmangé pajtueshméring e ploté me Konventén Ndérkombétare pér
Siguring e Jetés né Det SOLAS 74 Kapitulli XI -2 dhe Pjesa A e Kodit Ndérkombétar
t& Sigurisé s& Anijeve dhe Porteve (Kodi ISPS), pértej periudhés s& certifikatés
fillestare t& ndérmjetme. Kodi Ndérkombétar i Sigurisé s& Anijeve dhe Porteve, Pjesa
A specifikon rrethanat kur mund t& 1&shohet nj& Certifikaté ¢ Pérkohshme.

Nése pércaktohen arsye t& qarta si¢ pérshkruhet mé lart, Zyrtari i Kontrollit Shtetéror
Portual do t& informojé menjéheré autoritetin kompetent t& sigurisé (pérveg rastit kur
Zyrtari 1 Kontrollit Shtetéror Portual &shté gjithashtu njé Zyrtar i autorizuar sipas
rregullave pér siguring). Autoriteti kompetent i sigurisé do t& vendosé mé pas se cilat
masa t& tjera kontrolli jan& t& nevojshme duke marré parasysh nivelin e sigurisé né
pérputhje me Rregulloren 9 t& Konventss Ndérkombétare pér Siguring e Jetés né Det 74,
Kapitulli XI.
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SHTOJCA 4

SISTEMI I INFORMACIONIT MBI INSPEKTIMET

Pér t& ndihmuar Autoritetet né pérzgjedhjen ¢ anijeve me flamur t& huaj g& do t&
inspektohen né portet e tyre, &shté e nevojshme t& kené né dispozicion t& Autoriteteve
informacione t& pérditésuara pér inspektimin e njé anijeje t& caktuar me flamur t& huaj né
njé nga portet e tjera rajonale.

Pér két& qéllim, Autoritetet marrin pérsipér t'i garantojné njé Qendre Informacioni,
mundgsisht me ané t8 transmetimit kompjuterik t& t& dhénave, informacion pér anijet e
inspektuara né portet kombétare, duke u bazuar né informacionin e pércaktuar né shtojcén
5 t& Memorandumit. Futja e informacionit né dosjet ¢ inspektimit preferohet t& realizohet
me ané t& hyrjeve t& drejtpérdrejta dhe t& kompjuterizuara né baza ditore.

Pér qéllimin ¢ shkémbimit t& informacionit t& shpejté, sistemi i informacionit do t&
pérfshijé njé lehtési komunikimi q& lejon njé shkémbim t& drejtpérdrejts, t&
kompjuterizuar t& mesazheve ndérmjet autoriteteve individuale, duke pérfshiré njoftimet e
pérmendura né Seksionin 3.8 t& Memorandumit dhe shkémbimin e informacionit mbi
shkeljet operacionale si¢ pérmendet n& Seksionin 5 t& Memorandumit.

Informacioni si n& paragrafin 2 dhe 3 mé& sipér do t& trajtohet né njé formé t&
standardizuar dhe né& pérputhje me standardizimin e pércaktuar né udhézuesin pér
pérdoruesit e sistemit t& informacionit t& ofruar nga Qendra e Informacionit.

Qendra e Informacionit do t& organizojé p&érpunimin ¢ informacionit si né paragrafin 2 mé
sipér né ményré q& t& garantojé g8 t& dhénat e inspektimit t& jené lehtésisht t&
aksesueshme si pér qéllime konsultimi ashtu edhe pér pérditésime né& pérputhje me
procedurat e pércaktuara né udhézuesin pér pérdoruesit e sistemit t& informacionit t&
ofruar nga Qendra ¢ Informacionit.

Informacioni pér qéllime administrative, si¢ &shté informacioni statistikor, do t&
garantohet nga Sekretariati nén drejtimin ¢ Komitetit. Kjo do t& bazohet né t& dhénat e
ofruara nga Qendra ¢ Informacionit.

Sistemi i informacionit i treguar né paragrafét e mésipérm do t& zbatohet pér sa kohé& qé
Memorandumi t& hyjé né fuqi.

Studimet pér monitorimin dhe, kur &sht& e nevojshme, pér pérmirsimin e cilésisé s&
sistemit do t& kryhen né ményré t& vazhdueshme.

Sa heré q& konstatohen manggsi qé ¢ojné né vonesén ose ndalimin e njé anijeje, Autoriteti
Shtetéror Portual do t'i dérgojé njé kopje t& raportit, si¢ referohet né Shtojcén 5 t&
Memorandumit, administratés s& flamurit pérkatés.
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SHTOJCA 5

PUBLIKIMI I INFORMACIONIT PER KONTROLLIN SHTETEROR PORTUAL

Pérmbajtja
» Raporti i Inspektimit né pérputhje me Memorandumin e Mirékuptimit Mesdhetar

pér Kontrollin Shtetéror Portual né “Formé A/1” dhe “Formén A/2”

» Raporti i Inspektimit né pérputhje me Memorandumin e Mirékuptimit Mesdhetar
pér Kontrollin Shtetéror Portual “Forma B”

» NJOFTIMI PiiR NDALIMIN E ANIJES

» NJOFTIMI PiiR LIRIMIN E ANIJES

> SHKEMBIMI I MESAZHEVE NGA AUTORITETET E RAJONIT SIPAS
SEKSIONIT 3.8 TE MEMORANDUMIT
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RAPORTI I INSPEKTIMIT Ni PERPUTHJE ME

ﬂ\ MEMORANDUMIN MESDHETAR T§ MIREKUPTIMIT PER

~EDITERRANE KONTROLLIN SHTETEROR PORTUAL! FORMULARI A/1
(Autoriteti Raportues) Kopje pér: - Kapitetin ¢ Anijes

(Emri i Zyrés) - Zyrén Qendrore

(Adresa) - Zyrtarin e Kontrollit Shtetéror Portual

(Telefoni) nése anija éshté e ndaluar, kopje pér:

(Faksi) - Shtetin ¢ Flamurit

(E-maili) - Organizatén e njohur, nése &shté e zbatueshme

TE DHENAT E ANIJES®

2. Flamuri i anijes ...
4. Shenja e thirrjes .
6. Tonazhi bruto

1. Emri i anijes...

3. Lloji i anijes ...

5. Numri Organizatés Ndérkombétare Detare...

7. Data e vendosjes sé anijes/fillimi i konvertimit té madh........

8. Pesha e vdekur (kur &shté e zbatueshme...........c.covevevnernnns

9. Té dhénat e plota té kompanisé (identike me t& dhénat si ng Certifikatén ¢ Menaxhimit t& Siguris&)***
Numri i Kompanisé sé¢ Organizatés Ndérkombétare Detare: ...
Adresa:

Emri: ...
Vendi:...

10. Emri dhe nénshkrimi i kapitenit té anijes pér té vértetuar se informacioni né pikén 9 éshté i sakté:
BN coossspomsnmrons i s BREMNAY bvcqissmmmmns oo o e e

Ti DHENAT E INSPEKTIMIT?

11. Data e hipjes né anije: ..........c.cooooeiiiiiiiniiin 12. Vendi i InspekUnit; oo mmimmmuimmsinimms s
13. Nése anija ndalohet: Data e léshimit té njoftimit t& ndalimit: ................. Kohézgjatja e ndalimit:............................ Dité(t)

14. Data e raportimit: ...

15. Lloji i inspektimit: [ Inspektimi fillestar [ Inspektimi mé i detajuar [ Inspektimi i zgjeruar OecLey: .

! Ky raport inspektimi shté léshuar vetém pér qéllimin e informimit t& kapitenit dhe shteteve t& tjera portuale se &shté kryer njé inspektim nga shteti portual, 1
pérmendur né titull. Ky raport inspektimi nuk mund t& interpretohet si njé certifikaté e vlefshme pér detin qé tejkalon certifikatat q& anija duhet té mbajé.

2 Anije jo-ISM: Kapiteni duhet té furnizojé dhe nénshkruajé pikén 10 pér t& dhénat e plota e té sakta t& kompanisé.

3 Kapiteni, pronarét e anijeve dhe/ose operatorét késhillohen qé informacioni i detajuar mbi inspektimin mund t1 nénshtrohet publikimit (www.medmou.org)

4 Fushata e Pérgendruar e Inspektimit, njé pyetésor i veganté duhet t& depozitohet dhe t& regjistrohet né THETIS-Med.
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16. Vazhdimi i inspektimit(eve):

Nr.

1

Data e vizités

17. Kontrollet operacionale (nése ka):

O Tjeter .
anijes

O stervitja e zjarrit
[ Kontrolli i démtimit

18. Certifikatat pérkatése

[ Pajisjet ¢ komunikimit

[ Pajisje pér filtrimin ¢ vajrave

[ Gjeneratori i urgjencés

Ekipi i Inspektimit

[ Pompé zjarri emergjente
[ Pompé zjarri emergjente

FORMULARI A2

Vézhgimet

[ Stérvitja pér braktisjen e

Z
B

a. Titulli

b. Autoriteti Léshues

¢. Data e léshimit

d. Data e skadencés

Informacion mbi Anketén e fundit t€ ndérmjetme, periodike ose vjetore

Data e sondazhit

Autoriteti Gjeografik

Vendi

0|~ | Oy [~ W [ro | —
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FORMULARI A/3

19. Shogéria (shoqérité) e klasifikimit pérgjegjése pér léshimin e certifikatave té klasit:

................................................................................. LEShuar mss s Kaskaduarme: .o
................................................................................. Léshuar mé: ......cccoovevevrvennenennenns Ka skaduar m&: ......oooovvevvenrneenenne

21. Veprimet e ndérmarra pér inspektimin e anijes:

O U njoftua administrata e shtetit t& flamurit O Inspektimi &shté kryer né det O Vézhgimet pér inspektimin

O Shteti Bregdetar &shté informuar O Inspektimi i pezulluar [ Bazat e sistemeve kundér ndotjes

O Organizata e Njohur u informua O Pushuar pér arsye té sistemeve kundér ndotjes O Hetimi MARPOL i shkeljes s& dispozités s& shkarkimit

O Porti tjetér i thirrjes u informua O Anija débohet pér siguri O Shtetit t& flamurit i &shté kérkuar njé plan veprimi brenda afatit
O Organizata Ndérkombétare e Punés u informoa O Anija e débuar pér arsye té tjera O Faktori Mbéshtetés

0O Pérfagésuesi i sindikatés u informua O Autoriteti Heter 1 IFOTTIIAT ..o s e e et e e e s e e
22. Mangésité Ojo O po (shiko Formularin B) bashkélidhur

23. Dokumentacion mbéshtetés Ojo O po (shiko Shtojcén)

TE DHENAT E SHTETIT PORTUAL

e S S -

Adresa:

Telefoni:

Faksi:

E-mail: .

Emri(at) . Sa—— .

(Oficerét e Kontrollit Shtetéror Portual t& autoritetit raportues t& autorizuar sipas rregullave)

NENShKEIMI(E).....cviiviiiiieiiiiiiiis e et ees teeeebeeee st e e saese s e b nnenens

Ky raport duhet t& ruhet né bord pér njé periudhé prej t& paktén dy vietésh dhe duhet t& jeté gjithmong i disponueshém pér konsultim nga Oficerét
¢ Kontrollit Shtetéror Portual.
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RAPORTI I INSPEKTIMIT Ni PERPUTHJE ME
MEMORANDUMIN MESDHETAR TE MIREKUPTIMIT PER

KONTROLLIN SHTETEROR PORTUAL FORMULARI B
(Autoriteti Raportues) Kopje pér: - Kapitetin ¢ Anijes
(Adresa) - Zyrén Qendrore
(Telefoni) - Zyrtarin ¢ Kontrollit Shietéror Portual
(Faksi) nése anija éshté e ndaluar, kopje pér:
(E-mail) - Shtetin e Flamurit

- Organizatén ¢ njohur, nésc éshté ¢ zbatueshme
3. Data e Raportit 4. Vendi i Inspektimit.

1. Emri i anijes.. 2. Nr. Organizatés Ndérkombétare Detar

Manggésité e konstatuara dhe veprimet vijuese***

Kodi Artikulli me defekt ~ Natyra e defektit * Konventa ref.* Baza pér (AT) Dataeduhur Komente shtesé RO AD ISM
ndalim

Ooooogo
Ooooooo
OoOooooo

Emri(at)

(Oficerét e Kontrollit Shtetéror Portual té autoritetit raportues té autorizuar sipas rregullave)

Nénshkrimi(et)

apitenst, pronarét ¢ anijeve dhefose operatorét késhillohen e informacioni i detajuar mbi inspektimin mund t¢ jeté objekt publikimi (www.medmou.org)

' Ky inspektim nuk ishte njé studim i ploté dhe mangésité ¢ listuara mund t& mos jené shterucse. Né rast ndalimi, rekomandohet qé té kryhet njé studim i ploté dhe t&
Korrigiohen (& gjitha mangésité p & béhel njé kerkesé pér ri-inspekiim

2T plotésohet né rast ndalimi. (pér anijet jo-konvencionale <500 GT vetém si referencé)
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ﬂ\ KONTROLLI SHTETEROR PORTUAL
MR o NJOFTIMI PEER NDALIMIN E ANLJES *

Shteti i Flamurit / Konsullata

Shogqéria e klasifikimit/organizata e njohur
Nr. Faksi

E-mail

Numri i fageve, pérfshiré kété

I nderuar zotéri, zonjé,
[Emri i anijes, flamuri, Nr. Organizatés Ndérkombétare té Punés] - Ndalimi i anijes

Autoriteti Detar ........ccoovevniiiiiice ka kryer mé [daté] njé inspektim t& anijes s&
mésipérme né [Portin, Vendin].

Anija ndalohet né orén ¢ [kohés s€ ndalimit] pér shkak t& mangésive t& méposhtme t& ndalimit:

Bashkélidhur ju lutemi gjeni njé kopje t& Raportit t& formularéve t& inspektimit A & B.
Pér pyetje t& métejshme, ju lutemi kontaktoni: [Emri dhe detajet e kontaktit]

I juaji me besnikéri,

* Sipas Qarkores 1011 t& Organizatés Ndérkombétare Detare (IMO) - Késhillit té Kujdestarisé Detare (MSC) dhe
Qarkores 383 t& Komitetit pér Mbrojtjen e Mjedisit Detar (MEPC)

VENDOSNI NE PIESEN E PASME TE KETIJ DOKUMENTI PROCEDUREN E DEDIKUAR TE ANKESES
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KONTROLLI SHTETEROR PORTUAL
NJOFTIMI PiiR LIRIMIN E ANLJES *

Shteti i Flamurit / Konsullata

Shoqéria e klasifikimit/organizata e njohur
Nr. Faksi

E-mail

Numri i faqeve, pérfshiré kété

I nderuar zotéri, zonjé,

[Emri i anijes, flamuri, Nr. Organizatés Ndérkombétare t€ Punés] — Lirimi i anijes

Autoriteti Detar ...

ka kryer mé [daté] njé inspektim t& anijes s&
mésipérme né [Portin, Vendi

n].

Anija lirohet né orén e [kohés sé lirimit].

[Futja e tekstit té liré, nése ka].

Bashkélidhur ju lutemi gjeni njé kopje t& Raportit t& formularéve t& inspektimit A & B.

1 juaji me besnikéri,

* Sipas Qarkores 1011 t& Organizatés Ndérkombétare Detare (IMO) - Késhillit té Kujdestarisé Detare (MSC) dhe
Qarkores 383 t& Komitetit pér Mbrojtjen e Mjedisit Detar (MEPC)
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1.

SHKEMBIMI I MESAZHEVE NGAAUTORITETET E RAJONIT SIPAS SEKSIONIT
3.8 TE MEMORANDUMIT

N& rastin ¢ mangésive t& pa korrigjuara plotésisht ose vetém t& riparuara pérkohésisht, njé
mesazh do t'i dérgohet Autoritetit kompetent t& Shtetit rajonal ku ndodhet porti i ardhshém i
thirrjes s& anijes.

Shk&mbimi i mesazheve, si né paragrafin 1 mé sipér, do t& hyjé né fuqi népérmjet pérdorimit
t& lehtésive t& komunikimit t& inkorporuara né sistemin e informacionit si¢ pérshkruhet ng
aneksin 4 dhe/ose me faks n& formularin e pérfshiré né shtojcén e késaj shtojce.

Cdo mesazh si n& paragrafin 1 mé sipér, duhet t& pérmbajé informacionin ¢ méposhtém:

data:

nga (vendi):

porti:

pér (vendin): portin:

njé deklaraté q& lexon mangésité q& duhen korrigjuar:
emri i anijes:

Numri i identifikimit t& Organizatés Ndérkombétare Detare (nése disponohet):
1loji i anijes:

flamuri i anijes:

shenja e thirrjes:

tonazhi bruto:

viti 1 ndértimit:

autoriteti 18shues i certifikatave pérkatése:

data e nisjes:

vendi dhe koha e parashikuar e mbérritjes:

natyra ¢ manggsive:

veprimet ¢ marra:

veprim i sugjeruar né portin tjetér t& thirrjes:

emri dhe numri i faksit t& dérguesit.

VVVVVVVVVVVVVVYVYVVVYY
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SHTOJCA 6

KRITERET CILESORE PER ZBATIMIN E MEMORANDUMIT MESDHETAR Ti
MIREKUPTIMIT

Autoriteti Detar i njé Shteti mund t& aderojé si anétar i ploté, me kusht q& t& plotésohen t&
gjitha kriteret ¢ m&poshtme cilésore:

Ky Autoritet Detar do t& pajtohet né ményré eksplicite pér angazhimet sipas Memorandumit
me géllim q& t& kontribuojé né pérpjekjen e pérbashkét pér t& eliminuar funksionimin e
anijeve nén standarde;

Ky Autoritet Detar do t& marré t& gjitha masat e nevojshme pér t& inkurajuar ratifikimin e t&
gjitha instrumenteve pérkatése né fuqi. Kontrolli Shtetéror Portual nuk do t& zbatohet nga ky
Autoritet Detar pér ato instrumente q& nuk i ka ratifikuar ende.

Autoritete t& tilla detare do t& kené kapacitete t& mjaftueshme, logjistike dhe thelb&sore, pér
t& zbatuar né ményré t8 pérshtatshme pérputhjen me standardet ndérkombétare detare né
lidhje me siguring detare, parandalimin ¢ ndotjes dhe kushtet ¢ jetesés dhe t& punés né bord
né lidhje me anijet q& kang t& drejté t& mbajné flamurin e saj, q& pérfshin punésimin e
inspektoréve t& kualifikuar si¢ duhet q& veprojné nén pérgjegjésiné e Administratss sé tij, pér
t'u demonstruar sipas bindjes s& Komitetit t& pérmendur né paragrafin 6.1 t& Memorandumit;

Ky Autoritet Detar do t& keté kapacitete t& mjaftueshme, logjistike dhe thelb&sore, pér t&
pérmbushur plotésisht t& gjitha dispozitat dhe aktivitetet ¢ specifikuara né Memorandum, né
ményré qé t& rrisé angazhimin e tij, i cili do t& pérfshijé punésimin e oficeréve t& kontrollit t&
shtetit portual t& kualifikuar g8 veprojné nén pérgjegjésiné ¢ administrimit t& tij, pér t'u
demonstruar sipas bindjes s8 Komitetit t& pérmendur né paragrafin 6.1 t& Memorandumit;

Ky Autoritet Detar, né datén efektive t& anétarésimit, do t& krijojé njé lidhje online me
sistemin e informacionit t& pérmendur né Shtojcén 4;

Ky Autoritet Detar do t8 nénshkruajé njé marréveshje financiare pér pagesén e pjesés sé tij né
koston operative t& Memorandumit dhe né datén e hyrjes né fuqi t& tij do t& paguajé
kontributin e tij financiar né buxhet si¢ &shté miratuar nga Komiteti i pérmendur né
paragrafin 6.1 t& Memorandumit.
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SHTOJCA 7

KRITERET DHE KERKESAT E ZYRTARIT T KONTROLLIT SHTETEROR

PORTUAL
Pérmbajtja
Seksioni 1 Kriteret e Kualifikimit pér Oficerét e Kontrollit Shtetéror Portual
Seksioni 2 Kérkesat pér Kartén e Identitetit pér Inspektorét ¢ Kontrollit Shtetéror

Portual
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Seksioni 1 KRITERET E KUALIFIKIMIT PER OFICERET E KONTROLLIT
SHTETEROR PORTUAL

1. Ng& zbatim t& dispozitave t& paragrafit 3.5 t& Memorandumit, Zyrtari i Kontrollit Shtetéror
Portual duhet t& jeté i kualifikuar dhe i autorizuar si¢ duhet nga Autoriteti pér t& kryer
inspektime t& kontrollit shtetéror portual [pa cenuar dispozitat kombétare].

2. Njé Oficer i Kontrollit Shtetéror Portual i kualifikuar si¢ duhet duhet t& keté kryer t& paktén
njé vit shérbim si kontrollor i shtetit flamur q& merret me sondazhet dhe certifikimin né
pérputhje me instrumentet pérkatése dhe t& keté n& zotérim:

1. njé certifikaté kompetence si kapiten, q& i mundéson atij personi t& marré komandén e
njé anijeje me tonazh bruto 1,600 toné ose mé& shumé (shih STCW, Rregullorja 11/2),
ose

2. njé certifikaté kompetence si kryeinxhinier, q&¢ i mundéson atij personi t& marré até
detyré né bordin e njé anijeje, termocentrali kryesor i s& cilés ka nj& fuqi t& barabarté
ose mé t& larté se 3,000 kW (shih STCW, Rregullorja II/2), ose

3. ka dhé&né njé provim t& njohur nga Autoriteti si arkitekt detar, inxhinier mekanik ose
inxhinier né fushén e detit dhe ka punuar né até cilési pér t& paktén 5 vjet.

Oficerét e Kontrollit Shtetéror Portual t& pérmendur né paragrafét 2.1 dhe 2.2 mé sipér
duhet t& kené shérbyer pér njé periudhé jo mé& pak se pesé vjet né det si oficeré né
departamentin ¢ kuvertés ose motorit.

3. Pérndryshe, njé Oficer i Kontrollit Shtetéror Portual konsiderohet i kualifikuar si¢ duhet nése
ai person:
1. zotéron nj& diplomé& universitare pérkatése ose njé trajnim t& barasvlershém, dhe
2. &shté trajnuar dhe kualifikuar n& njé shkollé pér inspektorét e sigurisé s& anijeve, dhe
3. ka shérbyer t& paktén 2 vjet si kontrollor i shtetit flamur q& merret me sondazhet dhe
certifikimin né pérputhje me instrumentet pérkatése.

4. Njé Oficer i Kontrollit Shtetéror Portual i kualifikuar si¢ duhet duhet t& jeté né gjendje t&
komunikojé me gojé dhe me shkrim me detarét né gjuhén & flitet mé shpesh né det.

5. Njé oficer i kontrollit t& shtetit portual i kualifikuar si¢ duhet duhet t& keté njohurité ¢ duhura
pér dispozitat e instrumenteve pérkatése dhe pér procedurat pérkatése pér kontrollin e shtetit
portual.

6. Njé oficer i kontrollit shtetéror portual i kualifikuar si¢ duhet duhet t& mbetet i pérditésuar me
instrumentet dhe rregulloret e reja pérkatése. Né& arritjen ¢ q&llimit t& ruajtjes dhe pérditésimit
t& njohurive t& tyre, Zyrtari i Kontrollit Shtetéror Portual duhet t& pérdoré Programet e
Mésimit né Distancé né dispozicion.

7. Oficerét e Kontrollit Shtetéror Portual q& nuk plotésojné kriteret ¢ mésipérme pranohen
gjithashtu nése jan& punésuar pér kontrollin shtetéror portual nga Autoritetet para datés 1
korrik 1996.
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Seksioni 2 KERKESAT PiER KARTEN E IDENTITETIT PER INSPEKTORET
E KONTROLLIT SHTETEROR PORTUAL

1. Karta e identitetit duhet t& pérmbajé t& paktén t& dhénat e méposhtme:

emrin dhe Autoritetin 18shues;

emrin e ploté t& mbajtésit t& kartés s& identitetit

fotografing e pérditésuar t& mbajtésit t& letérnjoftimit;

nénshkrimin e mbajtésit t& letérnjoftimit;

njé deklaraté qé pohon se mbajtési i kartés s& identitetit &shté i autorizuar t& kryejé
kontrolle n& pérputhje me legjislacionin kombétar.

B 1 8 =

2. Nése gjuha kryesore ¢ pérdorur né kartén e identitetit nuk &shté anglishtja, ajo duhet t&
pérfshijé njé pérkthim né até gjuhé.

3. Formati i kart&s s& identitetit lihet né gjykimin e autoriteteve kompetente.
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Seksioni 1

Seksioni 2

SHTOJCA 8
PROCEDURAT E ANKESAVE DHE SHQYRTIMIT

Procedura e ankimit

Neni 3.13 i Memorandumi i Mir&kuptimit Mesdhetar thoté se “pronari ose
operatori i njé anijeje do t& ket t& drejtén e ankimimit kundér njé vendimi
ndalimi né Autoritetin mé t& larté administrativ ose né Gjykatén e juridiksionit
kompetent, sipas ligjit né ¢do vend. Megjithaté, ankesa nuk shkakton pezullimin e
ndalimit.”

Pronarét ose operatorét késhillohen t& pérdorin procedurén e Autoritetit zyrtar
nése déshirojné t& apelojné njé urdhér ndalimi. Procedurat bazé t& apelimit né
shtetet anétare t& Memorandumit t& Mirékuptimit Mesdhetar jané renditur ng
dokumentin e quajtur: Procedurat ¢ apelimit né shtetet anétare t& Med MoU (sig
&shté publikuar né fagen ¢ internetit www.medmou.org).

Procedura e Rishikimit

N& rast se njé pronar ose operator refuzon t& pérdoré procedurén zyrtare té
apelimit t& Autoritetit, por ende déshiron t& ankohet pér njé vendim ndalimi, njé
ankesé e till¢ duhet t'i dérgohet shtetit t& flamurit ose organizatés s& njohur (nése
autorizohet t& veprojé pér shtetin e flamurit).

Shteti i flamurit ose organizata e njohur mund t'i kérkojé mé pas shtetit portual t&
rishqyrtojé vendimin e tij pér ndalimin e anijes.

N& raste t& tilla, shteti portual duhet t& hetojé vendimin dhe t& informojé shtetin e
flamurit ose organizatén e njohur pér rezultatin. Né&se shteti portual pranon té
rezervojé vendimin e tij, ai duhet gjithashtu t& informojé menaxherin e bazés & t&
dhénave t& Memorandumit t& Mirékuptimit Mesdhetar dhe Sekretariatin e
Memorandumit t& Mirékuptimit Mesdhetar.

Nése shteti i flamurit ose organizata ¢ njohur nuk pajtohen me rezultatin ¢ hetimit
si¢ u pérmend mé lart, njé kérkesé pér rishikim mund t'i dérgohet Sekretariatit t&
Memorandumit t& Mirékuptimit Mesdhetar brenda 90 ditéve, nga data e ndalimit.
Njé kérkesé e tills duhet t& shogérohet me t& gjitha informacionet & kang t& b&jné
me ndalimin  n& format elektronik  (dorézim me e-mail né&:
secretariat@medmou.org) dhe né gjuhén angleze.

Sekretariati do t8 ngrejé njé “Panel Shqyrtues: i pérbéré nga Sekretariati si
Koordinator dhe 3 Autoritetet ¢ Memorandumit t& Mirékuptimit Mesdhetar t&
kérkuara né bazé té& rotacionit alfabetik, duke pérjashtuar portin dhe shtetin e
flamurit. Sekretariati do t& informojé gjithashtu shtetin portual pér kérkesén e
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rishikimit dhe do t& ftojé shtetin portual t& paraqesé informacionin pérkatés né
format elektronik.

Paneli Shqyrtues do t& marré né konsideraté aspektet procedurale dhe teknike t&
inspektimit bazuar né informacionin ¢ dhéné nga shteti i flamurit dhe/ose
Organizata ¢ Njohur dhe shteti portual. Anétarét e Panelit Shqyrtues i kthejng
opinionet e tyre Sekretariatit. Nése kérkohet informacion shtess, Sekretariati do t&
organizojé qé ky informacion t'u jepet t& gjithé anétaréve t& Panelit Shqyrtues.
Detajet e korrespondencés ruhen si njé ¢éshtje e brendshme. Konstatimet e Panelit
Shqyrtues pérfaqésojné opinionin e shumicés.

Sekretariati do t& pérgatisé njé pérmbledhje t& opinioneve t& Panelit Shqyrtues dhe
do t& informojé shtetin e flamurit ose Organizatén ¢ Njohur, sipas rastit, kontrollin
shtetéror portual dhe Bordin késhillues t& Memorandumit t& Mirékuptimit.

Nése piképamja ¢ Panelit Shqyrtues mbéshtet ankesén e Shtetit t& flamurit ose t&
Organizatés s& Njohur, kontrollin shtetéror portual do t'i kérkohet t& rishqyrtojé
sérish vendimin e tij.

Konstatimet e Panelit Shqyrtues nuk jané t& detyrueshme, por mund t8 ofrojné
justifikim pér shtetin port q& t& ndryshojé t& dhénat e tij t& inspektimit t& futura
tashmé né& bazén e t& dhénave dhe t& informojé menaxherin ¢ bazés s& t& dhénave
dhe Sekretariatin né pérputhje me rrethanat. Sekretariati do t& informojé Shtetin e
flamurit ose Organizatén e Njohur, sipas rastit, pér veprimin (jo) t& ndérmarré nga
shteti portual.

Konstatimet e Panelit Shqyrtues nuk mund t& pérdoren si bazé pér t& kérkuar
kompensim financiar.
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. SHTOJCA 9
KRITERET E PERZGJEDHJES (FAKTORI I SYNUAR)

Llogaritja e Faktorit t& Synuar ndahet né dy pjesé:

1
2

Faktori Gjenerik, bazuar né elementé t& profilit t& anijeve.
Faktori Historik, bazuar né historikun ¢ inspektimit t& anijeve né Memorandumin e
Mir¢kuptimit Mesdhetar

Faktori Gjenerik

Faktori Gjenerik pér njé anije individuale llogaritet duke mbledhur s& bashku elementét

pérkatés t& profilit t& saj:

o Flamujt e synuar

e Llojin e anijes né shénjestér

e  Shoqérité klasifikuese jo anétare t& Shogqatés Ndérkombétare t& Shogqérive t&
Klasifikimit IACS

o Moshén ¢ anijeve

Faktori Gjenerik pérditésohet kur t& dhénat ¢ anijes ndryshojné ose statusi i flamurit t& saj
ekzistues ndryshon.

Faktori Historik

Faktori Historik zbatohet né Faktorin Gjenerik pér t& pasqyruar gjendjen aktuale t& anijes
s& konstatuar pas inspektimeve t& Kontrollit Shtetéror Portual.

Faktori Historik llogaritet duke zbatuar elementét ¢ méposhtém t8 Memorandumit t&
Mirékuptimit Mesdhetar pér ¢do inspektim t& kryer t& anijes:

Intervalin e inspektimit

Ndalimin

Numrin ¢ manggsive

Manggsité e pazgjidhura

Faktori i pérgjithshém i synuar llogaritet duke shtuar Faktorin Gjenerik dhe Historik, por
ai nuk mund t& jet& mé i vogél se Faktori Gjenerik.

Pavarésisht nga vlera e faktorit t& synuar, anijet ¢ méposhtme do t& konsiderohen si parési

kryesore pér inspektim:

1. Anijet t& cilat jang raportuar si parési kryesore nga pilotét ose autoritetet portuale né
pérputhje me nenin 1.5 t&€ Memorandumit;

2. Anijet g& transportojné mallra t& rrezikshme ose ndotése, t& cilat nuk kang raportuar
t& gjithé informacionin pérkatés né lidhje me t& dhénat e anijes, 18vizjet ¢ anijes dhe
né lidhje me mallrat ¢ rrezikshme ose ndotése q& transportohen tek autoriteti
kompetent i portit dhe shtetit bregdetar;

3. Anijet g8 kané genég objekt raportimi ose njoftimi nga njé autoritet tjetér;
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6.

7.

Anijet t& cilat kan& gen& objekt i njé raporti ose ankese nga kapiteni, njé anétar i
ekuipazhit, ose ¢gdo person ose organizaté me njé interes legjitim pér funksionimin e
sigurt t& anijes, kushtet e jetesés dhe punds né anije ose parandalimin ¢ ndotjes,
pérveg rasteve kur Autoriteti né fjalg e konsideron raportin ose ankesén si haptazi t&
pabazuar; identiteti i personit q& paraget raportin ose ankesén nuk duhet t'i zbulohet
kapitenit ose pronarit t& anijes né fjalé;

Anijet t& cilat kang qené:

i t& pérfshira né njé pérplasje, tok&zim ose bllokim né rrugén e tyre pér né port,

ii.  t& akuzuara pér shkelje t& pretenduar t& dispozitave pér shkarkimin e
substancave ose efluenteve té€ démshme,

iii.  manovruar né njé ményré t& crregullt ose t& pasigurté ku nuk jan& ndjekur
masat e rrugés, t& miratuara nga IMO, ose praktikat dhe procedurat e sigurta t&
navigimit, ose

iv.  operuar né até ményré qé t& paraqesé rrezik pér personat, pronén ose mjedisin;

Anijet t& cilat jan& pezulluar ose térhequr nga klasa e tyre pér arsye sigurie gjaté 6
muajve t& méparshém;
Anije qé nuk mund t¢ identifikohen né sistemin e informacionit THETIS-Med'.

5 Autoritetet do t'i japin pérparési pér inspektim anijeve me Faktor t& Synuar mé t& larté sig
specifikohet nga sistemi THETIS-Med'. Kriteret dhe pesha e tyre specifikohen né tabelén
1 t& ké&saj shtojce. Faktori i Synuar i anijes do t& jeté shuma e t& gjithé pikéve t8 kritereve
t& zbatueshme. Zbatimi i ploté i Sistemit t& targetimit do t& b&het i zbatueshém kur t&
dhénat statistikore pér t& gjitha kriteret jané t& disponueshme né systemin THETIS-Med!.
Elementét ¢ méposhtém jané t& réndésishém pér faktorin e synimit:

1.

2
3.

Anijet g8 vizitojné njé port t& njé shteti, Autoriteti i t& cilit &shté nénshkrues i
Memorandumit, pér heré t& paré ose pas njé mungese prej 12 muajsh ose mé shumé.
Anije t& pa inspektuara nga ndonjé autoritet brenda 6 muajve t& méparshém,
Anijet, certifikatat statutore t& t& cilave pér ndértimin dhe pajisjet e anijes, t& l8shuara
né pérputhje me Konventat, dhe certifikatat ¢ klasifikimit, jan& l&shuar nga njé
organizaté jo pjesé e Shoqérisé Ndérkombétare t& Shoqérive t& Klasifikimit (IACTS);
Anijet q& mbajné flamurin e njé shteti q8 figurojné né listén e zezé sig &shté publikuar
né raportin vjetor t& Memorandumit t& Mirékuptimit;
Anijet t& cilat jang lejuar nga Autoriteti t& largohen nga njé port i shtetit t& tij né
kushte t& caktuara:
i.  manggsi q& duhet t& korrigjohen para nisjes;

ii.  mangési q& do t& korrigjohen né portin tjetér;

iii.  mangési q& duhet t& korrigjohen brenda 14 ditéve;

iv.  manggsi pér té cilat jang specifikuar kushte t& tjera;

v. nése lidhur me anijen jan& ndérmarré veprimet ¢ duhura dhe t& gjitha

manggsité jané korrigjuar;

Anijet pér t& cilat jang regjistruar manggsi gjaté njé kontrolli t& méparshém, sipas
numrit t& mangésive;
Anijet g& jan& ndalur né njé port t& m&parshém,

L PSCC23/16 - duke zévendésuar t& gjitha referencat pér MEDSIS (sistemet e informacionit t& Med MoU) pér t&
gené THETIS-Med
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8. Anijet q& mbajné flamurin e njé shteti g8 nuk &shté palé né njé instrument pérkatés;

9. Anije t& tjera mbi 13 vite t& vjetra.

TABELA 1

KRITERET

FAKTORI I SYNUAR

Mosha e anijes

0-35vite: 0piké

6 - 10 vite: 5 piké

11 - 15 vite: 10 pikg

16 - 20 vite: 10 + 1 piké pér ¢do vit mbi 15 vjet
>20 vite: 15 + 2 pik& pér ¢do vit mbi 20 vjet

Lloji i anijes

4 piké pér anijet me kodet e tipit 13, 30, 40, 55,
60, 61,70, 71 dhe prej 15 vitesh dhe mbi O piké
pér t& gjithé t& tjerst

Flamuri i anijes - Tejkalimi i ndalimit
mesatar, bazuar né shifrén mesatare 3-vjecare

+1 piké pér ¢do piké pérqindje t& tepért (numri
dhjetor i rrumbullakosur)

0,6 piké pér ¢do mangési t& konstatuar né 4

Mangésité inspektimet e fundit fillestare ose né vazhdim me
manggési té re (numri dhjetor i rrumbullakosur)
N& varési t& numrit t& ndalimeve né 4
inspektimet e fundit:

Ndalimet 1 ndalim - 15 piké

2 ndalime - 30 piké
3 ndalime - 60 piké
4 ndalime - 100 piké

Shogéria e Klasifikimit - jo pjesé ¢ IACS

10 piké

Mangési té theksuara )
(Njé manggsi e regjistruar né THETIS-Med' né
inspektimin e fundit dhe e pa shénuarsi e

2 piké pér ¢do mangési t& pazgjidhur

korrigjuar
(Kodil0))
Koha qé€ nga inspektimi i fundit:
6-12 muaj 3 piks
12-24 muaj 6 piks
Mbi 24 muaj ose nuk &shté inspektuar kurré né pike
50 piks

rajonin ¢ Memorandumit t& Mirékuptimit
Mesdhetar Med MoU (pérfshiré anijet e reja)

Meényra e llogaritjes

Faktori i Synuar &shté shuma e vlerave t&
Faktor&ve t& Synuar t& llogaritur ¢do dité

Niveli i prioritetit
Faktori i Synuar
101 -
41-100
11 - 40
0-10

Prioriteti 1 (shumé i lartg)
Prioriteti 2 (i lart&)
Prioriteti 3 (i mesém)
Prioriteti 4 (i ulét)
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Seksioni 1

Seksioni 2

SHTOJCA 10
REFUZIMI I HYRJES

Dispozitat e Pérgjithshme

N& pérputhje me seksionin 3.8.2 t& Memorandumit, Shtetet ¢ Memorandumit t&

Mirékuptimit Mesdhetar duhet t& refuzojné hyrjen né portet e tyre pér anijet qé&:

1. kang shkuar n& det pa respektuar masat korrigjuese t8 pércaktuara nga porti i
ndalimit (ndalimi i shkelur),

2. nuk kané shkuar né kantierin e treguar t& riparimit;

Ndalimi mund t& higet vetém pas njé riinspektimi t& anijes me shpenzimet e
kompanisé né njé port t& réné dakord nga Oficerét ¢ Kontrollit Shtetéror Portual t&
shtetit ndalues dhe nése ofrohen prova sipas bindjes s& tij se anija pé&rputhet
plotésisht me kérkesat ¢ zbatueshme t& Konventave Ndérkombétare.

Kontrolli Shtetéror Portual mund t& lejojé hyrjen e njé anijeje né rast t& forcés
madhore ose konsideratave mbizotéruese t& sigurisé ose pér t8 zvogéluar ose
minimizuar rrezikun e ndotjes ose pér t& korrigjuar manggsité.

Procedurat pér rastet e méposhtme si dhe dokumentet e sugjeruara t& komunikimit
jan& pérshkruar mé poshté:
1. Lejimi i njé anijeje t& lundrojé né njé kantier riparimi;
Veprimet nése njé anije nuk ia del t& arrij§é n& njé kantier riparimi t&
dakorduar;
3. Veprimet nése njé anije nuk pérmbush urdhrin e ndalimit (ndalimi i shkelur).

Procedura pér Lejimin e njé Anijeje té Lundrojé né njé Kantier Riparimi té
Réné Dakord

Shteti i flamurit ose Organizata ¢ Njohur q& vepron né emér té shtetit t& flamurit
duhet t& konfirmojé me shkrim se anija lejohet t& kalojé né portin mé t& afért t&
disponueshém dhe t& pérshtatshém t& riparimit dhe t& késhillojé ¢do kusht pér
udhétimin (shih letrén “Kérkesé pér Marréveshje pér t& Vazhduar me Njé Kantier
Riparimi”). Kantieri i caktuar i riparimit duhet t& jeté i pranueshém nga shteti i
flamurit/Organizata ¢ Njohur dhe autoriteti i Kontrolli Shtetéror Portual. Kushtet
pér lirim duhet t& jeng t& pranueshme pér shtetin port q& mund t& vendosé kushte
shtesé.

Shteti i flamurit ose organizata e njohur qé vepron né emér t& shtetit t& flamurit
duhet gjithashtu t& 18shojé certifikata t& vetme udhétimi ose mund&sisht t&
miratojé certifikatat ekzistuese. Udh&timi do t& jeté n& balaste dhe do t&
pérjashtojé ¢do operacion tregtar. Pérjashtimisht, ngarkesa tashmé né& bord mund
t& transportohet né portin e riparimit, ose né portet ¢ ndérmjetme t& specifikuara,
kur &shté e sigurts pér ta kryer ké&té. Kéto porte duhet t& pérfshihen né kushtet e
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Seksioni 3

1&shimit (shih letrén “Kushtet e Lirimit nga Ndalimi né njé Port Riparimi”) dhe t&
informohen nése do ta pranonin anijen.

Kompania dhe/ose Kapiteni duhet t'i japin Autoritetit t& Kontrollit Shtetéror
Portual konfirmimin me shkrim t& njé kontrate riparimi ose furnizimi me pajisje
sipas rastit.

Kantieri i riparimit pér t& cilin &shté réné dakord do t& jeté né njé port né t& cilin
do t& ndérmerren veprimet vijuese dhe para se t& lirojé anijen, Zyrtari i Kontrollit
Shtetéror Portual duhet t& marré konfirmimin me shkrim nga autoriteti shtetéror
portual pérkatés se anija do t& pranohet dhe se ata do t'i pérmbahen procedures sé&
komunikimit t& Marréveshjes s& Mirékuptimit (shih letrén “Kérkesé pér
Marréveshje pér t& Vazhduar né njé Kantier Riparimi”)

Kapiteni duhet té informohet me shkrim pér kushtet e lirimit. Kapiteni duhet
gjithashtu t& informohet se anija mund t& ndalohet nése nuk pérmbush kéto kushte
ose nuk hyn né portin e riparimit (shih letrén “Kushtet ¢ Lirimit nga Ndalimi né
njé Port Riparimi).

Kapiteni duhet t& informohet me shkrim se, si kusht lirimi, porti i ndalimit duhet
t& njoftohet menjéheré me shkrim nga autoriteti i kontrollit shtetéror portual t&
portit t& riparimit se anija ka mbé&rritur né kantierin ¢ dakorduar t& riparimit (shih
letrén “Kushtet e Lirimit nga Ndalimi n& nj& Port Riparimi). Né&se nuk dérgohet
njé njoftim, porti ndalues mund t& vazhdojé me 1&shimin e njé urdhri pér
Refuzimin e Hyrjes.

Formulari i inspektimit t& Kontrollit Shtetéror Portual duhet t& b&jé t& qarté se né
cilin port lejohet t& lundrojé anija dhe kohén e parashikuar t& mbérritjes s saj.

Autoriteti i kontrollit shtetéror portual i portit t& riparimit, shteti i flamurit dhe
organizata ¢ njohur duhet t8 informohen pér nisjen ¢ anijes dhe kohén e
parashikuar t& mbérritjes s& saj né portin e riparimit (shih letrén “Kushtet e
Lirimit nga Ndalimi n& njé Port Riparimi)

Procedura Nése njé Anije nuk Arrin té Hyjé né njé Kantier Riparimi té Réné
Dakord

Nése njé anije nuk arrin t& hyjé n& kantierin e riparimit t& réné dakord ose nuk
arrin t& arrijé né kohén e paracaktuar, anija &shté pérgjegjése pér ndalimin.
Vendimi pér t& zbatuar njé ndalim &shté pér shtetin portual q& ndalon, pas
konfirmimit se anija nuk &shté drejtuar né kantierin ¢ dakorduar t& riparimit ose
nuk pérmbush kushtet e lirimit (pérfshiré njoftimin ¢ mbérritjes) ose ndryshe nuk
ka respektuar urdhér ndalimin. Para 18shimit t& Urdhrit t& Refuzimit t& Hyrjes,
shteti ndalues mund t& kérkojé konsultime me Administratén Shtetérore t&
flamurit t& anijes.
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2 Kur zbatohet njé ndalim, Autoriteti Detar i shtetit ndalues do t& ké&shillojé
Kompaning ISM! qé ndalimi éshté né fuqi. Kjo letér do t'i dérgohet edhe shtetit t&
flamurit, organizatave t& njohura, shoqérive t& klasifikimit, anétaréve t&
Memorandumit t& Mirékuptimit Mesdhetar, Sekretariatit t& Memorandumit t&
Mirékuptimit Mesdhetar, menaxherit t& THETIS-Med!, Sekretariateve t&
Memorandumit t& Mirékuptimit bashk&punues dhe Rojes Bregdetare t& Shteteve
t& Bashkuara. Menaxheri i bazés s& t& dhénave duhet t8 informohet p&rmes
sistemit t& informacionit.

3 Njoftimi se njé anije e ndaluar do & shfaqet né ekranin e identifikimit t& anijes n&
sistemin e informacionit THETIS-Med' dhe lista e anijeve t& ndaluara né fagen e
internetit t& Med MoU do t& pérditésohet njékohé&sisht.

4 N& rastin e njé anijeje t& ndaluar pér mospérputhje me kushtet pér njé lundrim t&
sigurté dhe t8 vetém né njé kantier riparimi, njé kérkesé zyrtare nga kompania
ISM pér heqgjen e ndalimit duhet t'i b&het shtetit ndalues. Ndalimi mund t& higet
vetém pas njé ri-inspektimi t& anijes me shpenzimet e kompanisé né njé port té
réné dakord nga Zyrtari i Kontrollit Shtetéror Portual i shtetit ndalues dhe nése
ofrohen prova sipas bindjes s& tij se anija &shté plotésisht né pérputhje me
kérkesat e zbatueshme t& Konventave Ndérkombétare.

5 Nése porti i ri-inspektimit pér t& cilin &shté réné dakord &shté né rajonin e
Memorandumit t& Mirékuptimit Mesdhetar, autoriteti shtetéror portual i atij porti,
me marréveshjen e shtetit port ndalues, mund t8 autorizojé anijen t& vazhdojé me
t&, me qéllimin e vetém pér t& verifikuar q& anija pérmbush kushtet e specifikuara
né paragrafin 4. Kur shteti ndalues dhe kompania ISM bien dakord t&
riinspektojné né njé port jashté rajonit t& Memorandumit t& MirSkuptimit
Mesdhetar, kompania do t& konsultohet me até shtet port pér t& réné dakord pér
hyrjen dhe nése po, kompania do t'i dérgojé konfirmim me shkrim shtetit ndalues.
Vendimi pér hegjen e ndalimit i mbetet shtetit ndalues.

6 T& gjitha shpenzimet q& lidhen me ri-inspektimin ¢ njé anijeje t& ndaluar do t&
pérballohen nga kompania ISM.

7 Nése ri-inspektimi nuk ka rezultate t& kénaqshme, ndalimi nuk do t& higet.
8 Nése anija &shté né nj& port jashté juridiksionit t& Zyrtarit t& Kontrollit Shtetéror

Portual q& kryen ri-inspektimin dhe Zyrtari i Kontrollit Shtetéror Portual beson se
anija &shté né gjendje t& ndalueshme, atéheré Zyrtari i Kontrollit Shtetéror Portual
duhet t& informojé shtetin port ku ndodhet anija né ményré q& t& mund t&
shqyrtojé veprimet pér ndalimin ¢ anijes. Nése anija nuk p&rmbush kérkesat,
ndalimi nuk do t& higet.

1 Shénim i Pérkthyesit: Kompania ISM nénkupton entitetin juridik g& menaxhon anijen né pérputhje me Kodet e
Menaxhimit Ndérkombétar t& Sigurisé (ISM) dhe Kodet Ndérkombétare t& Anijeve dhe Porteve (ISPS).
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10

11

12

Pér t& hequr ndalimin, kompania duhet t'i drejtojé njé kérkesé zyrtare autoritetit
Kontrollit Shtetéror Portual t8 shtetit anétar q& ka vendosur ndalimin. Kjo kérkesé
duhet t& shogérohet me:

1. njé dokument nga administrata ¢ shtetit t& flamurit q& specifikon se anija
&shté plotésisht n& pérputhje me t& gjitha dispozitat ¢ konventave
ndérkombétare né fuqi. Dokumenti mund t& jeté né formén e njé deklarate
zyrtare, por duhet t& l&shohet nga administrata ¢ flamurit dhe jo njé
organizaté ¢ njohur.

2 njé dokument nga shogéria/shoqatat e klasifikimit q& klasifikon anijen q&
anija pérputhet me standardet e klasés t& pércaktuara nga ajo
shoqéri/shoqéri. Shoqgéria(té) e klasifikimit duhet gjithashtu t& sigurojé
déshmi se njé vizité n& bord &sht& kryer para 1&shimit t& dokumentit, nése
&shté e pérshtatshme

Nése ri-inspektimi siguron prova té kénaqshme pér shtetin ndalues se anija
pérmbush plotésisht t& gjitha kérkesat ¢ Konventave, ndalimi do t& hiqet.
Kompania do t& informohet pér heqgjen ¢ ndalimit nga shteti ndalues. Kjo letér do
t'i kopjohet shtetit t& flamurit, organizatave t& njohura, shoqgérive t& klasifikimit,
anétaréve t& Memorandumit t& Mirékuptimit Mesdhetar, Sekretariatit t&
Memorandumit t& Mirékuptimit Mesdhetar, menaxherit t& THETIS-Med:,
Sekretariateve t& Memorandumit t& Mirékuptimit bashképunues dhe Roja
Bregdetare e Shteteve t& Bashkuara.

THETIS-Med' do t& heqé njoftimin nga ekrani i identifikimit t& anijes. Anija do t&
higet nga lista ¢ ndaluar né fagen e internetit t& Memorandumit t& Mirékuptimit
Mesdhetar njékohésisht.

Kompania ka t& drejté t& apelojé kundér ndalimit né pérputhje me legjislacionin e
veté shteteve portuale.
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. . KONTROLLI SH'}:ETEROR PORTUAL
KERKESE PER MARREVESHJE PER TE VAZHDUAR NE NJE KANTIER RIPARIMI

Nga: (Zyra e Kontrollit Shtetéror Portual e (portit)) Faksi:
Pér: (Autoriteti Shtetéror Portual i kantierit té riparimit)

(Autoriteti i Shtetit té Flamurit)
Kopje pér:  (Organizatén e Njohur qé léshon certifikatat pérkatése)

Emri i anijes ....
Lloji i anijes .
Tonazhi bruto ..

Shenja e thirrjes ...

Organizata(t) ¢ Njohura .............. Shoqéria(t8) e Klasifikimit ........cccovovrvernnen

Anija ¢ lartpérmendur &shté ¢ ndaluar ng (port) por nuk mund t& korrigjojé t& gjitha
mangésité. Mjeti lundrues ka kérkuar g& t& riparohen manggsité e méposhtme né (port).
Mangésité qé nuk mund Veprimi i sugjeruar:

té riparohen né portin aktual (pérfshiré veprimin né portin tjetér)

Para se té Iéshojé anijen, ky Autoritet kérkon:

1. Autoriteti i Kontrollit Shtetéror Portual pér portin e [emri] t& konfirmojé me faks ose email
nése anija e sipérpérmendur lejohet t& hyjé né até port dhe se do t& kryhet njé inspektim
vijues;

2. Autoriteti i Shtetit t& Flamurit (nése &shté e nevojshme népérmjet organizatés sé tij t& njohur)
t& konfirmojé me faks se anija e sipérpérmendur lejohet t& vazhdojé né (port) dhe ¢do kusht
pér lundrimin.

Autoriteti Raportues .........ovvvovrvsecnsinencenenns L
Faksi:
Email:
Tel:
Data
Emri & Nénshkrimi

(Oficeri i Kontrollit Shtetéror Portual i autorizuar sipas rregullave)
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SHTOJCA 11
LISTA E CERTIFIKATAVE QE DUHET VERIFIKUAR

Gjaté njé inspektimi, Zyrtari i Kontrollit Shtetéror Portual do t& shqyrtojé minimalisht dhe ng
masén e zbatueshme dokumentet ¢ méposhtme:

1.

11.

12.

13.

14.
15.

16.
17.
18.
19.
20.

21.

22.

Certifikata Ndérkombétare e Tonazhit (1969) (ITC, Neni 7),

Certifikata ¢ Regjistrit ose dokument tjetér i shtetésisé (Konventa ¢ Kombeve t&
Bashkuara pér t& Drejtén e Detit),

Certifikatat pér forcén e trupit t8 anijes dhe instalimet ¢ makinerive t& l&shuara nga
shoqgéria e klasifikimit né fjals (q& kérkohet vetém nése anija mban klasén e saj me njé
shogqgri klasifikimi),

Raportet ¢ inspektimeve t& méparshme t& kontrollit shtetéror portual;

Certifikata e sigurisé s& anijes sé& pasagjeréve (SOLAS 1988 Amendamenti/CI/Regj.12,
Protokolli SOLAS 1988/CI/Regj.12),

Certifikata e ndértimit t& sigurisé s& anijes sé& ngarkesave (SOLAS/CI/Reg .12, Protokolli
SOLAS 1988/CI/Regj.12),

Certifikata e Sigurisé s& Pajisjeve t& Anijeve t& Mallrave (SOLAS 1988
Amendamenti/CI/Regj.12, protokolli SOLAS 1988/CI/Regj. 12);

Certifikata e Radios s& Sigurisé s& Anijeve t& Mallrave (SOLAS 1988
Amendamenti/CI/Regj.12, Protokolli SOLAS 1988/CI/Regj.12);

Certifikata e sigurisé s& anijes s& ngarkesave (Protokolli SOLAS 1988/CI/Regj.12),
Certifikata e sigurisé s& anijes pér géllime t& veganta (Kodi SPS, CI/Art.1.7.4, Res. A.791
(19));

Pér anijet ¢ pasagjeréve ro-ro, informacion mbi raportin A/A-maksimal (SOLAS 1995
Amendamenti/CII-1/Regj.8-1),

Planet dhe broshurat e kontrollit t& démeve (SOLAS 2006 Amendamenti/CII-1/Regj.19,
20, 239;

Broshura e Stabilitetit dhe informacioni (SOLAS 2008 Amendamenti/CII-1/Regj.5,
SOLAS/C//-1/Regj.22, LLP88, Regj.10),

Broshura i manovrimit dhe informacionit (SOLAS 1981 Amendamenti/CII-1/Regj.28.2);
Evidenca e hapésirave t& pambikéqyrura té makinerisé (UMS) (SOLAS 1981
Amendamenti/CII-1/Regj.46.3),

Certifikata e p&rjashtimit dhe ¢do listé ngarkesash (SOLAS/CII-2/Regj.10.7.1.4);

Plani i kontrollit t& zjarrit (SOLAS 2000 Amendamenti/CII-2/Reg .15.2.4),

Broshura operacionale e sigurisé nga zjarri (SOLAS 2000 Amendamenti/CII-
2/Regj.16.3.1),

Lista speciale ose manifesti i mallrave t8 rrezikshme, ose plani i detajuar i depozitimit
(SOLAS 2000 Amendamenti/CII- 2/Regj.19);

Dokumenti i pérputhshmérisé Mallrat ¢ Rrezikshme (SOLAS 2001 Amendamenti/CII-
2/Regj.19.4),

Ditari i anijes né lidhje me t& dhénat e stérvitjeve, duke pérfshiré stérvitjet e sigurisé, dhe
regjistrin pér regjistrimet ¢ inspektimit dhe mirémbajtjes sé& pajisjeve dhe rregullimeve
pér shpétimin e jetés dhe pajisjeve dhe rregullimeve t& zjarrfikésve (SOLAS 2006
Amendamenti/CIII/Regj.37, 19.3, 19.4, 20);

Dokumenti Personeli Minimal i Sigurisé (SOLAS 2000 Amendamenti/CV/Regj.14.2);
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23.

24.

25.

26.

27.

28.

29.

30.

31

32.

33.

34

35.

36.

37.

38.

39.

40.

41.

42.
43.

Plani i koordinimit t& Konventés Ndérkombétare pér Kérkimin dhe Shpétimin Detar
(SAR) pér anijet e pasagjeréve q& tregtojné né rrugé fikse (SOLAS 1995
Amendamenti/CV/Reg .15, 7.2);

Raporti i Testit t& Konformitetit LRIT (SOLAS/CV/Regj.19.1);

Kopje ¢ Dokumentit t& pérputhshmérisé t& l&shuar nga objekti i testimit, duke treguar
datén e pérputhshmérisé dhe standardet e zbatueshme t& performancés s& VDR
(Regjistruesit t& t& Dhénave t& Udhétimit) (SOLAS/CV/Regj.18.8);

Raporti 1 testit t& Sistemit Automatik t& Identifikimit AIS (SOLAS 2010
Amendamenti/CV/Reg .18.9),

Pér anijet e pasagjeréve, Lista e kufizimeve operacionale (SOLAS 2001
Amendamenti/CV/Regj.30.2),

Manuali i Sigurimit t& Ngarkesave (SOLAS 2002 Amendamenti/CVI/Regj.5.6);

Broshura e Transportuesit me Shumicé (SOLAS 1996 Amendamenti/CVI/Regj.7.3);

Plani i Ngarkimit/Shkarkimit pér Transportuesit me Shumicé (SOLAS 1996
Amendamenti/CVI/Regj. 7.3),

Dokumenti i  autorizimit pé&r  transportin e  grurit (SOLAS 1991
Amendamenti/CVI/Regj.9);

Fletst e t& Dhénave t& Siguris¢ s& Materialit (MSD) (SOLAS 2009
Amendamenti/CVI/Regj.5-1);

INF (Kodi Ndérkombétar pér Transportin e Sigurté t& Karburantit Bérthamor t& Paketuar
t& Rrezatuar, Plutoniumit dhe Mbetjeve Radioaktive t& Nivelit t& Larté né Bord)
Certifikata e Pérshtatshmérisé (SOLAS 1999 Amendamenti/CVII/Regj.16, INFC 1.39),
Kopja e Dokumentit t& Pajtueshmérisé e 18shuar né pérputhje me Kodin Ndérkombétar t&
Menaxhimit pér Operimin e Sigurté t& Anijeve pér Parandalimin e Ndotjes (DoC) Kodi
ISM (SOLAS 1994 Amendamenti/CIX/Regj.4.1),

Certifikata ¢ Menaxhimit t& Sigurisé e l&shuar n& pérputhje me Kodin Ndérkombétar t&
Menaxhimit pér Operimin ¢ Sigurté t& Anijeve dhe pér Parandalimin ¢ Ndotjes (SMC)
(SOLAS 1994 Amendamenti/CIX/Regj.4.2, 4.3);

Certifikata e Sigurisé s& Mjeteve me Shpejtési t& Larté dhe Leja pér t& Operuar me Anije
me Shpejtési t& Larté (SOLAS 1994 Amendamenti/CX/Regj.3 .2, HSCC 1.8.1,2);
Regjistrim i Pérmbledhjes s& Vazhdueshme (SOLAS 2005 Amendamenti/CXI1-1/Reg .5);
Certifikata Ndérkombétare ¢ Pérshtatshmérisé pér Transportimin e Gazrave t& Léngshém
me Shumicé, ose Certifikata ¢ Pérshtatshmérisé pér Transportin ¢ Gazrave t& Léngshém
me Shumicg, cilado q& &shté e pérshtatshme (GCC-4/CI/NI .6.4, IGCC/CIUNI .5.4),
Certifikata Ndérkombétare e Pérshtatshmérisé pér Transportin ¢ Kimikateve t&
Rrezikshme me Shumicg, ose Certifikata e Pérshtatshmérisé pér Transportin e
Kimikateve t& Rrezikshme me Shumicg, cilado q& &shté e pérshtatshme (BCC-
10/CI/NL6.3, IBCC/CI/NL. 5.4, BCH/1/1.6.1),

Certifikata ~ Ndérkombétare e Parandalimit ~ t& Ndotjes nga  Nafta
(MARPOL/ANT/Regj.7.1),

Dosjet e Raportit t& Anketds (né rastin e transportuesve me shumicé ose cisternave té
naftés) (SOLAS X/-1 Regj.2, 2011 Kodi Programi i Mbikqyrjes s& Pérmirésuar (ESP));
Libri i t& Dhénave t& Naftés, pjesa I dhe II (MARPOL/ANI/R17, Regj.36),

Plani i emergjencés pér ndotjen detare t& anijeve pér substancat e 1&ngshme t& démshme
(MARPOL/ANII/Regj.17),
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66.
67.

68.

69.

70.

71.

Deklarata (¢ ndérmjetme) e Pérputhshmérisé Skema e Vlerésimit t& Gjendjes (CAS)
(MARPOL/ANT/Regj.20.6, 21.6.1);

Pér cisternat ¢ naftés, regjistrimi i sistemit t& monitorimit dhe kontrollit t8 shkarkimit t&
naftés pér lundrimin e fundit t& gakéllit (MARPOL/ANT/Regj.31.2);

Plani Emergjent i Ndotjes s& Naftés né Anije (SOPEP) (MARPOL/ANT/Regj.37.1),

Plani i Operacionit Anije né Anije STS dhe Regjistrimet e Operacioneve Anije né Anije
(MARPOL ANT/Regj.41);

Certifikata Ndérkombétare e Parandalimit t& Ndotjes pér Transportin ¢ Substancave t&
Léngshme t8 Démshme me Shumicé (NLS) (MARPOL/ANII/Regj.9.1);

Libri i Regjistrimit t8 Ngarkesave (MARPOL/ANII/Regj.15, MARPOL/ANII-Shtojca 2),
Manuali i Procedurave dhe Marréveshjeve (cisterna kimike dhe cisterna t& Substancave t&
Léngshme t8 Démshme) (MARPOL/ANII/Regj.14.1+ manuali P& A),

Certifikata Ndérkombétare ¢ Parandalimit t& Ndotjes s& Ujérave t& Zeza (ISPPC)
(MARPOL/ANIV/Regj.5.1);

Plani i Menaxhimit t& Plehrave (MARPOL/ANV/Shtojca I);

Libri i Regjistrimit t& Mbetjeve (MARPOL/ANV/Shtojca II);

Certifikata Ndérkombétare e Parandalimit t& Ndotjes s& Ajrit (IAPPC)
(MARPOL/ANVI/Regj.6.1);

Ditari pér ndérrimin e karburantit MARPOL/ANVT/Regj.14.5);

Certifikata ¢ miratimit t& tipit t8 inceneratorit (MARPOL/ANVI/Regj.16.6.1+Shtojca
v(D;

Fletén e dorézimit t& karburantit t& naftés (MARPOL/ANVI/Regj.18.5+ Shtojca V);
Certifikata Ndérkombétare e Efigencés s& Energjisé (MARPOL/ANVI/Regj.6),

Plani i Menaxhimit t& Efigencés s& Energjisé s& Anijeve (SEEMP)
(MARPOL/ANVI/Regj.22),

Dosja  Teknike Indeksi 1 Projektimit t& Efikasitetit t8 Energjis¢ EEDI
(ARPOL/ANVI/Reg. 20);

Deklarata ¢ Pajtueshmérisé-Raportimi i Konsumit t& Naftés (MARPOL/ANVI/Regj.6);
Certifikata Ndérkombétare e Parandalimit t& Ndotjes s& Ajrit t& Motorit (EIAPPC)
(NoxTC2008/21.1.1),

Dosjet teknike (NoxTC2008/2.3.6),

Libri i regjistrimeve t8 parametrave t& motorit (NoxTC2008/6.2.2.7.1);

Certifikata Ndérkombétare e Linjés s& Ngarkesés (1966) (LLP'88 Art.16 .1);

Certifikata e Pérjashtimit nga Linja Ndérkombétare ¢ Ngarkesés (LLP'88 Neni 16.2),
Certifikatat e L&shuara né& pérputhje me Konventén Ndérkombétare pér Standardet e
Trajnimit, Certifikimit dhe Vrojtimit pér Detarét (STCW) (STCW95/Neni VI, RI/2, Kodi
STCW/Neni A-1/2),

Certifikata ¢ Pun&s Detare dhe Deklarata e Pérputhshmérisé sé Punés Detare pjesé e tokés
II (Konventa ¢ Puné&s Detare dhe Deklarata ¢ Pérputhshmérisé s& Punés Detare (DMLC)
pjesa I dhe IT) (MLC, 2006/Regj.5.1/standardi A5.1.3);

Certifikata mjek&sore (MLC, 2006/ Regj.1.2/Standard AL.2),

Tabela ¢ aranzhimeve t& punds né anije (MLC, 2006/Regj.2.3/standard A2.3, 10 dhe
STCW95/A VIIV1.5),

Té& dhénat e oréve t& punds ose pushimit t& detaréve (MLC, 2006/Reg. 2.3/standard A2.3,
12 dhe STCW95/A-VIII/1.5),
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76.
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Certifikaté ose déshmi dokumentare e sigurisé financiare pér riatdhesim (MLC,
2006/Regj.2.5/standard A2.5.2),

Certifikaté ose dé&shmi dokumentare ¢ sigurisé financiare né lidhje me detyrimin e
pronaréve t& anijeve (MLC, 2006/Regj.4.2/standard A4.2.1),

Certifikata ¢ Sigurisé e Njésisé s& Shpimit t8 Lé&vizshém né Det t& hapur (MODU
Kodi/I/Neni 6);

Certifikaté sigurimi ose ¢do garanci tjetér financiare né lidhje me pérgjegjésing civile pér
démet nga ndotja e naftés (CLC69P92/AVIL2),

Certifikaté sigurimi ose ¢do garanci tjetér financiare né lidhje me pérgjegjésing civile pér
démtimin e ndotjes nga nafta e bunkerit (BUNKERS 2001/Neni 7.2);

Certifikata Ndérkombétare e Sigurisé s& Anijeve (ISSC) (ISPSC/PA/19.2.1);

Regjistrimi i Sistemeve Kundér Ndotjes (AFS/Shtojca 4/Rregullorja 2(1),

Certifikata Ndérkombétare ¢ Sistemit Kundér Ndotjes (Certifikata IAFS) (AFS/Shtojca4
/Regj.2(1),

Deklarata pér Sistemet Kundér Ndotjes (AFS/Shtojca 4/Rregullorja 5(1));

Certifikata Ndérkombétare ¢ Menaxhimit t& Ujit Caké&ll IBWMC) (BWMC Neni 9.1 (a)),
Libri i Regjistrimit t& Ujit Cakéll (BWRB) (BWMC Neni 9.1 (b)),

Certifikaté sigurimi ose siguri tjetér financiare né lidhje me pérgjegjésing pér eleminimin
e rrénojave (Nairobi WRC 2007/Neni 12.2)
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MEMORANDUM OF UNDERSTANDING ON PORT STATE CONTROL
IN THE MEDITERRANEAN REGION

The Maritime Authorities'of
Algeria

Croatia®

Cyprus

Egypt

Isracl

Jordan?

Lebanon

Malta

Morocco

Tunisia

Turkey

Palestinian Authority*

hereinafter referred to as "the Authorities"

Recognizing the need to increase maritime safety and the protection of the marine environment and the
importance of improving living and working conditions on board ships;

Recalling the Declaration adopted on 28 November 1995 on the occasion of the Euro-Mediterranean
Conference in Barcelona, establishing a Euro-Mediterranean partnership and including, inter alia, co-
operation in maritime safety and pollution prevention in the Mediterranean basin;

Noting with appreciation the progress achieved in these fields, in particular by the International Maritime
Organization (IMO) and the International Labour Organization (ILO);

Noting also the contribution which has and which can be made by the European Community towards
meeting the above-mentioned objectives;

Mindful that the principal responsibility for the effective application of standards laid down in international
instruments rests upon the authorities of the State whose flag a ship is entitled to fly;

Recognizing nevertheless that effective action by port States is required to prevent the operation of
substandard ships;

Recognizing also the need to avoid distorting competition between ports;

Convinced of the necessity, for these purposes, of an improved and harmonized system of port State control
and of strengthening co-operation and the exchange of information;
Have reached the following understanding:

! Maritime Authorities are the national maritime administrations designated for the implementation of this Memorandum.

2 Croatia adhered to the Memorandum starting from the 1% of January 2024

3 Jordan joined the Med MoU in 1999 {Amendment No.(2)}

4 Palestine Authority memberships was discussed by the committee in its 1* meeting and noted the communication by the Maritime Authority of Israel informing
on certain internal procedural arrangements witch would prevent the signing of the Mediterranean MoU by the Palestinian Authority. In the absence of the
delegations of Isracl and Palestinian Authority, the committee agreed to defer consideration of the matter until both Authorities presented in the committee
meeting. The committee noted, however, that as the delegation of the Palestinian Authority was unable to sign the Mediterranean MoU within the period
prescribed for its signature (i.e. 12 July 1997 to 23 Feb. 1998 ) considered that the matter raised by the Maritime Authority of Isracl can be dealt with in due
course under the procedures prescribed in Section 8 of the Memorandum. {Amendment No.(1)}
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Section 1 Commitments

1.1

1.2

1.3

1.4

1.5

Each Authority will give effect to the provisions of the present Memorandum and the Annexes
thereto which constitute an integral part of the Memorandum, and take all necessary steps to ratify
instruments relevant for the purposes of this Memorandum.

Each Authority will maintain an effective system of Port State Control with a view to ensuring that,
without discrimination as to flag, foreign merchant ships calling at a port of its State, or anchored off
such a port, comply with the standards laid down in the relevant instruments as defined in section 2.
Each Authority may also carry out controls on ships at off-shore installations.

Each Authority will achieve, within a period of 3 years from the coming into effect of the
Memorandum an annual total of inspections corresponding to 15% of the estimated number of
individual foreign merchant ships, hereinafter referred to as "ships", which entered the ports of its
State during a recent representative period of 12 months. The Committee established pursuant to
Section 6.1 will monitor the overall inspection activity and its effectiveness throughout the region.
The Committee will also adjust the target inspection rate based on experience gained and progress
made in the implementation of the Memorandum of Understanding.

Each Authority will consult, co-operate and exchange information with the other Authorities in
order to further the aims of the Memorandum.

Each Authority, or any other body, as the case may be, will establish an appropriate procedure for
pilot services and port authorities to immediately inform the competent Authority of the port State,
whenever they leamn in the course of their normal duties that there are deficiencies which may
prejudice the safety of the ship, or which may pose a threat of harm to the marine environment.

Section 2 Relevant instruments

21

2.2

2.3

2.4

For the purposes of the Memorandum "relevant instruments” are, together with the Protocols and
amendments to these instruments and related codes of mandatory status in force is as indicated in
(Annex 1)

With respect to the Merchant Shipping (Minimum Standards) Convention, 1976 (ILO Convention
147). Each Authority will apply the instructions in Annex 1 for the application of ILO publication
“Inspection of Labour Conditions on board Ship: Guidelines for procedure".

Each Authority will apply those relevant instruments which are in force and to which its State is a
Party. In the case of amendments to a relevant instrument, each Authority will apply those
amendments which are in force and which its State has accepted. An instrument so amended will
then be deemed to be the "relevant instrument" for that Authority.

When inspecting a ship flying the flag of a State not party to a Convention or a "relevant instrument”
as amended for the purposes of port State control, the Authorities which are party to such
Convention or "relevant instrument” as amended shall ensure that the treatment given to such ship
and its crew is not more favorable than that given to ships flying the flag of a State which is party to
that Convention or "relevant instrument”.
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2.5

In the case of ships below 500 tons gross tonnage the Authorities will apply those requirements of
the relevant instruments which are applicable and will to the extent that a relevant instrument does
not apply take such action as may be necessary to ensure that those ships are not clearly hazardous
to safety, health or the environment, having regard, in particular to Annex 1.

Section 3 Inspection procedures, Rectification and Detention

3.1.1

3.1.2

3.2.1

3.2.2

3.2.3

3.2.4

3.3

In implementing the Memorandum, the Authorities will carry out inspections which will consist of a
visit on board a ship in order to check the validity of the certificates and other documents relevant
for the purposes of the Memorandum as well as the condition of the ship, its equipment and crew, as
well as the living and working conditions of the crew.

The Authority shall ensure that the inspector shall, as a minimum, check the certificates and
documents listed in Annex 1, to the extent applicable and satisfy himself of the overall conditions of
the ship including the engine room and the accommodations and the hygienic conditions.

Whenever there are clear grounds for believing that the condition of a ship or of its equipment or
crew does not substantially meet the requirements of a relevant instrument a more detailed
inspection shall be carried out, including further checking of compliance with on-board operational
requirements.

Clear grounds exist when the inspector finds evidence which in his professional judgement warrants
a more detailed inspection of ship, equipment or crew. The Authorities will regard as clear ground,
inter alia, those set out in Annex 3.

Nothing in these procedures should be construed as restricting the powers of the Authorities to take
measures within its jurisdiction in respect of any matter to which the relevant instruments relate.

The relevant procedures and guidelines for control of ships specified in Annex 1 shall also be
applied.

In selecting ships for inspection, the Authorities shall give priority to the following ships:

Ships visiting a port of a State, the Authority of which is a signatory to the Memorandum, for
the first time or after an absence of 12 months or more;

Ships which have been permitted to leave the port of a State; the Authority of which is a
signatory to the Memorandum, on the condition that the deficiencies noted must be rectified
within a specified period, upon expiry of such period,

Ships which have been reported by pilots or port authorities as having deficiencies which may
prejudice their safe navigation;

Ships whose statutory certificates on the ship's construction and equipment, have not been
issued in accordance with the relevant instruments.

Ships carrying dangerous or polluting goods, which have failed to report all relevant
information concerning the ship's particulars, the ship's movements and concerning the
dangerous or polluting goods being carried to the competent authority of the port and coastal
State;
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3.4

3.5.1

3.5.2

3.53

3.5.4

3.6.1

3.6.2

3.6.3

3.6.4

3.6.5

Ships which have been suspended from their class for safety reasons in the course of the
preceding six months.

The Authorities will seek to endeavour to inspect ships which have not been inspecting within the
previous 6 months by other Authorities unless there are clear grounds for inspection. These
procedures are not applicable to ships listed under 3.3 which may be inspected whenever the
Authority deems appropriate.

Inspections will be carried out only by a person, duly authorized by his Authority to carry out port
State inspections and responsible to that Authority, who fulfils the requirements of paragraph 3.5.3
and the qualification criteria specified in Annex 7.

The inspector carrying out port State control may be assisted by a person with the required expertise
when such expertise cannot be provided by his Authority.

The inspector carrying out port State control and the person assisting him shall have no commercial
interest either in the port of inspection or in the ships inspected, nor shall the inspector be employed
or undertake work on behalf of non-governmental organizations which issue statutory and
classification certificates or which carry out the surveys necessary for the issue of those certificates
to ships.

Each Inspector shall carry a personal document in the form of an identity card issued by his
authority indicating that the inspector is authorized to carry out inspections. A common model for
such an identity card is attached at Annex 7.

On completion of an inspection the master of ship shall be provided by the inspector with a
document in the form specified in Annex 5 to this Memorandum of Understanding, giving the
results of the inspection and details of any decision taken by the inspector and of the corrective
action to be taken by the master, owner, or operator.

The Authority shall be satisfied that any deficiencies confirmed or revealed by the inspection are
rectified.

In the case of deficiencies which are clearly hazardous to safety, health or the environment the
Authority will detain the ship or will stop the operation in the course of which the deficiencies have
been revealed The detention order or the stoppage of the operation shall not be lifted until the hazard
is removed, except under the conditions provided for in 3.8.1 below.

When exercising his professional judgment as to whether or not a ship should be detained, the
inspector shall be guided by the criteria set out in Annex 1.

Where the ground for a detention is the result of accidental damage suftered on the ship’s voyage to
a port or during cargo operations, no detention order will be issued, provided that:

1. due account has been given to the requirements contained in Regulation I/11(c) of SOLAS
regarding notification to the flag Administration, the nominated surveyor or the recognized
organization responsible for issuing the relevant certificate;
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3.6.6

3.7

3.8.1

3.8.2

3.8.3

3.9

2. prior to entering a port or immediately after a damage has occurred, the master or ship owner has
submitted to the port State control authority details on the circumstances of the accident and the
damage suffered and information about the required notification of the flag Administration;

3. appropriate remedial action, to the satisfaction of the Authority, is being taken by the ship, and

4. the Authority has ensured, having been notified of the completion of the remedial action, that
deficiencies which were clearly hazardous to safety, health or the environment have been
addressed to the satisfaction of the Authority.

In exceptional circumstances where, as a result of a more detailed inspection, the overall condition
of a ship and its equipment, also taking the seafarers and their living and working conditions into
account, is found to be obviously substandard, the Authority may suspend an inspection. The
suspension of the inspection may continue until the responsible parties have taken the steps
necessary to ensure that the ship complies with the requirements of the relevant instruments. Prior to
suspending an inspection, the Authority must have recorded detainable deficiencies in several areas.
The notification of the detention to the responsible parties will state that the inspection is suspended
until the Authority has been informed that the ship complies with all relevant requirements.

In the event that a ship is detained the Authority shall immediately inform the administration of the
State whose flag the ship is entitled to fly and the consul or, in his absence, its nearest diplomatic
representative of the action taken. Where relevant, the organization responsible for the issue of the
certificates shall also be informed.

Where deficiencies referred to in 3.6.3 cannot be remedied in the port of inspection, the Authority
may allow the ship to proceed to another port, or the nearest repair yard subject to any appropriate
conditions determined by that Authority with a view to ensuring that the ship can so proceed without
danger to safety, health or the environment. In such circumstances the Authority will notify the
competent Authority of the region State where the next port of call or the repair yard is situated, the
parties mentioned in 3.7 and any other Authority as appropriate. Notification to Authorities will be
made in accordance with Annex 5. The Authority receiving such notification will inform the
notifying Authority of action taken.

The Authorities will take measures to ensure that ships referred to in 3.8.1 which either proceed to
sea without complying with the conditions determined by the Authority which detained the ship or
which do not call into the agreed port or yard to undertake repairs, shall be refused access to any
port within this Memorandum until the owner or operator and the flag State notify the Authority of
the State where the ship was found defective or the Authority which receives the vessel that the ship
complies with all applicable requirements of the relevant instruments. In the latter case, the
receiving Authority will notify all other Authorities of such compliance.

In the exceptional event of "force majeure", access to a specific port may be permitted to minimize
the risk of life or of pollution.

The provisions of Section 3.7 and 3.8 are without prejudice to the requirements of relevant
instruments or procedures established by international organizations concerning notification and
reporting procedures related to port State control.
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3.10

3.11

3.12

3.13

3.14

When exercising control under the Memorandum, the Authorities will make all possible efforts to
avoid unduly detaining or delaying a ship. Nothing in the Memorandum affects rights created by
provisions of relevant instruments relating to compensation for undue detention or delay.

In case the master, owner or agent of the ship notifies the port State control Authorities prior to or
upon arrival of the vessel at the port, of any damage, breakdown or deficiency to the ship, its
machinery and equipment, which is intended to be repaired or rectified before the ship sails from
that port, the detention should be recorded only if deficiencies justifying detentions are found after
the master has given notification that the ship was ready for inspectors. The same procedure applies
when the port State control Authorities are notified that the ship is scheduled to be surveyed at the
port with respect to flag, statutory or class requirements.

In exceptional circumstances, when a ship on its way to a specified repair yard needs to call at a port
for temporary repairs for safety reasons, it may be allowed into that port. All commercial operations
are forbidden, except the unloading of its cargo if required for safety reasons. The ship may be
allowed to proceed to the specified repair yard only if the flag State of the ship has issued statutory
certificates to the ship restricting their validity to that specific voyage, and the port State is satisfied
that such ship shall not pose undue risk to safety of ship, or to the environment or cause undue
hardship to the crew.

The owner or the operator of a ship will have the right of appeal against a detention decision to
higher administrative Authority or to the Court of competent jurisdiction, according to the law in
each country. However, an appeal shall not cause the detention to be suspended

Should an inspection reveal deficiencies warranting detention of a ship, all costs relating to
inspections subsequent to the first shall be covered by the ship owner or the operator. The detention
shall not be lifted until full payment has been made or a sufficient guarantee has been given for the
reimbursement of the costs.

Section 4 Provision of information

4.1

42
@

(b)

©

Each Authority will report on its inspections under the Memorandum and their results, in accordance
with the procedures specified in Annex 4.

The Authorities will supply the following information to the Memorandum Secretariat :

Number of inspectors working on their behalf on port State inspections. Where inspections
work on a part-time basis, the total is corrected into a number of full time employed inspectors;

Number of individual ships entering their ports in a representative year prior to the
Memorandum;

Fees for inspections, if any.

This information will be updated at least every three years.
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Section 3 Operational violations

The Authorities will upon the request of another Authority endeavour to secure evidence relating to
suspected violations of the requirements on operation matters of Rule 10 of the International Regulations for
Preventing Collisions at Sea, 1972 and the International Convention for the Prevention of Pollution from
Ships, 1973, as modified by the Protocol of 1978, relating thereto. In case of suspected violations involving
the discharge of harmful substances, an Authority will, upon the request of another Authority, visit in port the
ship suspected of such a violation in order to obtain information and, where appropriate, to take a sample of
any alleged pollutant. In the cases referred to in this article, the requesting Authority should state that the flag
State of the ship has already been notified of the alleged violation.

Section 6 Organization

6.1

6.2
6.3

6.4

6.5

6.6

A Committee composed of a representative of each of the Authorities that are party to the
Memorandum will be established. A representative of the International Maritime Organization, of
the International Labour Organization and of the European Commission will be invited to participate
without vote in the work of the Committee. Representatives of the maritime Authorities of other
Mediterranean Coastal States and, subject to the provisions of Section 8, any other Organization or
Authority which the Committee may deem appropriate, may be accorded the status of observer
without vote.

The Committee will meet once a year and at such other times as it may decide.
The Committee will:
Carry out the specific tasks assigned to it under the Memorandum.

Promote by all means necessary, including seminars for surveyors, the harmonization of
procedures and practices relating to the inspection, rectification, detection and the application of
2.4.

Develop and review guidelines for carrying out inspections under the Memorandum.
Develop and review procedures, including those related to the exchange of information.

Keep under review other matters relating to the operation and the effectiveness of the
Memorandum.

Promote by all means necessary the harmonization of the operation and effectiveness of this
Memorandum with those of similar agreements for other Regions.

Adopt the budget and decide the contributions of every Party to the Memorandum.

Except where provided otherwise (in Section 7), the Committee will take its decisions acting on
simple majority.

A Secretariat provided by the Maritime Authority of Egypt will be set up and will have its office in
Alexandria-Egypt.

The Secretariat, acting under the guidance of the Committee and within the limits of the resources
made available to it, will:
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*  Prepare meetings, circulate papers and provide such assistance as may be required to enable the
Committee to carry out its functions.

*  Facilitate the exchange of information, carry out the procedures outlined in Annex 4 and prepare
reports as may be necessary for the purposes of the Memorandum.

* Carry out such other work as may be necessary to ensure the effective operation of the
Memorandum and to revise the Memorandum periodically in 5 years duration.

6.7 A Secretariat Head Quarter Agreement must be established between the Med. MoU represented by
its Chairman & the Government of Egypt.

Section 7 Amendments

7.1 Any Authority, which has accepted the Memorandum, may propose amendments to the
Memorandum.

7.2 In the case of proposed amendments to sections of the Memorandum the following procedure will
apply:

(a) The proposed amendment will be submitted through the Secretariat for consideration by the
Committee.

(b) Amendments will be adopted by a two-thirds majority of the representative of the Authorities
present and voting in the Committee.

If so adopted an amendment will be communicated by the Secretariat to the Authorities for
acceptance.

The amendments of paragraph 1 of Section 2 are adopted by a two- thirds majority of the
representatives of the Authorities present and voting which are party to the new Convention
proposed for inclusion as "relevant instrument".

(¢) An amendment will be deemed to have been accepted either at the end of a period of six months
after adoption by the representatives of the Authorities in the Committee or at the end of any
different period determined unanimously by the representatives of the Authorities in the
Committee at the time of adoption, unless within the relevant period an objection is
communicated to the Secretariat by an Authority.

(d) An amendment will take effect 60 days after it has been accepted or at the end of any different
period determined unanimously by the representatives of the Authorities in the Committee.

7.3 In the case of proposed amendments to Annexes of the Memorandum the following procedure will
apply:

(a) the proposed amendment will be submitted through the Secretariat for consideration by the
Authorities.

(b) the amendment will be deemed to have been accepted at the end of a period of three months
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from the date on which it has been communicated by the Secretariat unless an Authority
requests in writing that the amendment should be considered by the Committee. In the latter
case the procedure specified in 7.2 will apply.

(c) the amendment will take effect 60 days after it has been accepted or at the end of any period
determined unanimously by the Authorities.

Section 8 Administrative provisions

8.1

8.2

83

8.4

8.5

8.6

8.7

8.8

8.9

The Memorandum is without prejudice to the rights and obligations under any international
Agreement.

A Maritime Authority of a State, which complies with the criteria specified in Annex 6, may adhere
to the Memorandum by the acceptance of simple majority of the representatives of the Authorities
present and voting in the Committee.

The Memorandum remains open for signature, at the Headquarters of the Secretariat of the
Committee from 11 July 1997 to 23 February 1998. Maritime Authorities meeting the requirements
specified in Annex 6 may become parties of the Memorandum by:

a) Signature without any reservations as to acceptance, or
b) Signature subject to acceptance, followed by acceptance.

Acceptance or accession will be effected by a written communication by the Maritime Authorities to
the Secretariat.

The Secretariat will inform the Maritime Authorities who have signed the Memorandum of any
signature or written communication, or of acceptance or accession and of the date on which such an
event has taken place.

This Memorandum will enter into force for each Authority on the date duly notified to the
Secretariat.

Any Maritime Authority or Organization wishing to participate as an observer will submit in writing
an application to the Committee and will be accepted as an observer subject to the unanimous
consent of the representatives of the Authorities present and voting at the Committee meeting.

Any Authority may withdraw from the Memorandum by providing the Committee with 60 days
notice in writing.

The English, French and Arabic versions are equally authentic. The English text is the official
version of the Memorandum in case of dispute.

Section 9 Training programmes and seminars

The Authorities will endeavour to establish appropriate training programmes and seminars.

Section 10 Financial Mechanism

The costs for running the Secretariat and the Information Centre are financed by:
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- The financial contribution of every party to the Memorandum.
- If possible, gifts and subventions by donor countries or organizations.

Financial contributions to the costs for running the Secretariat and the Information Centre of Parties to the
Memorandum are to be settled, in conformity with the decisions and procedures adopted by the Committee.

Signed at Malta in the English language, this Eleventh day of July of One Thousand Nine Hundred and
Ninety Seven.
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Annex 2

Annex 3

Annex 4

Annex 5

Annex 6

Annex7

Annex 8

Annex 9

Annex 10

Annex 11

ANNEXES TO MEMORANDUM

Port State control procedures

Procedures for investigation under MARPOL 73/78

Facts regarded as "Clear Grounds”

Information system on inspections

Publication of information for PSC

Qualitative criteria for adherence to the Med MoU

Port State control officer criteria and reguirements

Appeal and review procedures

Selection criteria (target factor)

Refusal of Access

List of Certificates to be Verified
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ANNEX 1

PORT STATE CONTROL PROCEDURES

Contents
Section 1 General
1.1 Guidelines to be observed in the inspection of foreign ships.
1.2 Principles governing rectification of deficiencies or detention of a ship.
13 Application of the clause of "no more favourable treatment”.
1.4 More Detailed Inspection
Section 2 Minimum manning standards and certification

21 Introduction

2.2 Manning control
23 Certification control
24 Detention

Section 3 Maritime Labour Convention, 2006 (MLC 2006) or Merchant Shipping (Minimum
Standards) Convention, 1976 (No. 147) and ILO 147 Protocol, 1966, if applicable

Section 4  Guidelines for surveyors to be observed in the inspection of cargo ships below 500 tons
gross tonnage and ships of traditional Build
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Section 1

1.1

General

Guidelines to be observed in the inspection of foreign ships.

1.1.1 The relevant instruments mentioned in section 2.1 of the Memorandum is as following:

1)
2)
3)
4)

5)

6)

7)

8)
9)
10)

11)

12)

13)
14)

15)

1.1.2

The International Convention on Load Lines, 1966 (LOAD LINES 66);
the Protocol of 1988 relating to the International Convention on Load Lines, 1966 (LL PROT 88);
The International Convention for the Safety of Life at Sea, 1974 (SOLAS 74);

The Protocol of 1988 relating to the International Convention for the Safety of Life at Sea, 1974
(SOLAS PROT 88);

The International Convention for the Prevention of Pollution from Ships, 1973, as modified by
the Protocol of 1978 relating thereto, and as further amended by the Protocol of 1997
(MARPOL);

The International Convention on Standards of Training, Certification and Watch keeping for
Seafarers, 1978 (STCW 78);

The Convention on the International Regulations for Preventing Collisions at Sea, 1972 (COLREG
72);

the International Convention on Tonnage Measurement of Ships, 1969 (TONNAGE 69);
The Maritime Labour Convention, 2006 (MLC 2006);

The Merchant Shipping (Minimum Standards) Convention, 1976 (ILO Convention No. 147) (ILO
147);

Protocol of 1992 to amend the International Convention on Civil Liability for Oil Pollution
Damage, 1969 (CLC PROT 1992);

International Convention on the Control of Harmful Anti Fouling Systems on Ships, 2001 (AFS
2001);

The International Convention on Civil Liability for Bunker Oil Pollution Damage, 2001;

The International Convention for the Control and Management of Ships' Ballast Water and
Sediments (BWM).

The Nairobi International Convention on the Removal of Wrecks (Nairobi WRC 2007).

The guidelines mentioned in section 3.1 of the Memorandum refer to the relevant provisions
of the following:

Procedures for Port State Control, 2011 (IMO resolution A.1052(27));

Principles of Safe Manning (IMO resolution A.1047 (27).

The Provisions of the International Maritime Dangerous Goods Code.

ILO publication " Inspection of Labour Conditions on board Ship: Guidelines for procedure ".
The Procedures lay down in the Annex to the Memorandum.
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1.2

1.3

1.4

Principles governing rectification of deficiencies or detention of a ship.

In taking a decision concerning the rectification of a deficiency or detention of a ship, the PSCO
shall take into consideration the results of the more detailed inspection carried out in accordance
with section 3 of the Memorandum. The PSCO shall exercise his professional judgment in
determining whether to detain the ship until the deficiencies are corrected or to allow it to sail
with certain deficiencies without unreasonable danger to the safety, health, or the environment,
having regard to the particular circumstances of the intended voyage. As regards minimum
manning standards and the provisions of the Maritime Labour Convention, 2006 (MLC 2006) and /
or ILO Convention No.147, special procedures shall be observed set out in sections 3 and 4 of this
Annex.

Application of the clause of "no more favourable treatment".

In applying Section 2.4 of the Memorandum, the following shall be observed. Ships entitled to fly
the flag of a State which is not a party to a relevant instrument listed in Section 2 of the
Memorandum and thus not provided with certificates representing prima facie evidence of
satisfactory conditions on board, shall receive a more detailed, or as appropriate, an expanded
inspection. In making such an inspection the PSCO should follow the same guidelines as provided
for ships to which the relevant instruments are applicable.

If the ship or the crew has some alternative form of certification, the Port State Control Officer, in
making this inspection, may take the form and content of this documentation into account. The
conditions of and on such a ship and its equipment and the certification of the crew, its number
and composition shall be compatible with the aims of the provisions of a relevant instrument
otherwise the ship shall be subject to such restrictions as are necessary to obtain a comparable
level of safety, otherwise the ship must be subject to such restrictions as are necessary to obtain a
comparable level of safety and protection of the marine environment.

More Detailed Inspection

In so far as there are clear grounds for a more detailed inspection relating to the provisions of the
SOLAS Convention, the Protocol thereto, the Load Lines Convention, Convention on Collision
Regulations and MARPOL 73/78, the PSCO when carrying out this inspection shall take into
account the considerations given in the guidelines for "Preparation and Type of a PSC Inspection”,
the provisions of the International Maritime Dangerous goods Code in its latest edition, and the
Provisions of Section 3 of this Annex with regard to living and working conditions on board ships.

Section 2 Minimum manning standards and certification

21

Introduction

The guiding principle for port State inspection of the manning of a foreign ship should be to
establish conformity with the flag State's safe manning requirements. Where this is in doubt the
flag State should be consulted. Such safe manning requirements stem from:

e The International Convention for the Safety of life at Sea (SOLAS) 1974.
e The Merchant Shipping (Minimum Standards) Convention 1976 (ILO Convention 147) which inter
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2.2

2.2.1

2.2.2

2.2.3

2.3

2.3.1

2.3.2

alia refers to the ILO Convention No. 53 Articles 3 and 4;
e The Maritime Labour Convention 2006 (MLC 2006);
e The International Convention on Standards of Training, Certification and Watch keeping for
Seafarers (STCW) 1978;
e The Principles of Safe Manning (IMO resolution A. 1047(27) as amended
Detention as port State action shall only be taken on the grounds laid down in the relevant
instruments and used in conjunction with advice from the flag State. Where such response is not
readily forthcoming, and the extent of the manning deficiency is such as to render the ship clearly
unsafe for the intended voyage or service, detention may be the only resort.

Manning control

If a ship is manned in accordance with a safe manning document or equivalent document issued
by the flag State, the PSCO should accept that the ship is safely manned unless the document has
clearly been issued without regard to the principles contained in the relevant instruments and in
the IMO Guidelines for the Application of Principles of Safe Manning. In this last case, the PSCO
should act according to the procedures defined in paragraph 2.2.3

If the actual crew number or composition does not confirm to the manning document, the port
State should request the flag State for advice whether or not the ship can sail with the actual
number of crew and its composition. Such request should be made as quickly as possible.

The reply if any, from the flag State should be confirmed writing. If the actual crew number and
composition is not brought into accordance with the safe manning document or the flag State
does not advise that the ship could sail, the ship may be considered for detention after the criteria
set out in paragraph 2.4 of this Annex have been taken into proper account.

If the ship does not carry a safe manning document or equivalent, the port State should request
the flag State to specify the required number of crew and its composition and to issue a document
as quickly as possible. In case the actual number or composition of the crew does not confirm to
the specifications received from the flag State, the procedure as contained in paragraph 2.2.2
applies. If the flag State does not respond to the request this will be considered as a clear ground
for a more detailed inspection to ensure that the number and composition of the crew is in
accordance with the principles laid down in Paragraph2.1. The ship shall only be allowed to
proceed if it is safe to do so, taking into account the criteria for detention under paragraph 2.4. In
any such case the minimum standards to be applied shall be no more stringent than those applied
to ships flying the flag of the port State. The lack of a safe manning document shall be reported as
a deficiency.

Certification control

General certification control upon ships should be carried out in accordance with the procedures
stipulated in Article X and in Regulation 1/4 of the STCW Convention.

Certification control upon ships engaged in the carriage of liguid hazardous cargo in bulk should be
more stringent. The PSCO should satisfy himself that the officers responsible for cargo handling
and operation possess documentary evidence of having had the appropriate training and
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2.4

experience.

No exemption from the carriage of such documentary evidence should be accepted. Where a
deficiency is found the master should be informed and the deficiency rectified. With regard to
appropriate training, reference is made to chapter V of the STCW Convention, to resolutions 10,
11 and 12 adopted by the International Conference on Training and Certification of Seafarers 1978
and to the relevant sections of the International Code for the Construction and Equipment of ships
Carrying Dangerous Chemicals in Bulk and the International Code for the Construction and
Equipment of Ships carrying Liquefied Gases in Bulk.

Detention

Before detaining a ship under paragraph 2.2 or 2.3 of this Annex, the following circumstances
should be considered:

Length and nature of the intended voyage or service;

Whether or not the deficiency poses a danger to ship, persons on board or the environment;
Whether or not appropriate rest periods of the crew can be observed;

Size and type of ship and equipment provided;

Nature of cargo

YL g O B S

The absence of a Deck or Engineer Officer required to be certificated should not be grounds for
detention where the absence is in accordance with any exceptional provisions approved by the
flag State.

Section 3 Maritime Labour Convention, 2006 (MLC 2006) or Merchant Shipping (Minimum

3.1

3.1.1

3.2

3.2.1

Standards) Convention, 1976 (No. 147) and ILO 147 Protocol, 1966, if applicable
Maritime Labour Convention, 2006 (MLC, 2006), if applicable

In the exercise of control of the MLC, 2006, the Port State Control Officer (PSCO) will decide, on
the basis of the clear grounds listed in Annex 3 and his/her professional judgment, whether the
ship will receive a more detailed inspection. All complaints not manifestly unfounded regarding
conditions on board will be investigated thoroughly and action taken as deemed necessary. The
PSCO will also use his/her professional judgment to determine whether the conditions on board
give rise to a hazard to the safety or health of the seafarers which necessitates the rectification of
conditions and may, if necessary, detain the ship until appropriate corrective action is taken.
Reporting procedures for detentions are provided in Annex 5.

[Implementation of PSC procedures which are specific to MLC, 2006, may be found in the ILO
publication “Guidelines for port State control officers carrying out inspections under the Maritime
Labour Convention 2006”]

Merchant Shipping (Minimum Standards) Convention, 1976 (ILO147) and ILO 147 Protocol, 1996, if
applicable

Inspections on board ships under the Merchant Shipping (Minimum Standards) Convention 1976
(ILO Convention No. 147) shall relate to:
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3.3

3.4

3.5

3.6

1.  the Minimum Age Convention, 1973 (No.138); or the Minimum Age (Sea) Convention
(Revised, 1936 (N0.58), or the Minimum Age (Sea) Convention, 1920 (No.7);

the Medical Examination (Seafarers) Convention, 1946 (No.73);

the Prevention of Accidents (Seafarers) Convention, 1970 (No.134) (Articles 4 and 7);

the Accommaodation of Crews Convention (Revised), 1949 (No.92);

the Food and Catering (Ship's Crews) Convention, 1946 (No.68) (Articles 5);

6. the Officers' Competency Certificates Convention, 1936 (No.53) (Articles 3 and 4).

Inspection regarding certificates of competency is dealt with in Section 2 of this Annex. In the
exercise of control of the conventions listed above in (.1) to (.6) the Port State Control Officer
PSCO will decide on the basis of the clear grounds listed in Annex 3, and in the light of his/hers
general impression of the ship, will have to use his / hers professional judgment to decide whether
the ship shall receive a more detailed inspection. All complaints regarding conditions on board
should be investigated thoroughly and action taken as deemed necessary by the circumstances.
He shall also use his professional judgment to determine whether the conditions on board give
rise to a hazard to the safety or health of the crew which necessitates the rectification of
conditions, and may if necessary detain the ship until appropriate corrective action is taken.
Reporting procedures for detentions are provided in Annex 5.

S

In so far as there are clear grounds for a more detailed inspection relating to the provisions of ILO
Convention No.147, the Port State Control Officer when carrying out an inspection shall take into
account the previous paragraph in this section and the considerations given in the ILO publication
"Inspection of Labour Conditions on board Ship: guidelines for procedure™.

The Conventions relevant in the framework of the provisions of paragraph 3.5 are:

1. the Seamen’s Articles of Agreement Convention, 1926 (No.22);

2. the Repatriation of Seamen Convention 1926 (No.23);

3. the Ship owners' Liability (Sick and Injured Seamen) Convention, 1936 (No.55); or the
Sickness Insurance (Sea) Convention, 1936 (No.56); or the Medical Care and Sickness
Benefits Convention, 1968 (No.130);

4.  the Freedom of Association and protection of the Right to Organize Convention, 1948

(No.87);

the Right to Organize and Collective Bargaining Convention, 1949 (No.98);

the Seafarers’ Identity Documents Convention, 1958 (no. 108);

the Workers’ Representatives Convention, 1971 (no. 135);

the Health Protection and Medical Care (Seafarers) Convention, 1987 (no. 164);

the Repatriation of Seafarers Convention (Revised), 1987, (no. 166).

D" 00! il O U

If the Port State Control Officer receives a complaint to the effect that the standards laid down in
the Conventions listed in paragraph 3.4 are not met, the matter should be reported to the nearest
maritime, consular or diplomatic representation of the flag State for further action. If deemed
necessary, the appropriate Authority may prepare a report to the flag State, if possible with
evidence, with a copy to the ILO.

Those parts of the ILO publication "Inspection of Labour Conditions on board Ship: Guidelines for
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procedure” which deal with:

Control procedures for national flag ships;
Vocational training;

Officer’s certificates of competency;
Hours of work and manning;

0 N s

Should not be considered as relevant provisions for the inspection of ships but as information to
Port State Control Officers only.

Section 4 Guidelines for surveyors to be observed in the inspection of cargo ships below 500 tons

4.1

4.1.1

4.1.2

4.1.3

4.2

4.2.1

4.2.2

4.2.3

gross tonnage and ships of traditional build

Mediterranean cargo ships below S00 tons gross tonnage

The following is a guide for the application of section 2.5 of the Memorandum in respect of
Mediterranean cargo ships below 500 tons gross tonnage.

Authorities that have accepted and applied the "Mediterranean Cargo Ship Safety Regulations” on
their vessels may to the extent a relevant instrument is not applicable to a ship below 500 tons
gross tonnage; be guided with said regulations.

Authorities that cannot apply the provisions of 4.1.2 above, to the extent a relevant instrument is
not applicable to a ship below convention size, the Port State Control Officer's task will be to assess
whether the ship is of an acceptable standard in regard to safety, health or the environment. In
making that assessment, the Port State Control Officer will take due account of such factors as the
length and nature of the intended voyage or service, the size and type of the ship, the equipment
provided and the nature of the cargo.

Ships of Traditional build

The following is a guide for the application of Section 2.5 of the Memorandum in respect of
ships of traditional build

To the extent a relevant instrument is not applicable to a ship of traditional build, the PSCO's task
will be to assess whether the ship is of an acceptable standard in regard to safety, health or the
environment. In making that assessment the PSCO shall take due account of such factors as the
length and nature of the intended voyage or service, the size and type of the ship, the equipment
provided and the nature of the cargo.

In the exercise of his functions under paragraph 2.2, the PSCO should be guided by any certificates
and other documents issued by the flag State. The PSCO will, in the light of such certificates and
documents and in his general impression of the ship, use his professional judgment in deciding
whether and in what respects the ship shall receive a more detailed inspection, taking into account
the factors mentioned in paragraph 2.2 when carrying out a more detailed inspection the PSCO
shall, to the extent he deems necessary, pay attention to the items listed in paragraph 2.4. The list
is not considered
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4.2.4  Items of general importance
4.2.4.1 TItems related to the conditions of assignment of load lines:

Weather tight (or watertight as the case may be) integrity of exposed decks;
Hatches and closing appliances;

weather tight closures to openings in superstructures;

freeing arrangements;

side outlets;

ventilators and air pipes;

Moo s o

Stability information.

4.2.4.2 Other items related to the safety of life at sea:

life-saving appliances;
fire-fighting appliances;
General structural conditions (i.e. hull, deck, hatch covers, etc.);

Main machinery and electrical installations;

o= e B

Navigational equipment including radio installations.

4.2.4.3 Ttems related to the prevention of pollution from ships:

6. means for the control of discharge of oil and oily mixtures, e.g., oily water separating or
other equivalent means (tank(s)) for retaining oil, oily mixtures, oil residues;

7. Presence of oil in the engine room bilges.

4.2.5 In the case of deficiencies which are considered to safety, health or the environment the PSCO
shall take such action, which may include detention as may be necessary, having regard to the
factors mentioned in paragraph 2.2, to ensure that the deficiency is rectified or that the ship, if
allowed to proceed to another port, does not present a clear hazard to safety, health or the
environment.
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5.5  Conclusion
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Section 1 Procedures for discharge requirements under Annexes I and II to MARPOL 73/78

1.1

1.2

1.3

Acting upon a report or notification of an alleged violation of the discharge requirements under
Annexes | and Il to MARPOL 73/78, the port State control officer will be guided by the procedures
set out in sections 2 and 3 of this Annex with regard to investigations into alleged contravention of
the discharge provisions of Annex | to MARPOL 73/78 and in sections 4 and 5 of this Annex with
regard to investigations into alleged contravention of the discharge provisions of Annex Il to
MARPOL 73/78.

When exercising control on alleged violations of the discharge requirements under Annexes | and Il
to MARPOL 73/78, the port State control officer will give due regard to the provisions of 4.3.1 and
4.3.2 of IMO Resolution A. 1052(27) as amended and of Appendix 3 of the same Resolution, and to
the instructions of the port State Administration based on these provisions.

In the event that his investigation reveals deficiencies which are clearly hazardous to safety, health
or the environment, the port State control officer will apply the provisions of 3.6.3 of the
Memorandum.

Section 2 Contravention of discharge provisions under Annex I to MARPOL 73/78

2.1

2.2

23

The provisions of sections 2 and 3 of this Annex are intended to identify information which is often
needed by a flag State Administration for the prosecution of such possible violations.

It is recommended that in preparing a port State control report on deficiencies, where
contravention of the discharge requirements is involved, the authorities of the coastal or port State
be guided by the itemized list of possible evidence as shown in section 3 of this Annex. It must be
borne in mind in this connection that:

1.  The report aims to provide the optimal collation of obtainable data; however, even if all the
information cannot be provided, as much information as possible must be submitted;

2. ltis important for all the information included in the report to be supported by facts which,
when considered as a whole, would lead the port or coastal State to believe a contravention
had occurred.

In addition to the port State control report on deficiencies, a report must be completed by a port
or coastal State, on the basis of the itemized list of possible evidence. It is important that these
reports are supplemented by documents such as:

1. A statement by the observer of the pollution. In addition to the information required in 3.1
of this Annex, the statement must include considerations which lead the observer to
conclude that none of any other possible pollution sources is in fact the source;

2.  Statements concerning the sampling procedures both of the slick and on board. These must
include location of and time when samples were taken, identity of person(s) taking the
samples and receipts identifying the persons having custody and receiving transfer of the
samples;
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3. reports of analyses of samples taken of the slick and on board; the reports must include the
results of the analyses, a description of the method employed, reference to or copies of
scientific documentation attesting to the accuracy and validity of the method employed and
names of persons performing the analyses and their experience;

4.  astatement by the port State control officer on board together with the port State control

officer's rank and organization;

statements by persons being questioned;

statements by witnesses;

photographs of the oil slick;

Copies of relevant pages of Oil Record Books, log books, discharge recordings, etc.

RNy

All observations, photographs and documentation must be supported by a signed verification of
their authenticity. All certifications, authentications or verifications shall be executed in accordance
with the laws of the State which prepares them. All statements must be signed and dated by the
person making the statement and, if possible, by a witness to the signing. The names of the
persons signing statements must be printed in legible script above or below the signature.

24 The report referred to in 2.2 and 2.3 of this annex must be sent to the flag State Administration. If
the coastal State observing the pollution and the port State carrying out the investigation on board
are not the same, the State carrying out the latter investigation must also send a copy of its
findings to the State observing the pollution and requesting the investigation.

Section 3 Itemized list of possible evidence on alleged contravention of the discharge provisions of
Annex I to MARPOL 73/78

3.1 Action on sighting oil pollution
3.1.1  Particulars of ship or ships suspected of contravention

Name of ship

Reasons for suspecting the ship

Date and time (UTC) of observation or identification

Position of ship

Flag and port of registry

Type (e.g. tanker, cargo ship, passenger ship, fishing vessel), size (estimated tonnage) and
other descriptive data (e.g. superstructure colour and funnel mark)

7. Draught condition (loaded or in ballast)

8. Approximate course and speed

9. Position of slick in relation to ship (e.g. astern, port, starboard)

10. Part of the ship from which side discharge was seen emanating

11. Whether discharge ceased when ship was observed or contacted by radio

o0 LN b 0 R e

3.1.2  Particulars of slick

1. Date and time (UTC) of observation if different from 3.1.1.3 of this Annex;
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3.1.3

3.14

W

14.
15.
16.

Position of oil slick in longitude and latitude if different from 3.1.1.4 of this Annex;
Approximate distance in nautical miles from the nearest landmark;

Approximate overall dimension of oil slick (length, width and percentage thereof covered by
oil);

Physical description of oil slick (direction and form e.g. continuous, in patches or in
windrows);

Appearance of oil slick (indicate categories);

Category A: Barely visible under most favourable light condition;

Category B: Visible as silvery sheen on water surface;

Category C: First trace of colour may be observed;

Category D: Bright band of colour;

. Category E: Colours begin to turn dull;
. Category F: Colours are much darker;
. Sky conditions (bright sunshine, overcast, etc.), light fall and visibility (kilometres) at the time

of observation;

Sea state;

Direction and speed of surface wind;
Direction and speed of current.

Identification of the observer(s)

Oy Ul W9 =

Name of the observer;

Organization with which observer is affiliated (if any);

Observer's status within the organization;

Observation made from aircraft/ship/shore/otherwise;

Name or identity of ship or aircraft from which the observation was made;

Specific location of ship, aircraft, place on shore or otherwise from which observation was
made;

Activity engaged in by observer when observation was made, for example: patrol, voyage,
flight (en route from .... to ....), etc.

Method of observation and documentation

Yl B =

Visual;

Conventional photographs;

Remote sensing records and/or remote sensing photographs;
Samples taken from slick;

Any other form of observation (specify);

Note: A photograph of the discharge must preferably be in colour. Photographs can provide the
following information: that a material on the sea surface is oil; that the quantity of oil discharged
does constitute a violation of the Convention; that the oil is being, or has been discharged from a
particular ship; and the identity of the ship.

Experience has shown that the aforementioned can be obtained with the following three
photographs:
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3.15

3.2

3.21

3.2.2

3.23

1. details of the slick taken almost vertically down from an altitude of less than 300 metres with
the sun behind the photographer;

2. anoverall view of the ship and “slick” showing oil emanating from a particular ship; and

3. details of the ship for the purposes of identification.

Other information if radio contact can be established

Master informed of pollution
Explanation of master

Ship's last port of call

Ship's next port of call

Name of ship's master and owner
Ship's call sign

O L b U R B

Investigation on board

Inspection of IOPP Certificate

1. Name of ship

2. Distinctive number or letters

3. Port of registry

4.  Type of ship

5. Date and place of issue

6. Date and place of endorsement

Note: If the ship is not issued an IOPP Certificate, as much as possible of the requested information
must be given.

Inspection of supplement to the IOPP Certificate

1. Applicable paragraphs of sections 2, 3, 4, 5 and 6 of the supplement to the IOPP Certificate
{non-oil tankers)

2. Applicable paragraphs of sections 2, 3, 4, 5, 6, 7, 8, 9 and 10 of the supplement to the IOPP
Certificate (oil tankers)

Note: If the ship does not have an IOPP Certificate, a description must be given of the equipment
and arrangements on board, designed to prevent marine pollution.

Inspection of Oil Record Book

1. Sufficient pages of the Oil Record Book - Part | must be copied to cover a period of 30 days
prior to the reported incident

2. Sufficient pages of the Oil Record Book - Part Il (if on board) must be copied to cover a full
loading/unloading/ballasting and tank cleaning cycle of the ship. A copy of the tank diagram
must also be taken.
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3.24

3.25

3.26

3.2.7

Inspection of log book

Last port, date of departure, draught forward and aft

Current port, date of arrival, draught forward and aft

Ship's position at or near the time the incident was reported

Spot check if positions mentioned in the log book agree with positions noted in the Oil Record
Book.
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Inspection of other documentation on board

Other documentation relevant for evidence (if necessary make copies) such as:
1. recent ullage sheets;
2. records of monitoring and control equipment.

Inspection of ship

Ship's equipment in accordance with the supplement of the IOPP Certificate;

Samples taken. State location on board;

Traces of oil in vicinity of overboard discharge outlets;

Condition of engine room and contents of bilges;

Condition of oily water separator, filtering equipment and alarm, stopping or monitoring
arrangements;

Contents of sludge and/or holding tanks;

Sources of considerable leakage;

8. On oil tankers the following additional evidence may be pertinent:

a. Oil on surface of segregated or dedicated clean ballast

b. Condition of pump-room bilges

c¢. Condition of crude oil washing system

d. Condition of inert gas system
e
f.
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. Condition of monitoring and control system
Slop tank contents (estimate quantity of water and of oil)

Statements of persons concerned

If Part | of the Oil Record Book has not been properly completed, information on the following

guestions may be pertinent:

1. Was there a discharge (accidental or intentional) at the time indicated on the incident report?

2. Is the bilge discharge controlled automatically?

3. If so, at what time was this system last put into operation and at what time was this system last
put on manual mode?

4. If not, what were date and time of the last bilge discharge?

What was the date of the last disposal of residue and how was disposal effected?

6. Is it usual to effect discharge of bilge water directly to the sea, or to store bilge water firstin a
collecting tank? Identify the collecting tank

7. Have oil fuel tanks recently been used as ballast tanks?
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