VENDIM
[bookmark: _GoBack]Nr. 252, datë 11.12.2018

MBI MIRATIMIN E PROPOZIMIT TË TË GJITHA OST-ve TË EVROPËS KONTINENTALE DHE NORDIKE PËR HIPOTEZAT DHE NJË METODOLOGJI TË ANALIZËS SË KOSTO-PËRFITIMIT NË PËRPUTHJE ME NENIN 156 (11) TË RREGULLORES SË KOMISIONIT TË BASHKIMIT EVROPIAN (BE) 2017 /1485, TË DATËS 2 GUSHT 2017, QË PËRCAKTON NJË UDHËZUES MBI OPERIMIN E SISTEMIT TË TRANSMETIMIT TË ENERGJISË ELEKTRIKE

Në mbështetje të neneve 7, 16, 56 dhe nenit 63 të ligjit nr. 43/2015, “Për sektorin e energjisë elektrike”, i ndryshuar, nenit 156(11) të Rregullores së Komisionit të Bashkimit Evropian (BE) 2017 /1485, të datës 2 gusht 2017; nenit 167 të “Kodit të Transmetimit”, miratuar me vendimin e Bordit të ERE-s nr. 186, datë 10.11.2017, dhe nenit 26 të “Rregullave të organizimit, funksionimit dhe procedurave të ERE-s”, miratuar me vendimin e Bordit të ERE-s nr. 96, datë 17.6.2016, Bordi i ERE-s, në mbledhjen e tij të datës 11.12.2018, mbasi shqyrtoi relacionin e drejtorive teknike në lidhje me propozimin e të gjitha OST-ve të Evropës Kontinentale dhe Nordike për hipotezat dhe një metodologji të analizës së kosto-përfitimit në përputhje me nenin 156(11) të Rregullores së Komisionit të Bashkimit Evropian (BE) 2017/1485, të datës 2 gusht 2017, që përcakton një udhëzues mbi operimin e sistemit të transmetimit të energjisë elektrike,
konstatoi se:
- OST sh.a., me shkresën nr. 5020 prot., datë 9.7.2018, protokolluar në ERE me nr. 500 prot., datë 10.7.2018, ka kërkuar miratimin e “Propozimit të të gjitha OST-ve të Evropës Kontinentale dhe Nordike, për hipotezat dhe një Metodologji të Analizës Kosto-Përfitim,  në përputhje me nenin 156(11) të Rregullores së Komisionit të Bashkimit Evropian (BE) 2017/1485, të datës 2 gusht 2017, që përcakton një udhëzues mbi operimin e sistemit të transmetimit të energjisë elektrike.
- Kjo kërkesë vjen si detyrim i zbatimit të parashikimeve të vendeve pjesëmarrëse në ENTSO-E, ku Operatori i Sistemit të Transmetimit të energjisë elektrike (OST sh.a.) është anëtar me të drejta të plota.
- Ky dokument është një propozim i përbashkët i hartuar nga të gjithë Operatorët e Sistemit të Transmetimit të Evropës Kontinentale dhe zonave sinkrone nordike, në lidhje me përcaktimin e hipotezave dhe një metodologjie për një analizë të kosto përfitimit që do të kryhet, me qëllim që të vlerësohet periudha kohore e kërkuar për rezervat e mbajtjes së frekuencës, njësitë ose grupet ofruese me rezervuare të kufizuara të energjisë për të mbetur të disponueshëm gjatë gjendjes së alarmit, në përputhje me nenin 156 (11) të Rregullores së Komisionit të Bashkimit Evropian (BE) 2017/1485, të datës 2 gusht 2017, që përcakton një udhëzues mbi operimin e sistemit të transmetimit të energjisë elektrike.
- Metodologjia e analizës së kosto-përfitim (CBA-së)  për propozimin e Rezervës së Mbajtjes të Frekuencës (FCR), merr në konsideratë parimet dhe qëllimet e përgjithshme të përcaktuara në Rregulloren e udhëzimit për operimin e sistemit, si dhe Rregulloren e komunitetit të energjisë (EC) nr. 714/2009, të Parlamentit Evropian dhe të Këshillit të datës 13.7.2009, mbi kushtet e aksesit në rrjet për shkëmbimet ndërkufitare të energjisë elektrike. 
- Metodologjia e analizës së kosto-përfitim (CBA-së) për propozimin e rezervës së mbajtjes të frekuencës (FCR) kontribuon në ndjekjen e objektivave të përgjithshëm të Rregullores së udhëzuesit për operimin e sistemit për ruajtjen e sigurisë operacionale duke përcaktuar periudhën e duhur kohore për aktivizimin e plotë të FCR-së në gjendjen e alarmit duke marrë parasysh kostot dhe përfitimet e periudhës kohore të përcaktuar, në të mirën e të gjithë pjesëmarrësve të tregut dhe konsumatorëve fundorë të energjisë elektrike.
- Kjo metodologji do të zbatohet për të gjitha OST-të e vendeve anëtare të Bashkimit Evropian, të cilat e përcjellin për miratim tek autoritet rregullatore respektive.
- Me vendimin nr. 171, datë 3.8.2018, Bordi i ERE-s ka vendosur të fillojë procedurën për miratimin e këtij propozimi.
- Me shkresën nr. 55/64 prot., datë 2.11.2018, ERE ka publikuar në median e shkruar njoftimin për vendimin e sipërcituar.
- Me shkresën nr. 500/1 prot., datë 5.11.2018, ERE-s i është drejtuar Ministrisë së Infrastrukturës dhe Energjisë për dhënie mendimi lidhur me propozimin e mësipërm. Me shkresën nr. 13638/1 prot., datë 3.12.2018, MIE është shprehur parimisht dakord për këtë propozim.
Për gjithë sa më sipër Bordi i ERE-s 

VENDOSI:

1. Të miratojë propozimin e të gjitha OST-ve të Evropës Kontinentale dhe Nordike për hipotezat dhe një Metodologji të Analizës së Kosto-Përfitimit, në përputhje me nenin 156 (11) të Rregullores së Komisionit të Bashkimit Evropian (BE) 2017/1485, të datës 2 gusht 2017, që përcakton një udhëzues mbi operimin e sistemit të transmetimit të energjisë elektrike. (Bashkëlidhur këtij vendimi.)
2. Versioni në gjuhën e origjinës (anglisht) ka përparësi në rast mosdakordësie nga palët në interpretim të versionit shqip.
3. Drejtoria Juridike dhe e Mbrojtjes së Konsumatorit të njoftojë palët e interesit për vendimin e Bordit të ERE-s.
Ky vendim hyn në fuqi menjëherë. 
Ky vendim botohet në Fletoren Zyrtare.  
Ky vendim mund të ankimohet në Gjykatën Administrative Tiranë, brenda 30 ditëve kalendarike nga  botimi në Fletoren Zyrtare.

KRYETARI
Petrit Ahmeti
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a. Devijimi deterministik i frekuencés
OST-té do té& marrin né konsideraté disbalancat e nxitura nga tregu, do t€ analizojné
trendin historik té frekuencés té secilés zoné sinkrone gjaté disa viteve dhe pastaj do té
pércaktojné statistikisht tendencat dhe amplitudat tipike té kétyre devijimeve té
frekuencés, né ményré qé ato té pérdoren si informacion hyrés né Modelin Probabilistik
Simulues.

b. Devijimi i géndrueshém i frekuencés.

OST-t€ do té marrin né konsideraté parasysh devijimet e géndrueshme té
frekuencés.

Ata do té analizojné trendin historik t& frekuencés né ményré qé té karakterizojné
fenomenin nga piképamja statistikore. Analiza do t& pércaktojé:

¢ numrin e ndodhjes sé kétyre ngjarjeve;

o kohézgjatjen tipike;

o trendin e devijimit pérfagésues té frekuencés

¢ koha tipike e ndodhjes, nése nxirret né pah nga analiza statistikore.
c. Ndérprerjet e elementeve té réndésishém té rrjetit.

QST-té do té pércaktojné njé listé té té gjithé elementéve té rrjetit, ndérprerjet e té
ciléve ¢ojné né humbje té réndésishme té ngarkesés ose gjenerimit dhe praktikisht né
aktivizimin pérkatés té FCR-sé.

Ndérprerjet e elementéve té rrjetit gé do té shqyrtohen jané sé paku: avarité né
centralet gjeneruese, difektet né zbarat kritke dhe c¢kycjet e nénstacionit té
réndésishém. Pér ¢do ndérprerje duhet té pércaktohet probabiliteti i humbjes.

1 gjithé informacioni né dispozicion né lidhje me ndérvarésiné midis tre burimeve té shqetésimeve
té frekuencés té listuara mé sipér do té& merret parasysh né ményré qé té& shmanget numérimi i
dyfishté i fenomenit.

3. Modeli Probabilistik i Simulimit do té pérdoret pér té llogaritur FCR e kérkuar pér secilin
skenar té pérshkruar né Nenin 6. Prandaj, pér modelin edhe variablat e méposhtém
paragesin informacion hyrés:

a. Periudha Kohore;
b. LER Share;

Pér mé tepér, edhe mesatarja e FAT e zonés sinkrone éshté njé parametér hyrés pér
Modelin Probabilistik té Simulimit.

4. Modeli probabilistik simulues llogarit FCR-né e kérkuar duke pérdorur metodén iterative. Né
¢do pérséritje, Modeli Propabilistik i Simulimit pérdor njé Proges Simulimi t& Monte Carlo-s
né ményré gé té verifikojé nése frekuenca e gjendjes sé géndrueshme éshté brenda
devijimit maksimal té frekuencés sé gjendjes sé& géndrueshme. Nése kushti nuk éshté
plotésuar, Modeli Probabilistik i Simulimit rrit gradualisht FCR-né dhe llogarit pérséritjen e
radhés. Iteracionet ndalojné sapo té plotésohet kushti. Pérfundimi i nxjerré nga Modeli
Probabilistik i Simulimit &shté FCR-ja e duhur pér té ruajtur frekuencén e gjendjes sé
géndrueshme brenda devijimit maksimal té frekuencés sé gjendjes sé géndrueshme.

5. Progesi i simulimit t& Monte Karlos duhet té jeté né gjendje té simulojé disa vite té kushteve
té operimit té secilés zoné sinkrone me ané té térhegjeve té rastésishme té devijimeve té
géndrueshme té frekuencés dhe ndérprerjeve té elementeve té réndésishém té rrjetit. Ai
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burimeve té& mundshme té luhatjeve té frekuencés. Megenése progesi i simulimit i Monte
Carlos punon né fushén e kohés, kjo metodé kérkon simulimin e njé periudhe té gjaté té
operimit té sistemit. Periudha e operimit gé do té simulohet duhet té jeté e gjaté
mjaftueshém sa pér té gjeneruar rezultate statistikisht té réndésishme.

6. Progesi i simulimit i Monte Carlo-s pérdor njé model dinamik simulimi pér té llogaritur
devijimin e frekuencés. Modeli i simulimit dinamik pérdor si informacion hyrés burimet e
shqgetésimeve té frekuencés, té gjeneruara rastésisht nga progesi i Simulimit i Monte Carlo-
s dhe simulon FCP-né dhe FRP-né.

7. Modeli Dinamik i Simulimit do té jeté né gjendje té simulojé shterimin e LER dhe efektet e
tij né devijimin e frekuencés, duke marré parasysh LER Share dhe Periudhén Kohore.

Neni 5. Vlerésimi i kostos sé FCR

1. Sasia minimale e FCR-sé sé nevojshme pér té ruajtur gjendjen e géndrueshme té frekuencés
brenda devijimit maksimal té frekuencés né gjendje né géndrueshme té llogaritur nga Modeli
Probabilistik Simulues, do té pérdoret pér té vierésuar koston e FCR-sé lidhur me secilin
skenar me ané té njé kurbe té kostos sé FCR-sé,

2. Té gjitha OST-té e zonés sinkrone do té pércaktojné kurbén e kostos sé FCR-sé, e cila pérfshin
ofruesit e LER dhe Jo-LER té FCR-sé.

3. Kostoja e FCR-sé pér ofruesit Jo-LER té FCR-sé do té llogaritet té& paktén duke krahasuar
koston marxhinale té ofruesit t&€ FCR-sé me ¢mimin marxhinal té energjisé s€ zonés ofertuese.
Krahasimi lejon té vlerésohet kostoja e kapacitetit rezervé pér sigurimin e FCR-sé,

4. Kostoja e FCR-sé pér LER-ét e ardhshém té instaluar do té llogaritet duke marré né
konsideraté: investimet, OPEX dhe kostot oportune (nése ka). Kéto kontribute duhet té
merren parasysh vetém nése jané té géndrueshme né ményré qé té kualifikohen pér ofrimin
e FCR.

5. Kostot e FCR-sé pér LER-Et tashmé ekzistuese do té llogariten duke marré né konsideraté:
OPEX dhe kostot oportune (nése ka). Kéto kontribute do té konsiderohen vetém nése ato
jané té géndrueshme me géllim qé té klasifikohen pér sigurimin e FCR.

6. Ndikimi mbi koston e FCR-sé& pér LER-&t duhet té merret né konsideraté pér shkak té
kérkesave té ndryshueshme té rezervuaréve té energjisé (t& lidhura me Periudhén Kohore).

Neni 6. Skenarét e simulimit

1. Analizat dhe progeset e pérshkruara né nenin 4 dhe 5 duhet té realizohen duke marré né
konsideraté skenaré té ndryshém dhe gé lejojné té llogaritet dimensionimi i FCR-sé dhe kosto
e FCR-sé duke marré parasysh supozime té ndryshme. Skenarét kané si qéllim té adresojné
pasigurité dhe té vlerésojné impaktin e hipotezave té ndryshme té cilat mund té ndikojné
rezultatet e Analizes sé Kosto-Pérfitimit.
2. Grupi i skenaréve duhet té€ pérfshijé té gjitha kombinimet e supozimeve né vijim:
a. Periudha kohore. N& ményré gé té vlerésohet zgjidhja mé e miré né termat té
periudhés minimale té aktivizimit, e cila nuk éshté mé e madhe se 30 min. ose mé
e vogél sé 15 min., intervali i zgjidhjeve té mundshme duhet té hulumtohet duke
miratuar njé pérafrim t& mundshém. Kur zbatohet metodologjia e CBA-sé pér
Propozimin e FCR, OST-té duhet té konsiderojné njé pérafrim prej 5 minutash,
késhtu gé duhet té vlerésohen rezultatet duke konsideruar periudhén kohore prej
prej ™5, 20, 25 dhe 30 minuta
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b. LER Share. Pjesa gé ndahet e LER-ve mund té ndikohet nga efikasiteti i kostos sé
LER, por gjithashtu edhe nga faktoré té tjeré, si prezenca e prokurimit té& FCR-sé me
bazé tregu ose impaktet e tjera teknike dhe rregullatore té shkarkimit té LER. Pér
kété arsye, do té analizohen LER Share té ndryshme né diapazonin 10-100% me
10% pérafrim.
3. Té gjitha analizat do té kryhen duke marré parasysh zhvillimet e mundshme té ardhshme té
sistemit energjetik dhe rregulloret né terma afat- shkurtér.
4. Pérpunimi i rezultateve té pérfituara nga kryerja e analizave té pérshkruara né nenet 4 dhe 5
né térésiné e skenaréve duhet té lejojé, pérfitimin e dimensionimit té& FCR-sé dhe kostot e FCR-
sé pér ¢do kombinim mes Periudhés Kohore dhe LER Share.

Neni 7. Simulimi i ngjarjeve mé té réndésishme té frekuences reale né
prezencén e LER

1. Crregullimet mé té réndésishme té frekuencés té ndodhura né té kaluarén do té simulohen
duke modeluar praniné e LER-vé dhe duke vlerésuar se si shterimi i energjisé potenciale do té
kishte ndikuar né géndrueshmériné e sistemit.

2. Simulimi i ngjarjeve reale mé té réndésishme té frekuencés, do té kryhet pér ¢do kombinim té
Periudhés Kohore dhe LER Share né pércaktuar Nenin 6 (2a) dhe (2b). Nése njé kombinim i
Periudhés Kohore dhe LER Share pérkeqéson potencialisht siguriné operacionale duke guar né
gjendje black-out, kombinimi do té konsiderohet i papranueshém.

Neni 9. Pércaktimi dhe pérditésimi i Periudhés Kohore

Sipas Nenit 156 (11), 12 muaj pas miratimit t& supozimeve dhe metodologjisé sé paraqitur kétu
nga té gjitha autoritetet rregullatore té rajonit respektiv, OST-té e Evropés Kontinentale dhe
zonave sinkrone Nordike duhet té dorézojné né autoritetet rregullatore pérkatése, rezultatet e
analizés sé tyre té kosto-pérfitimit, duke sugjeruar njé Periudhé Kohore gé nuk duhet té jeté mé
e madhe sé 30 minuta ose mé e vogél sé 15 minuta.

Né ¢do rast, pas ¢do ndryshimi té réndésishém té supozimeve pér analizén e kosto-pérfitimit, pas
hyrjes né fuqi té Periudhés Kohore, té gjitha OST-té e Evropés Kontinentale dhe zonave sinkrone
nordike duhet té paragesin rezultatet e njé analize t& kosto-pérfitim té pérditésuar tek autoritetet
pérkatése rregullatore, duke sugjeruar njé Periudhé& Kohore té pérditésuar e cila nuk duhet té
jeté mé e madhe sé 30 minuta ose mé e vogél sé 15 minuta.

Neni 10. Hipotezat e Analizés sé Kosto-Pérfitimit

1. Modeli Probabilistik i Simulimit i pérshkruar né Nenin 4 (1) (2) (3) (4), progesi i Simulimit i
Monte Karlo-s i p&rshkruar né Nenin 4 (1) (5) (6) dhe Modelin Dinamik Simulues té pérshkruar
né Nenin 4 ) (7) duhet t'i referohet njé zone té téré sinkrone.

2. Modeli Dinamik Simulues do té simulojé FRP-né me njé kontrollues té vetém té FRP-sé pa
kufizime té FRR-sé.

3. Modeli Dinamik Simulues mund té neglizhojé té gjithé progesin Ndérkufitar t& Kontrollit
Ngarkesé-Frekuencé.

4. Modeli Dinamik Simulues mund t& neglizhojé inerciné e sistemit dhe dinamikén e vendosjes sé
FCP-sé.
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5. Modeli Dinamik Simulues do té simulojé sé paku dinamikén e vendosjes sé FRP, pjerrésiné e
sistemit(system droop) dhe veté-rregullimin e ngarkesés.

6. Nése tejkalimi i vazhdueshém i diapazonit té frekuencés standarte con né nxitjen e njé gjendje
alarmi, energjia e aktivizuar dhe energjia e mbetur né rezervuar llogaritet nga tejkalimi i paré
i kufijve standarte té frekuencés.

7. Né disponueshmériné e ploté té rezervuarit, niveli i energjisé do té konsiderohet i barabarté
me gjysmén e kapacitetit té energjisé sé rezervuarit Ekuivalent.

Neni 11. Shtojca

Dokumenti i shtojcés ka pér géllim t'u ofrojé paléve té interesuara informacionin, shpjegimin dhe
hollésité e métejshme mbi kérkesat e specifikuara né metodologjiné e CBA-sé pér Propozimin e
FCR-sé dhe duhet té lexchet sé€ bashku me metodologjiné CBA-sé pér Propozimin e FCR-sé,

Neni 12, Publikimi dhe zbatimi i metodologjisé s&é CBA-sé pér Propozimin e FCR-
sé

1. Pasi té gjitha ERE-té e kané miratuar metodologjiné e propozuar té CBA-sé pér Propozimin e
FCR, né pérputhje me nenin 8 té Rregullores sé Udhézimit pér Operimin e Sistemit, cdo OST
e Evropés Kontinentale dhe Nordike do té publikojné metodologjiné e CBA-sé pér Propozimin
e FCR-sé pa vonesa té panevojshme.

2. OST-té e Evropés Kontinentale dhe Nordike duhet té zbatojné metodologjiné e miratuar té
CBA-sé pér Propozimin e FCR-s&, 12 muaj pas miratimit t& saj nga té gjitha autoritetet
rregullatore té zonave sinkrone té Evropés Kontinentale dhe zonave Nordike. Zbatimi do té
béhet duke paraqitur rezultatet e CBA-sé sé kryer nga OST-té e zonave sinkrone té Evropés
Kontinentale dhe Nordike sipas metodologjisé s& miratuar CBA-sé pér Propozimin e FCR tek
autoritetet pérkatése rregullatore dhe duke sugjeruar njé periudhé kohore pér ofruesit e FCR
me Rezervuaré té Kufizuar té Energjisé gjaté sé cilés ata duhet té jené né gjendje té aktivizojné
plotésisht FCR né vazhdimési né gjendje alarmi , ku kjo periudhé kohore nuk duhet té jeté me
e madhe sé 30 min ose mé e vogél sé 15 minuta.

Neni 13. Gjuha

Gjuha referente pér kété metodologji t& CBA-sé mbi Propozimin e FCR duhet té jeté Anglisht. Pér
shmangien e dyshimit, atje ku OST-té duhet té pérkthejné kété metodologji té CBA-sé pér
Propozimin e FCR-sé né gjuhén(t) e tyre kombétare, né rast té€ mospérputhjeve mes versionit né
gjuhén angleze té botuar nga OST-té né pajtim me Nenin 8 (1) té Rregullores sé Udhézimit pér
Operimin e Sistemit dhe ¢do versioni né njé gjuhé tjetér, OST-t€ pérkatése né pérputhje me
legjislacionin  kombétar duhet ti ofrojé autoriteteve pérkatése kombétare rregullatore njé
pérkthim té pérditésuar t& metodologjisé sé CBA-sé pér Propozimin e FCR-sé.
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All Continental Europe and Nordic TSOs, taking into account the following,

“)

)

O

&)

3)

‘Whereas

This document is a common proposal jointly developed by all Transmission System Operators of the
Continental Europe and the Nordic synchronous areas (hereafter referred to as the “TSOs”) regarding
the determination of assumptions and a methodology for a Cost Benefit Analysis (hereafter referred
to as “CBA”) to be conducted, in order to assess the time period required for frequency containment
reserves (hereafter referred to as “FCR”) providing units or groups (hereafter referred to as “FCR
providers™) with limited energy reservoirs to remain available during alert state, in accordance with
Article 156(11) of Commission Regulation (EU) 2017/1485 of 2 August 2017 establishing a
guideline on electricity transmission system operation (hereafter referred to as “System Operation
Guideline Regulation™). This proposal is hereafter referred to as “CBA methodology for FCR
Proposal”.

The CBA methodology for FCR Proposal takes into account the general principles and goals set in
the System Operation Guideline Regulation as well as Regulation (EC) No 714/2009 of the European
Parliament and of the Council of 13 July 2009 on conditions for access to the network for cross-
border exchanges in electricity (hereafter referred to as “Regulation (EC) No 714/2009”). The goal
of the System Operation Guideline Regulation is safeguarding operational security, frequency quality
and the efficient use of the interconnected system and resources. It sets for this purpose requirements
to FCR providers ensuring that their FCR providing units or groups with limited energy reservoirs
are able to fully activate FCR continuously in alert state for a minimum time period to be defined
pursuant to Article 156 (10) and (11) of the System Operation Guideline Regulation.

Article 156(9) of the System Operation Guideline Regulation provides that, in case no time period
has been determined pursuant to Article 156 (10) and (11) of the System Operation Guideline
Regulation, each FCR provider shall ensure that its FCR providing units or groups with limited
energy reservoirs are able to fully activate FCR continuously for at least 15 minutes or, in case of
frequency deviations that are smaller than a frequency deviation requiring full FCR activation, for an
equivalent length of time, or for a period defined by each TSO, which shall not be greater than 30 or
smaller than 15 minutes. Furthermore, it provides that, if a time period has been determined pursuant
to Article 156(10) and (11) of the System Operation Guideline Regulation, cach FCR provider shall
ensure that its FCR providing units or groups with limited energy reservoirs shall be able to fully
activate FCR continuously in alert state for that time period assessed.

Article 156(10) of the System Operation Guideline Regulation requires all Continental Europe and
Nordic TSOs to develop a proposal concerning the minimum activation period to be ensured by FCR
providers, and specifies that the period determined shall not be greater than 30 or smaller than 15
minutes. Such proposal shall take full account of the results of the CBA conducted pursuant to Article
156(11) of the System Operation Guideline Regulation.

Article 156(11) of the System Operation Guideline Regulation requires the TSOs of the Continental
Europe and Nordic synchronous areas to propose assumptions and methodology for a CBA to be
conducted, in order to assess the time period required for FCR providing units or groups with limited
energy reservoirs to remain available during alert state.

The CBA shall take into account at least:
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(a) experiences gathered with different timeframes and shares of emerging technologies in
different LFC blocks;

(b) the impact of a defined time period on the total cost of FCR reserves in the synchronous area;

(c) the impact of a defined time period on system stability risks, in particular through prolonged
or repeated frequency events;

(d) the impact on system stability risks and total cost of FCR in case of increasing total volume
of FCR;

(e) the impact of technological developments on costs of availability periods for FCR from its
FCR providing units or groups with limited energy reservoirs.

This CBA methodology for FCR Proposal is exclusively related to FCR providing units or group
with limited energy reservoirs.

According to Article 6(6) of the System Operation Guideline Regulation, the expected impact of the
CBA methodology for FCR Proposal on the objectives of the System Operation Guideline Regulation
(as listed in Article 4(1) of the System Operation Guideline Regulation) has to be described. The
proposed CBA methodology for FCR Proposal generally contributes to the achievement of the
objectives of Article 4(1) of the System Operation Guideline Regulation. Specifically, the CBA
methodology for FCR Proposal provides the TSOs of the CE and Nordic synchronous areas with a
methodology to assess and develop a proposal concerning the minimum activation period to be
ensured by FCR providers. The determination of a minimum activation period to be ensured by FCR
providers during alert state contributes to the determination of common operational security
requirements and principles as set in the Article 4 (1) (a) of System Operation Guideline Regulation.
It furthermore contributes to ensuring the conditions for maintaining operational security throughout
the Union as set in Article 4 (1) (d) of System Operation Guideline Regulation. Finally it contributes
to the efficient operation and development of the electricity transmission system and electricity sector
in the Union as set in Article 4 (1) (h) of System Operation Guideline Regulation. The CBA
methodology for FCR Proposal does not impact on the other objectives listed in Article 4(1) of the
System Operation Guideline Regulation.

In conclusion, the CBA methodology for FCR Proposal contributes to pursue the general objectives
of the System Operation Guideline Regulation of safeguarding operational security by defining the
proper time period for the full FCR activation in the alert state taking into account costs and benefits
of the defined time period, to the benefit of all market participants and electricity end consumers.

SUBMIT THE FOLLOWING CBA METHODOLOGY FOR FCR PROPOSAL TO ALL REGULATORY
AUTHORITIES OF THE CE AND NORDIC SYNCHRONOUS AREA:

Article 1
Subject matter and scope

The CBA assumptions and methodology as determined in this CBA methodology for FCR Proposal shall be
considered as the common proposal of all Continental Europe and Nordic TSOs in accordance with Article
156(11) of the System Operation Guideline Regulation and shall form the basis on which the TSOs of the CE
and Nordic synchronous areas shall assess the minimum activation period to be ensured by FCR providers in
accordance with Article 156(10) of the System Operation Guideline Regulation.
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Article 2
Definitions and interpretation

1. For the purposes of the CBA methodology for FCR Proposal, terms used in this document shall have the
meaning of the definitions included in Article 3 of the System Operation Guideline Regulation, of
Regulation (EC) 714/2009, Directive 2009/72/EC and Regulation (EU) 543/2013.

2. In addition, in this CBA methodology for FCR Proposal, unless the context requires otherwise, the
following terms shall have the meaning below:

a)
b)
<)

U]

g)

h)

‘LER’ means ‘FCR production units or groups with limited energy reservoirs’;

‘LER Share’ means the ‘share of LER on the total FCR providers",

‘Market induced imbalances’ means the ‘generation-load imbalance caused by the change in
generation set points according to the results of the market scheduling’.

‘System droop’ means ‘the ratio between frequency deviation and steady state power response
provided by FCP’;

‘FCR cost curve” means ‘the set of all the offered quantity of FCR with their corresponding cost’;
‘Time Period’, according to Article 156 (9) of System Operation Guideline Regulation, means ‘the
time for which each FCR provider shall ensure that its FCR providing units or groups with limited
energy reservoirs are able to fully activate FCR continuously, as of triggering the alert state and
during the alert state”;

‘Long lasting frequency deviation’ means an ‘event with an average steady state frequency deviation
larger than the standard frequency range over a period longer than the time to restore frequency’.
‘FAT’ means ‘FRR Full Activation Time’ as defined in Article 3 (101) and (143) of System Operation
Guideline Regulation.

‘Equivalent reservoir energy capacity” means the energy requirement for LER associated to the Time
Period and shall amount to twice the energy provided by the full activation of LER for the Time
Period.

3. In this CBA methodology for FCR Proposal, unless the context requires otherwise:

a)
b)

)

U]

the singular indicates the plural and vice versa;

unless otherwise provided, any reference to an Article means an article of this CBA methodology for
FCR Proposal;

the table of contents and headings are inserted for convenience only and do not affect the
interpretation of this CBA methodology for FCR Proposal; and

any reference to legislation, regulation, directive, order, instrument, code or any other enactment shall
include any modification, extension or re-enactment of it then in force.

Article 3
CBA methodology outcomes and processes

For each combination of LER Share and Time Period (as described in Article 6 (2)(a) and Article 6 (2)(b)),
the outcomes of the CBA methodology are:

a)
b)

the FCR cost (as described in Article 4 and Article 5);
the acceptability of the combination against the most relevant real frequency events (as described in
Article 7).

The FCR cost is calculated by means of two sequential processes.

The first process is a Probabilistic Simulation Model (described in Article 4) whose outcome is the amount
of FCR.
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The second process is an Assessment of cost of FCR (described in Article 5) which associates a cost to the
required amount of FCR calculated by the Probabilistic Simulation Model.

The acceptability of the combination against the most relevant real frequency events is assessed by means
of a dedicated process (described in Article 7).

Article 4
Probabilistic Simulation Model

1. All TSOs of a synchronous area shall develop a Probabilistic Simulation Model able to calculate the
minimum amount of FCR needed to mantain the steady state frequency within maximum steady state
frequency deviation.

2. The following sources of frequency disturbance are inputs of the Probabilistic Simulation Model:
a. Deterministic frequency deviation.
The TSOs shall consider the market induced imbalances, analyse frequency historical trend of each
synchronous area over several years, and then statistically determine the typical trends and
amplitudes of these frequency deviations in order to use them as an input of the Probabilistic
Simulation Model.
b. Long lasting frequency deviation.
The TSOs shall take into account Long lasting frequency deviations.
They shall analyse frequency historical trends in order to characterize the phenomena from a
statistical point of view. The analysis shall determine:
« the number of occurrences of these events;
« the typical duration;
« a representative frequency deviation trend,
« typical time of occurrence, if highlighted by statistical analysis.
¢. Outages of relevant grid elements.
The TSOs shall define a list of all the grid elements whose outages lead to relevant load or
generation losses and indeed to relevant FCR activation.
The grid elements outages to be investigated are at least: generation plants failure, critical busbar
fault and critical substation blackout. For each outage a probability of failure shall be defined.

All the available informations related to the dependence amongst the three sources of frequency
disturbance listed above shall be taken into account in order to avoid the double counting of phenomena.

3. The Probabilistic Simulation Model shall be used to calculate the requested FCR in each scenario
described in Article 6. Therefore also the following variables represent inputs for the model:
a. Time Period,
b. LER Share;
Moreover, also the average FAT of the synchronous area is an input parameter for the Probabilistic
Simulation Model.

4. The Probabilistic Simulation Model calculates the required FCR using an iterative method. At every
iteration the Probabilistic Simulation Model uses a Monte Carlo Simulation Process in order to verify if
the steady state frequency is within maximum steady state frequency deviation. If the condition is not
fulfilled, the Probabilistic Simulation Model increases gradually the FCR and calculates the next
iteration. The iterations stop once the condition is fulfilled. The output of the Probabilistic Simulation
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Model is the FCR required to mantain the steady state frequency within maximum steady state frequency
deviation.

5. The Monte Carlo Simulation Process shall be able to simulate several years of operation conditions of
each synchronous area by means of random draws of long lasting frequency deviations and outages of
relevant grid elements. It has the aim to generate a large number of random combinations of all the
possible sources of frequency disturbance. Since the Monte Carlo Simulation Process works on the time
domain, this approach requires to simulate a long system operation period. The operation period to be
simulated shall be long enough to generate statistically significant results.

6. The Monte Carlo Simulation Process uses a Dynamic Simulation Model in order to calculate the
frequency deviation. The Dynamic Simulation Model uses as input the sources of frequency disturbance
as randomly generated by Monte Carlo Simulation Process and simulates the FCP and FRP.

7. The Dynamic Simulation Model shall be able to simulate the depletion of LER and its effects on the
frequency deviation, taking into account the LER Share and the Time Period.

Article 5
Assessment of cost of FCR

1. The minimum amount of FCR needed to mantain the steady state frequency within maximum steady state
frequency deviation calculated by the Probabilistic Simulation Model shall be used to assess the FCR cost
associated to each scenario by means of a FCR cost curve.

2. All TSOs of a synchronous area shall define a FCR cost curve which includes both LER and non-LER
FCR providers.

The FCR cost for non-LER FCR providers shall be calculated at least by comparing the marginal cost of
the FCR provider with the energy marginal price of the bidding zone. The comparison allows to estimate
the cost of reserving capacity for FCR provision.

The FCR cost for future installed LER shall be calculated considering: investment, OPEX and opportunity
costs (if any). These contributions shall be considered only if they are sustained in order to qualify for
FCR provision.

The FCR cost for already existing LER shall be calculated considering: OPEX and opportunity costs (if
any). These contributions shall be considered only if they are sustained in order to qualify for FCR
provision.

The impact on FCR cost for LER due to variations of energy reservoir requirement (associated to the
Time Period) shall be taken into account.
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Article 6
Simulation scenarios

1. The analyses and processes described in Articles 4 and 5 shall be performed considering different
scenarios and allow to calculate both FCR dimensioning and cost of FCR taking into account different
assumptions. Scenarios are aimed to address uncertainties and assess the impact of different hypotheses
which can affect the results of the CBA.

2. The set of scenarios shall include all the combinations of the following assumptions:

a) Time Period. In order to evaluate the best solution in terms of minimum activation period which
is not greater than 30 or smaller than 15 minutes, the interval of possible solutions have to be
explored adopting an opportune discretization. When implementing the CBA methodology for
FCR Proposal, the TSOs shall consider a discretization of 5 minutes, thus the results considering
Time Periods of 15, 20, 25 and 30 minutes shall be assessed.

b) LER Share. The share of the LER can be affected by the cost effectiveness of LER but also by
other factors, such as the presence of a market based procurement of FCR, or other technical and
regulatory impacts on LER deployment. For this reason, different LER Shares shall be analysed
in the 10-100% range with 10% discretization.

3. All the analyses shall be performed considering potential future developments of the energy system and
regulations in the short term.

4. The elaboration of the results obtained performing the analyses described in Articles 4 and 5 to the whole
set of scenarios shall allow to obtain FCR dimensioning and costs of FCR for each combination of Time
Period and LER Share.

Article 7
Simulation of the most relevant real frequency events in presence of LER

1. The most relevant frequency disturbances occurred in the past shall be simulated modelling the presence
of LER and assessing how the potential energy depletion would have affected the system stability.

2. Simulation of the most relevant real frequency events shall be performed for each combination of Time
Period and LER Share defined in Article 6 (2a) and (2b). If a combination of Time Period and LER Share
worsens operational security potentially leading to a blackout state, the combination shall be considered
not acceptable.

Article 9
Determination and update of Time Period

According to Article 156 (11), by 12 months after approval of the assumptions and methodology contained
herein by all regulatory authorities of the concerned region, the TSOs of the CE and Nordic synchronous
areas shall submit the results of their cost-benefit analysis to the concerned regulatory authorities, suggesting
a Time Period which shall not be greater than 30 or smaller than 15 minutes.

In any case following any significant change of the assumptions for the cost benefit analysis after entering
into force of the Time Period, all TSOs of the CE and Nordic synchronous arcas shall submit the results of
an updated cost-benefit analysis to the concerned regulatory authorities, suggesting an updated Time Period
which shall not be greater than 30 or smaller than 15 minutes.
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Article 10
CBA assumptions

1. The Probabilistic Simulation Model described in Article 4(1)(2)(3)(4), the Monte Carlo Simulation
Process described in Article 4(1)(5)(6) and the Dynamic Simulation Model described in Article 4(6)(7)
shall be referred to a whole synchronous arca.

2. The Dynamic Simulation Model shall simulate the FRP with a single FRP controller without FRR

limitations.

The Dynamic Simulation Model can neglect the entire Cross-Border Load-Frequency Control Process.

The Dynamic Simulation Model can neglect both system inertia and FCP deployment dynamic.

5. The Dynamic Simulation Model shall simulate at least the FRP deployment dynamic, the system droop
and the self-regulation of load.

6. If a continuous exceeding of the standard frequency range leads to the triggering of an alert state, the
activated energy and the residual energy in the reservoir is calculated from the first exceeding of the
standard frequency range limits.

7. At the full availability of the reservoir, the energy level will be considered equal to half of the Equivalent
reservoir energy capacity.

Eale

Article 11
Annex

The annexed document aims to provide interested parties with the background information, explanation and
further details about the requirements specified in the CBA methodology for FCR Proposal and should be
read in conjunction with CBA methodology for FCR Proposal.

Article 12
Publication and implementation of the CBA methodology for FCR Proposal

1. Each Continental Europe and Nordic TSO shall publish the CBA methodology for FCR Proposal without
undue delay after all NRAs have approved the proposed CBA methodology for FCR Proposal, in
accordance with Article 8 of the System Operation Guideline Regulation.

2. The Continental Europe and Nordic TSOs shall have implemented the adopted CBA methodology for
FCR Proposal by 12 months after its approval by all regulatory authorities of the CE and Nordic
synchronous areas. The implementation shall take place by submitting the results of the CBA conducted
by the TSOs of the CE and Nordic synchronous areas according to the adopted CBA methodology for
FCR Proposal to the concerned regulatory authorities suggesting a time period for FCR providers with
limited energy reservoirs during which they shall be able to fully activate FCR continuously in alert state,
whereas this time period shall not be greater than 30 or smaller than 15 minutes.

Article 13
Language

The reference language for this CBA methodology for FCR Proposal shall be English. For the avoidance of
doubt, where TSOs need to translate this CBA methodology for FCR Proposal into their national language(s),
in the event of inconsistencies between the English version published by TSOs in accordance with Article
8(1) of the System Operation Guideline Regulation and any version in another language, the relevant TSOs
shall, in accordance with national legislation, provide the relevant national regulatory authorities with an
updated translation of the CBA methodology for FCR Proposal.
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Té gjitha OST-té e Evropés Kontinentale dhe vendeve Nordike, duke marré parasysh si mé
poshté gé:

1. Ky dokument éshté njé propozim i pérbashkét i hartuar nga té gjithé Operatorét e Sistemit té
Transmetimit té& Evropés Kontinentale dhe zonave sinkrone Nordike (kétej e tutje referuar si
"OST-té") né lidhje me pércaktimin e hipotezave dhe njé metodologjie pér njé Analizé té Kosto-
Pérfitimit (kétej e tutje referuar si "CBA") gé do té kryhet, me qgéllim gé té vlerésohet periudha
kohore e kérkuar pér rezervat e mbajtjes sé frekuencés (kétej e tutje referuar si "FCR") njésité
ose grupet ofruese (kétej e tutje referuar si "ofruesit e FCR-sé€") me Rezervuaré té Kufizuar té
Energjisé pér té mbetur té disponueshem gjaté gjendjes sé alarmit, né pérputhje me nenin 156
(11) té Rregullores sé Komisionit (BE) 2017/1485 té datés 2 gusht 2017, qé pércakton njé
udhézues mbi operimin e sistemit té transmetimit té energjisé elektrike (kétej e tutje referuar
si "Rregullorja e Udh&zuesit pér Operimin e Sistemit"). Kétij propozimi kétej e tutje i referohemi
si "Metodologjia e CBA-sé pér Propozimin e FCR".

2. Metodologjia e CBA-sé pér Propozimin e FCR merr né konsideraté parimet dhe géllimet e
pérgjithshme té pércaktuara né Rregulloren e Udhézimit pér Operimin e Sistemit si dhe
Rregulloren (EC) Nr 714/2009 té Parlamentit Evropian dhe t& Késhillit té€ datés 13 korrik 2009
mbi kushtet e aksesit né rrjet pér shkémbimet ndérkufitare té energjisé elektrike (kétej e tutje
referuar si "Rregullorja KE, Nr 714/2009"). Qéllimi i Rregullores sé Udhé&zuesit pér Operimin e
Sistemit éshté ruajtja e sigurisé operacionale, cilésisé sé frekuencés dhe pérdorimi efikas i
sistemit dhe burimeve té ndérlidhura. Ai pércakton pér kété géllim kérkesat pér ofruesit e FCR-
sé&, duke siguruar qé njésité ose grupet ofruese té tyre té& FCR-sé me Rezervuaré té Kufizuar té
Energjisé té jené né gjendje té aktivizojné plotésisht FCR-né né ményré té vazhdueshme né
gjendje alarmi, pér njé periudhé kohore minimale qé do té pércaktohet né pérputhje me Nenin
156 (10) dhe (11) té Rregullores sé Udhézuesit pér Operimin e Sistemit.

3. Neni 156 (9) i Rregullores sé Udhézuesit pér Operimin e Sistemit parashikon q&, né rast se nuk
Eshté pércaktuar asnjé afat kohor né pajtim me Nenin 156 (10) dhe (11) té& Rregullores sé
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Té gjitha OST-té e Evropés Kontinentale dhe vendeve Nordike, duke marré parasysh si mé
poshté gé:

1. Ky dokument éshté njé propozim i pérbashkét i hartuar nga té gjithé Operatorét e Sistemit té&
Transmetimit t& Evropés Kontinentale dhe zonave sinkrone Nordike (kétej e tutje referuar si
"OST-té") né lidhje me pércaktimin e hipotezave dhe njé metodologjie pér njé Analizé té Kosto-
Pérfitimit (kétej e tutje referuar si "CBA") gé do té kryhet, me géllim gé té vlerésohet periudha
kohore e kérkuar pér rezervat e mbaijtjes sé frekuencés (kétej e tutje referuar si "FCR") njésité
ose grupet ofruese (kétej e tutje referuar si "ofruesit e FCR-sé") me Rezervuaré té Kufizuar té
Energjisé pér té mbetur t& disponueshem gjaté gjendjes sé alarmit, né pérputhje me nenin 156
(11) té Rregullores sé Komisionit (BE) 2017/1485 té datés 2 gusht 2017, g€ pércakton njé
udhézues mbi operimin e sistemit té transmetimit t& energjisé elektrike (kétej e tutje referuar
si "Rregullorja e Udhézuesit pér Operimin e Sistemit"). Kétij propozimi kétej e tutje i referohemi
si "Metodologjia e CBA-sé pér Propozimin e FCR".

2. Metodologjia e CBA-s& pér Propozimin e FCR merr né konsideraté parimet dhe géllimet e
pérgjithshme té pércaktuara né Rregulloren e Udhézimit pér Operimin e Sistemit si dhe
Rregulloren (EC) Nr 714/2009 té Parlamentit Evropian dhe té Késhillit té datés 13 korrik 2009
mbi kushtet e aksesit né rrjet pér shkémbimet ndérkufitare té energjisé elektrike (kétej e tutje
referuar si "Rregullorja KE, Nr 714/2009"). Qéllimi i Rregullores sé Udhézuesit pér Operimin e
Sistemit éshté ruajtja e sigurisé operacionale, cilésisé sé frekuencés dhe pérdorimi efikas i
sistemit dhe burimeve té ndérlidhura. Ai pércakton pér kété qéllim kérkesat pér ofruesit e FCR-
sé, duke siguruar gé njésité ose grupet ofruese té tyre t€ FCR-sé me Rezervuaré té Kufizuar té
Energjisé té jené né gjendje té aktivizojné plotésisht FCR-né né ményré té vazhdueshme né
gjendje alarmi, pér njé periudhé kohore minimale qé do té pércaktohet né pérputhje me Nenin
156 (10) dhe (11) té Rregullores sé Udhézuesit pér Operimin e Sistemit.

3. Neni 156 (9) i Rregullores sé Udhézuesit pér Operimin e Sistemit parashikon gé&, né rast se nuk
8shté pércaktuar asnjé afat kohor né pajtim me Nenin 156 (10) dhe (11) t& Rregullores sé
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e tij ofruese té FCR me Rezervuaré té Kufizuar té Energjisé jané né gjendje té aktivizojné
plotésisht FCR né ményré té vazhdueshme sé paku pér 15 minuta ose, né rast té devijimeve té
frekuencés gé jané mé té vogla sé njé devijim i frekuencés gé kérkon aktivizimin e ploté té
FCR-s&, pér njé periudhé kohe té barabarté ose pér njé periudhé té pércaktuar nga secili OST,
e cila nuk duhet té jeté mé e madhe sé 30 min ose mé e vogél sé 15 minuta. Pér mé tepér,
parashikohet gé, nése éshté pércaktuar njé periudhé kohe né pajtim me Nenin 156 (10) dhe
(11) té Rregullores sé Udhézuesit pér Operimin e Sistemit, secili ofrues i FCR-sé duhet té
sigurojé gé njésité ose grupet ofruese té FCR-sé sé tij me Rezervuaré té Kufizuar té Energjisé
duhet té jené né gjendje té aktivizojné plotésisht FCR né ményré té vazhdueshme né gjendjen
e alarmit pér até periudhé kohe té vlerésuar.
. Neni 156 (10) i Rregullores sé Udhézuesit pér Operimin e Sistemit kérkon gé té gjithé OST-té
e Evropés Kontinentale dhe Nordike té& hartojné njé propozim né lidhje me periudhén minimale
té aktivizimit gé duhet té sigurohet nga ofruesit e FCR-sé dhe specifikon gé periudha e
pércaktuar nuk duhet té jeté mé e madhe sé 30 min ose mé e vogél sé 15 minuta. Propozimi i
tillé duhet t& marré parasysh plotésisht rezultatet e CBA-sé sé kryer né pajtim me Nenin 156
(11) té Rregullores sé Udhézuesit pér Operimin e Sistemit.
. CBA do té marré parasysh sé paku:
a) pérvojat e mbledhura me afatet kohore dhe pjesémarrjes sé teknologjive né
zhvillim né blloge té ndryshme té LFC;
b) ndikimin e njé periudhe kohore té pércaktuar né koston totale té rezervave té FCR
né zonén sinkrone;
¢) ndikimin e njé periudhe kohore té pércaktuar né rrezikimin e géndrueshmérisé sé
sistemit, né veganti gjaté ngjarjeve té zgjatura ose té pérséritura té frekuencés;
d) ndikimin mbi rrezikimin e sigurisé sé sistemit dhe koston totale t& FCR-sé né rast té
rritjes sé volumit total té FCR-sé&;
e) ndikimin e zhvillimeve teknologjike né kostot e periudhave té disponueshmérisé
pér FCR-né nga njésité ose grupet ofruese té FCR-sé sé tij me Rezervuaré té
Kufizuar té Energjisé.
. Kjo metodologji e CBA-s€ pér Propozimin e FCR &shté e lidhur ekskluzivisht me njésité ose
grupet ofruese té FCR-s& me Rezervuaré té Kufizuar té Energjisé.

Sipas nenit 6 (6) té Rregullores sé Udhézuesit pér Operimin e Sistemit, duhet pérshkruar ndikimi
i pritshém i metodologjisé s& CBA-sé pér Propozimin e FCR mbi objektivat e Rregullores sé
Udhézuesit pér Operimin e Sistemit (si¢ &shté e listuar né Nenin 4 (1) t& Rregullores sé
Udhézuesit pér Operimin e Sistemit). Metodologjia e propozuar e CBA-sé pér Propozimin e FCR
né pérgjithési kontribuon né arritjen e objektivave té Nenit 4 (1) té Rregullores sé Udhézuesit
pér Operimin e Sistemit. Né ményré té€ vecanté, metodologjia e CBA-sé€ pér Propozimin e FCR
iu siguron OST-ve té& zonave sinkrone té& Evropés Kontinentale dhe Nordike njé metodologji pér
té vlerésuar dhe hartuar njé propozim né lidhje me periudhén minimale té aktivizimit qé duhet
té sigurohet nga ofruesit e FCR. Pércaktimi i njé periudhe kohore minimale té aktivizimit qé
duhet té sigurohet nga ofruesit e FCR gjaté gjendjes sé alarmit, kontribuon né& pércaktimin e
kérkesave dhe parimeve té pérbashkéta té sigurisé operacionale, té pércaktuara né nenin 4 (1)
(a) té Rregullores sé Udhézuesit pér Operimin e Sistemit. Pér mé tepér, ai kontribuon né
sigurimin e kushteve pér ruajtjen e sigurisé operacionale né té gjithé Unionin sig parashikohet
né nenin 4 (1) (d) t& Rregullores s& Udhézuesit pér Operimin e Sistemit. S& fundmi ai kontribuon
né operimin efikas dhe zhvillimin e sistemit té transmetimit t& energjisé elektrike dhe té sektorit
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Propozimi i té gjitha OST-ve t& Evropés Kontinentale dhe Nordike pér hipotezat dhe njé metodolagji té Analizés s& Kosto-Pérfitimit né
pérputhje me Nenin 156 (11) té Rregullores s& Komisionit (BE) 2017/1485 té datés 2 gusht 2017, qé pércakton njé udhézues mbi
operimin e sistemit té transmetimit té energjisé elektrike

Udhézuesit pér Operimin e Sistemit. Metodologjia e CBA-sé pér Propozimin e FCR nuk ndikon
né objektivat e tjeré té listuara né Nenin 4 (1) té Rregullores sé Udhé&zuesit pér Operimin e
Sistemit.

7. Né pérfundim, metodologjia CBA-sé pér Propozimin e FCR kontribuon né ndjekjen e objektivave
té pérgjithshme té& Rregullores sé Udhézuesit pér Operimin e Sistemit pér ruajtjen e sigurisé
operacionale duke pércaktuar periudhén e duhur kohore pér aktivizimin e ploté té FCR né
gjendjen e alarmit duke marré parasysh kostot dhe pérfitimet e periudhés kohore té pércaktuar,
né té mirén e té gjithé pjesémarrésve té tregut dhe konsumatoréve fundoré té energjisé
elektrike.

PARAQESIN METODOLOGIINE E MEPOSHTME TE CBA-sé PER PROPOZIMIN E FCR TE GIITHA
AUTORITETEVE RREGULLATORE TE ZONES SE EVROPES KONTINENTALE DHE NORDIKE:

Neni 1. Objekti i Iéndés dhe fushéveprimi

Hipotezat dhe metodologjia e CBA-sé si¢ pércaktohet né ké&té metodologji té CBA-sé pér
Propozimin e FCR do té konsiderohet si propozimi i pérbashkét i té gjithé OST-ve t& Evropés
Kontinentale dhe Nordike né pérputhje me nenin 156 (11) té Rregullores sé Udhézuesit pér
Operimin e Sistemit dhe do té pérbéjé bazén mbi té cilén OST-té e zonave sinkrone té Evropes
Kontinentale dhe Nordike duhet té vlerésojné periudhén kohore minimale té aktivizimit & duhet
té sigurohet nga ofruesit e FCR-s€ né pérputhje me Nenin 156 (10) té Rregullores sé€ Udhé&zuesit
pér Operimin e Sistemit.

Neni 2. Pérkufizimet dhe interpretimi

1. Pér géllime t& metodologjisé s& CBA-sé& pé&r Propozimin e FCR-sé&, termat e pérdorur né kété
dokument kané kuptimin e pérkufizimeve té pérfshira né nenin 3 té Rregullores sé Rreguliores
sé Udhézuesit pér Operimin e Sistemit, Rregullores té (KE) 714/2009, Direktivés 2009/72 / KE
dhe Rreguliores (BE) 543/2013.

2. Pérveg késaj, né kété metodologji t& CBA-sé pér Propozimin e FCR, pérveg nése konteksti e
kérkon ndryshe, termat e méposhtém kané kuptimin si vijon:

a) “LER” nénkupton “njésité ose grupet gjeneruese té FCR-sé& me Rezervuaré té Kufizuar
té Energjisé”;

b) “LER Share” nénkupton “pjesén e LER né ofruesit totalé t& FCR-s&”;

c) “Disbalancat e nxitura nga tregu” nénkuptojné “disbalanca gjenerim-ngarkesé e
shkaktuar nga ndryshimi né tarimet e gjenerimit né pérputhje me rezultatet e
skedulimit té tregut”.

d) “Pjerrésia i sistemit” (system droop) nénkupton “raportin midis devijimit té frekuencés
dhe pérgjigjes sé fuqisé sé gjendjes sé qéndrueshme, té siguruar nga FCP”;

e) “Kurba e kostos s& FCR” nénkupton “grupin e té gjithé sasive té ofruara t& FCR me
kostot e tyre respektive”;

f) "Periudha kohore", né pérputhje me Nenin 156 (9) té Rregullores sé& Udhé&zuesit pér
Operimin e Sistemit, nénkupton "koha pér té cilén secili ofrues i FCR duhet t& sigurojé
aé niésité nse arunet e tii siauruese me Rezervuaré té Kufizuar té Fneraiisé té FCR-
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s€, jané né gjendje té aktivizojné plotésisht FCR-né né ményré té vazhdueshme, sapo
nxitet gjendja e alarmit dhe gjaté gjendjes sé alarmit”;

g) “Devijimi i géndrueshém i frekuencés” nénkupton njé “ngjarje me njé devijim té
géndrueshém mesatar té frekuencés mé té madh se sa diapazoni standard i
frekuencés, kundrejt njé periudhe mé té& gjaté se sa koha pér rivendosjen e
frekuencés”.

h) “FAT" do té thoté “Koha e aktivizimit t& FRR-sé plotésisht” sig pércaktohet né nenin 3
(101) dhe (143) t& Rregullores sé Udhézuesit pér Operimin e Sistemit.

“Kapaciteti ekuivalent i rezervuarit t& energjisé” nénkupton kérkesén pér energji pér
LER-ét lidhur me Periudhé&n Kohore dhe do té konsiderchet sa dyfishi i energjisé sé
siguruar nga aktivizimi i ploté i LER pér Periudhén Kohore.

3. Né kété metodologji t& CBA-sé pér Propozimin e FCR-s&, pérve¢ nése konteksti kérkon ndryshe:

a) njéjési tregon shumésin dhe anasjelltas;

b) pérveg nése nuk parashikohet ndryshe, ¢do referencé né njé Nen nénkupton njé Nen
té késaj metodologjie t& CBA-sé pér Propozimin e FCR-sé&;

c) tabela e pérmbajtjes dhe titujt jané vendosur vetém pér lehtési dhe nuk ndikojné né
interpretimin e késaj metodologjie t&€ CBA-sé pér Propozimin e FCR-sé; dhe

d) cdo referencé né legjislacion, rregullore, direktivé, urdhér, instrument, kod ose ndonjé
akt tjetér do té pérfshijé ¢do modifikim, shtesé ose ri-miratim té tij dhe mé pas hyn né
fugi.

Neni 3. Rezultatet dhe progeset e metodologjisé sé CBA

Pér ¢do kombinim té LER Share dhe Periudhés Kohore (sig pérshkruhet né Nenin 6 (2) (a) dhe
Nenin 6 (2) (b)), rezultatet e metodologjisé sé CBA-sé jané:

a) kosto e FCR-sé (si¢ pérshkruhet né Nenin 4 dhe Nenin 5);
b) pranimi i kombinimit kundrejt ngjarjeve reale mé té réndésishme té frekuencés (si¢
pérshkruhet né Nenin 7).

Kostoja e FCR-sé llogaritet me ané té dy progeseve vijuese.

Procesi i paré éshté njé Model Probabilistik Simulimi (i pérshkruar né Nenin 4), rezultati i té cilit
&shté sasia e FCR-sé.

Procesi i dyté éshté njé Vlerésim i kostos sé FCR-sé (i pérshkruar né Nenin 5) i cili lidh njé kosto
me sasiné e kérkuar té FCR-sé & llogaritur nga Modeli Probabilistik i Simulimit.

Pranimi i kombinimit kundrejt ngjarjeve reale mé té réndésishme té frekuencés vlerésohet me
ané té njé progesi té dedikuar (i pérshkruar né Nenin 7).

Neni 4. Modeli Propabilistik i Simulimit

1. Té gjithé OST-té e njé zone sinkrone do té hartojné njé Model Probabilistik Simulimi i cili t&
jeté né gjendje té llogarisé sasiné minimale t& FCR-sé sé nevojshme pér té ruajtur frekuencén
né gjendje té géndrueshme brenda devijimit maksimal té frekuencés né gjendje té
géndrueshme.

2. Burimet e méposhtme té shqetésimeve té frekuencés jané informacion hyrés i Modelit
‘probalistik- t& simulimit




