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VENDIM
Nr. 829, datë 7.10.2015

PËR MIRATIMIN E DOKUMENTIT “STANDARDET SHTETËRORE PËR SPECIFIKIMET TEKNIKE TË INFRASRUKTURËS SË INFORMACIONIT GJEOHAPËSINOR NË SHQIPËRI-TEMA HIDROGRAFIA”

Në mbështetje të nenit 100 të Kushtetutës dhe të neneve 12,  pika 1, 13,  pikat 1 e 4, e 16, pika 1, të ligjit nr.72/2012, “Për organizimin dhe funksionimin e infrastrukturës kombëtare të informacionit gjeohapësinor”, me propozimin e ministrit të Shtetit për Inovacionin dhe Administratën Publike, Këshilli i Ministrave




VENDOSI:

1. Miratimin e dokumentit “Standardet shtetërore për specifikimet teknike të infra-strukturës së informacionit gjeohapësinor në Shqipëri-tema hidrografia”, sipas tekstit, që i bashkëlidhet këtij vendimi dhe është pjesë përbërëse e tij.
2. Ngarkohen ministri i Shtetit për Inovacionin dhe Administratën Publike, Autoriteti Shtetëror për Informacionin Gjeohapësinor (ASIG) dhe autoritetet përgjegjëse për krijimin, ruajtjen dhe përditësimin e të dhënave gjeohapësinore për ndjekjen dhe zbatimin e këtij vendimi.
Ky vendim hyn në fuqi pas botimit në Fletoren Zyrtare.
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FOHAPESINOR

1. PERSHKRIM MBI STANDARTIN

Ky dokument pérmban standartet e t& dhénave gjeohapsinore pér ndértimin ¢ NSDI, duke u mbéshtur né
Direktiven INSPIRE. Autori i kétij produkti &shté Autoriteti Shtetéror pér Informacionin Gjeohapsinor
(ASIG) dhe ne bashkepunim me Sekretariati Teknik i Keshillit Kombetar i Ujit (STKKU). Data ¢ publikimit
t& versionit Nr. 1 &shté Maj 2015. Emértimi i dokumetit &shté: ASIG_Standart NSDI_2015_HID_v.1 ku:

ASIG — Autoriteti pérgjegjés pér krijimin e standartit
Standart — Lloji i dokumentit

NSDI — Qéllimi i dokumentit

2015 — Viti 1 krijimit

HID — Tema pér t& cilén &shté krijuar standarti

v.1 —Nr i versionit t& standartit

2. HYRJE

2.1. SILEXOHET DOKUMENTI.
Ky material &shté i strukturuar né katér kapituj kryesoré:

1
2.

3.
4.

Pérshkrim mbi standartet — ku jepet emértimi dhe autori i standartéve.

Hyrje — N& kété pjesé jepen pérshkrime dhe shpjegime pér t& kuptuar ményrén si organizohet i
gjithé informacioni dhe si mund t& kuptohet mé lehté.

Tema — Ne kapitullin e treté jepen specifikimet teknike pér secilén temé.

Anekse — Kjo &shté pjesa e fundit ku jepen informacione shtése shpjeguese né ndihmé t& lexuesve.

Pérmbajtja e kapitullit 3 &shté e strukturuar pér secilén temé né katér pjesé kryesore:

1- Pérshkrimi mbi temén — I cili flet né ményré t& pérgjithshme pér pérmbajtjen e temés.
2- UML - Pérmbajtja e Katalogut t& Tipologjisé pérkthyer sipas gjuhgs UML.

3-

Katalogu i Tipologjisé — Kétu shpjegohet struktura ¢ temés me gjithé elementét pérbérés & saj.
N¢ tabelat ¢ mé&poshtme jepet njé shpjegim mbi pérmbajtjen dhe ményrén e organizimit té
informacionit ng tabelat ¢ t& dhénave ng katalogun ¢ tipologjisé.

Tabela Nr.1, me ané t& njé shablloni, shpjegon ményrén e organizimit t& informacionit né tabelén
e tipologjisé dhe t& atributeve t& tyre.

Tabela Nr.2, me ané t& njé shablloni, shpjegon ményrén e organizimit t& informacionit né tabelén
e kodlistés.
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Tabela nr.l

Nr | Emértimi i tipologjisé

Pérkufizimi:
| Pérshkrimi:
Tipi i tipologjisé

| Gjeometria

| Lidhet me

Pérkufizimi sipas direktives INSPIRE pér tipologjing.
Shénime dhe pérshkrime t& tjera pér tipologjing.

[ Tipi i elementit hidrografik, i cili mund t& jeté i kétyre llojeve:

«featureType» - njé clement hidrografik i cili mund t& jeté real né
térren apo njé fenomen abstrakt

«dataType» - njé element tabelor i cili shérben vetém si tabelé
atributesh pér tu lidhur me njé element tjetér.
«kodListé» - list& e parapergatitur vlerash q& duhet t& marri njé
atribut “né formé domain-i”
«imported» - t& dhéna t& specifikuara né tema t& tjera t& dircktivés
INSPIRE.

| Gjeometria ¢ clementit sipas formatit vektor (piké, linjé apo poligon)

Abstrakt — kur elemnti nuk &shté element real né terren por mendohet
vetém si fenomen.

| N& momentin qé elemnti X lidhet me elemntin Y, t& gjithé atributet ¢

elemntit Y i shtohen tabelés s atributit t& elemenit X.

Atributi: Emértimi i atributit

Pérkufizimi: Peérkufizimi sipas direktives INSPIRE té& elementit hidrografik
| Pérshkrimi Shénime dhe pérshkrime t& tjera pér elementin hidrografik.
| Lloji i viergs | Lloji i vlerss q& do marri atributi.
| Viers shémbull | Njé vleré shémbull q& mund t& marri atributi q& t& shérbejé si orientim.
[ Shuméllojshméria: ' Lloji dhe numri i vlerave q& mund t& marri atributi
0..* - mund t& marri shumé lloje vlerash ose asnjé vleré
1..* - mund t& marri minimum 1 vleré ose shumé vlera
0..1 - mund t& mos marri asnj& vleré ose nése merr vleré duhet t& marri
vetém 1 vleré t& vetme.
1 - duhet t& marri detyrimisht 1 vleré
[ Detyrueshme | Po — nése atributi &shis i detyrueshem t& plotésohet
Jo — nése atributi nuk &shté i detyrueshém t& plotésohet
Tabela Nr.2
Emértimi i kodlistés
Pérkufizimi Pérkufizimi sipas direktivés INSPIRE té kodlistés
Link | Linku ku mund & gjendet kodlista sipas direktives INSPIRE
Emértimi i vlerés sé atributit i shkurtuar
Emri: Emertimi i ploté
Pérkufizimi: | Perkufizimi i1 vlerés se atributit sipas dircktivés INSPIRE

4- Metadata - Kétu jepen specifikimet teknike pér metadatat ¢ temés pérkatése.
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2.2. DETYRIMET LIGJORE

N& bazg t& ligjit Nr 72/2012, neni 16, “Per organizimin dhe funksionimin e Infrastrukturés Kombetare t&
Informacionit Gjeohapsinor né Republikén e Shqiperisé”ASIG &shté pérgjegjés pér krijimin e standarteve
pér secilén nga temat e pércaktuara né ligj (neni 11), n& pérputhje mé standartet europiane (direktiva
INSPIRE).

Standartet teknike t& t& dhénave gjeohapsinore pér krijimin ¢ NSDI né Shqipéri, jané pérshtatur nga
specifikimet teknike t& temave pérkatése ng direktivén INSPIRE. Pér implementimin ¢ direktivés, kérkohet
qé t& gjithé aktorét t& implementojné disa standarte t& pérbashkeéta, t& cilat mundésojné ndérveprimin e
shérbimeve dhe harmonizimin ¢ t& dhénave.

Standartet (Rregullat ¢ Implementimit (IR)) duhet t& krijohen pér fushat ¢ méposhtme:

e Metadata — n& kété fushe, direktiva pércakton standardet sesi metadata duhet té jené. Ky standard
&shté unik dhe i aplikueshém pér t& gjithé institucionét ose palét e treta (si¢ &shté e pércaktuar né
fushén e veprimit t& késaj direktive), t& cilét do implementojné kété direktive.

o Specifikimi i té dhénave — Standartet ¢ késaj katégorie pérfshing t& gjitha atributét e objektéve t&
ndryshme t& cilat do t& publikohen. INSPIRE ka pércaktuar disa atribute si bazg ¢ cila do shérbejé
pér publikimin ¢ t& dhénave t& ndryshme. N& varési t& ligjeve ose nevojave t& bréndshme mund té
shtohen atribute t& tjera, pér t& béré sa mé t& pérdorshme t& dhénat. Te gjitha t& dhénat q& do shtohen
duhet t& jené t& dokumentuara dhe t& aprovuara nga institucionét pérgjegjése lokale.
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2.3. FUSHA E VEPRIMIT.

Té gjithé autoritetet publike, kompani privaté apo individ, t& cilét mbajné ose pérpunojné t& dhéna
gjeohapsinore pér llogari t& Institucioneve Publike, jang t& detyruar ti nénshtrohen késaj rregulloreje.

Bazuar n& modelet ¢ proceseve t& biznésit, sistemi i propozuar nga direktiva INSPIRE ka proceset dhe
ciklin jetésor si mé poshté:

Shkatrimi

Arkivimi

Planifikimi Shperndarja Analizimi

Perditesimi

Planifikimi — Procesi gjaté t& cilit krijohen strukturat ¢ t& dhénave t& névojshme pér t& publikuar
informacionin n& portal. Rezultatet e kétij procesi jang modelet ¢ ndryshme t& t& dhénave.

Vlerésimi — Procesi gjaté t& cilit t& dhénat ekzistuese testohen kundrejt modelit. Rezultatet e kétij procesi
do jeté certifikimi i t& dhénave ose nevoja pér t& modifikuar t& dhénat pér tu pérshtatur me modelet e
pércaktuara gjaté procesit t& vlerésimit.

Procesimi — Eshté procesi gjaté té cilit mblidhen dhe manipulohen atributet ¢ t& dhénave pér t& prodhuar
informacion kuptimploté. Manipulimi i tyre b&het kundrejt modeleve t& pércaktuar gjaté planifikimit.
Rezultatét e kétij procesi, jané bashkési t& dhénash t& cilat jang gati pér tu publikuar.

Shpérndarja — Procesi gjaté & cilit t& dhénat vihen n& dispozicion pér pérdoruesit (Qytétarét, Autoritéts
publike, Organizata ose palé t& treta). Pérdoruesi mund ti shkarkoj, pérdori, analizojé ose ti citojé ato.
Publikimi i t& dhénave bazohet né modelet e ndryshme t& pérdorimit.

Zbulimi — Proces i vazhdueshém mbi t& dhénat ¢ publikuara, gjaté t& cilit zbulohen t& dhéna t& reja ose t&
dhéna jo cilésore.

Analiza — Procesi i analizimit t& t& dhénave t& evidentuara ng fazén e zbulimit. Gjaté kétij procesi merret
vendimi cfaré do béhet mé t& dhénat q& jang evidentuar.

Pérditésim — Procesi kur propozohet shtimi, modifikimi ose fshirja ¢ t& dhénave. Ky proces inigizohet nga
procesi i analizimit t& t& dhénave ckzistuese dhe t& publikuara.

5|Faqe
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Arkivimi — Procesi gjaté té cilit, bashkésité e t& dhénave q& nuk nevojiten t& aksesohen, arkivohen duke u
bazuar ng standarte lokale dhe legjislacionin né fuqi t& véndeve ku implementimet. Rezultati i kétij procesi
jané t& dhénat t& cilat béhen t& pa aksesueshme pér publikun, me akses vetém nga autoritet specifike. Kéto
t& dhéna vazhdojné t& ruhen pér arsye t& pérputhshmérisé me kuadrin ligjor né fuqi ose standarde specifike.

Shkatérrimi — Procesi gjaté t& cilit, t& dhénat béhen t& pa rikuperueshme. Ky proces bazohet né standarte
lokale ose legjislaciong né fugqi.

6|Faqe
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3. TEMA

3.1. HIDROGRAFIA

3.1.1. PERSHKRIMII TEMES

Hidrografia n& kontekstin e specifikimit t& t& dhénave perfshin pershkrimet mbi:

e detin
e ligenet
e lumenjt

ujérat ¢ tjera

dhe me fenomenét e tyre dhe t& t& gjitha elementéve hidrografike. Pér qéllime t& hartés, pérfshihen t& gjitha
elementét kryesore hidrografike - natyrore dhe artificiale. Gjeografikisht, tema mbi hidrografing mbulon t&
gjitha zonat ujore.

Qéllimi i kétij dokumenti &shté t& specifikojé t& dhénat hapésinore t& harmonizuara pér temén ¢ hidrografisé
si¢ pércaktohet n& Aneksin I t& Direktivés INSPIRE.!

Sipas direktives INSPIRE dhe né mbeshtétje t& nenit 11 t& ligjit Nr. 72/2012 “Per organizimin dhe
funksionimin ¢ Infrastrukturés Kombetare t& Informacionit Gjeohapsinor né Republikén ¢ Shqiperisé”, kjo
temé ka lidhje t& ndérsjellté me temat ¢ permendura si me poshté:

Emeértimet Gjeografike - Emrat e elementéve ujore.

Njésité Administrative — Njésité administrative t& percaktuara nga element hidrografik.
Rijetet e Transportit — Lundrimet, Navigimet.

Modeli dixhital i térrenit — N& lidhje me qéndrueshmering gjeometrike.

Mbulesa e tokes — Tokat e lagura, trupi i ujit, débora, akullnajat dhe ngricat.

Gjeologjia — Gjeomorfologjia dhe ujrat néntokésore.

Infrastruktura urbang dhe shérbimet qeveritare — Furnizimi me ujé dhe pikat ¢ shkarkimit
Infrastruktura p&r monitorimin ¢ mjedisit — stacionét hidrometrike, monitorimi 1 cilésisé s& ujit.
Infrastruktura industriale — Objektet pér nxjertjen e ujit.

Infrastruktura bujqésore dhe akuakultura — Sistemet ¢ ujitjes.

Zonat me pérdorim t& kufizuar — Zonat ¢ basenéve lumore

Zonat me rrezige natyrore — Zonat e pérmbytjeve, erozioni i zonave.

Detet — Kufiri mes tokgs dhe detit.

Pér t& pérmbushur kérkesat e direktivave t& EU pér ujin; ky standart pérfshin:

e rrjetin e lumit dhe kanalit;

! hitp://INSPIRE. ec.europa.ew/documents/Data_Specifications/INSPIRE DataSpecification HY v3.1.pdf

7|Faqe
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e ujin né sipérfaqe, brenda dhe rreth basenéve lumore qé jang kategorizuar si lumenj,
e ligene,

e ujérat kalimtare apo ujérat bregdetare, apo trupave artificialé ujoré.

e sipérfageve, apo organeve t& modifikuar t& ujérave sipérfagésore.

Specifikimet hidrografike jang t& gjeré dhe pér kété arsye &shté ¢ ndare né tre skemat e aplikimit:

- Hidro Baza — Hydro Base;
- Rujeti Hidrografik — Hydro Network;
- Ujrat Fizike - Physical waters.

8|Faqe
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3.1.2. SkEmA UML

N& mbeshtetjé t& direktives INSPIRE mbi ndérveprimin skematik t& elementéve t& Hidrografisé jang
paraqitur diagramat UML. Diagramat ¢ gjuhés UML jang paraqitur n& gjuhén Angleze si gjuhé unike pér
ndértimin e gjuh&s s& programimit sipas Direktivés INSPIRE si méposhté:

pkg Hydrography package structure

«applicatiorSchemax
Hydro - base
A
- '
” '
. '
. '
«applicationSchema» «applicationSchema»
Hydro - Network Hydro - Physical Waters

Figura 1— Diagrama UML: Pérmbajtia e skemés sé aplikimit t¢ ‘Hydro base — Hidro Baza’

class Hydro - base: spatial object types /

+relatedHydroObject|
«voidables 0.*

«featureTypes

HydroObject

wvoidables
+ geographicalName: GeographicalName [0..]
+ hydmld: Hydroldentifier [0.."]

Figura 2— Diagrama UML: Pérmbajtja e skemés sé aplikimit té ‘HydroObject — Objekt Hidrik’
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class Hydro - Network: base /

+relatedHydroObject
«voidablex 0..* \I/_I
«featuraTypes
Hydro - base::HydroObject
GradeSeparatedCrossing| £ avaidabies S LinkSequence]
featursTypes + geographicalName: GeographicalName 0.7 «featureTypes
Watercourse SeparatedCrossing + hydrold: Hydroldentifier [0..] WatercourseLinkSequence
Link Node
«leatureTypes «leatureTypas
WatercourseLink HydroNode

Figura 3 — Diagrama UML: Pérmbajtia e skemés sé aplikimit té ‘Hydro Network — Rrjeti Hidrografik’

class Hydro - Network: spatial object mu/

GeneralisedLi

«featureTypes

«dataTypes HydroObject|
—— «leatureTypes
WatercourseLinkSequence
+ direction: Sign|

“link\|/1

GeneralisedLini +spoteStart +tartNode
e faborat uvoidables
~element « ypes oe Pt
ATRSUnGTyPAS ink «leatureTypes
Networks: 2.0 +spokeEnd +endNode|  Network::Node
GradeSeparatedCrossing ordered] |+ centedineGeometry: GM_( «voidables
foriemd) |+ folifious Boolesn s felis i 0.1 eometry: GM
HydroObject| HydroObject HydroObject|
wfeatureTypes "-.hmv-'ryv-- wfeatureTypes
wvoidable, lifeCyclelnfos «voidable, lifeCycleinfos
+ beginLifespanVersion: DateTime + beginLifespanVersion: DateTime
+ endLifespanVerson: DateTime [0..1]| + endLifespanVersion: DateTime [0..1]
wvoidables «voidables
+ flowbirection: LinkDirectionValue + hydroNodeCategory: HydroNodeCateganyValue

+ langth: Length

Figura 4— Diagrama UML: Elementét hapsinor té ‘Hydro Network - Rrjeti Hidrografik’
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class Hydro - Network: codel... /

wcodeListy
HydroNodeCategoryValue
+ boundary
+ flowConstriction
+ flowRegulation
junction
outlet
source

+ 4+

Figura 5 — Diagrama UML: Kodlista e ‘Hydro Network - Rrjeti Hidrografik’
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Figura 6 — Diagrama UML: ‘Generic Network Model’
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class Hydro - Physical Waters: base /

«featureTypex»
ManMadeObject|

«featureT...
Wetland

«placeholder.f...
Examples:
GlacierSnowfield

afeatureTypen
HydroPointOfinterest|

«featureTypes
LandWaterBoundary|

AbstractObservedEvent
«featureTypen
Floods Example_Model.
/\/ InundatedLand

«featureTyper

Hydro - base::HydroObject 0.*

+relatedHydroObject

«wwidable»

+ geographicalName :GeographicalName [0..]
+ hydrold :Hydroldentifier [0.."]

[N——_| «featureTypen

+drainsBasin S
«woidable» i -
/ A
Al +containsBasin
+outlet «widablex»

*+bank «featureT...\oidables 0>

«woldabler | syrfaceWater|
5. I

Figura 7— Diagrama UML: Pérmbajtia e skemés sé aplikimit ‘Hydro — Physical Waters - Ujrat Fizike’
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class Hydro - Physical Waters matial object types |/

i
:
i
!sJ]

HyaroCeect|
deatureTypes ateatureTypes
Snore. Surtacewater
Inspisks idertifler S Peometry GM_Primitte + peometry [GM_Surtxce
:—-nm-— Sty :na-u—- ¢  igivett tenbter
| voiasties + lewiODetal MD_Resoksion [0..1] soutiet cranaBasin r-n-‘-
B erdane, oidabie s area
S comenitn BTy rh..m < . 31+ basinOmer HyarcOmierCoce [0.1]
4 endLiespanversion -DateTime [0..1] + ongn Orignvalue
wwidatie, eCyclentos
+ beginUfespariversion -DateTme pr—— ke, mCyciss
+ endLiksparversion DateTime . ‘LocaiseaCharacterstnng [0 SegeddspmiVorsion DwteTme
0.1 .nim- o1 + endLiespanversion DateTime [0. 1]
. ‘HycrogicaPersistencoVaie s
+ bl Bosiean GargestEmin eSSy
— i T
LanawaterBoundary
+ geometry -GM_Cune
wokdatie, HeCyciemtos
+ begniiespany/ersion DateTime _""“‘ _-_~’—
+ encLilespanersion -DateTime 10..11
voicaties oidaies woidaties :
+ ongn -OnginVake + condiion -ConationOfF aciity Value [0 1] + emation ‘Length
+ walerLeveiCategary ‘WaterlovelVakie | 4 deneationknown -Bociean + meanDesth :Length
+ length Length 4 sutweres -Ama
+ level VertcalPostionValue
+ streamirder HydroCrdesCode (0. 1] ke
e Do {geometrysSutaceOrPant
ateatureTypes "
Wellend igeometryCuneOrSutce)
PR ——— Danks ShalBeDferent ShorOtyects)
+ geometry (GM_Surtace {ortyManmadeHasCandtionAtn)
wvauables
+ locaType LocaseoCraracterSting 10.1]
+ baw Bookean
evasabie. iReCycierio
+ begriifespanversion DateTime:
4 endUfespanVersion DuteTime [0 1)

Candidate types & placenciders Litimataly not included n the IR

“HydroObject] AMI ‘FyarOorec
et Tyges «placencider. eatureTypes
Sea Reglonsiseadrea satureTypes ExamplesiGlacierSnowteld
Fioods Example Modelzimundatedland
mspireid_Kerntter + geometry “GM_Surtace
% = '+ dateOmbseation DateTime + napiekd idertiter
+ extont ManneExtent [1.] . oCorsequences CbservedConsequences 11,77 ewidatte, BECycieinbs
+ pammetervale [ParametsVakeFair 0.7 Ty 4 begrisespanversion ‘DateTime
vkastie. MeCycient. {The genenc sk or hazard category 15 "FIood” for afl Fwrdated lands} 4 endlitespanVersion -OateTime (0. 4]
+  DeginLiespany/ension |
+ endflespanVersion -CaeTime 10 1)

Figura 8 — Diagrama UML: Elementét hapsinor té ‘Physical Waters’ - ‘Ujrat Fizike’ (pérmban edhe
elementé nga temat e tjera)
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class Hydro - Physical Waters: spatial object types (HydroPointOfinterest) /

HydroObject
ufeatureTypes
HydroPointOfinterest

+ inspireld: Identifier
+ levelOfDetail: MD_Resolution [0..1]]
avoidable, lifeCyclelnfos

+ beginLifespanVerson: DateTime
+ endLifespanVersion: DateTime [0..J1
«voidablaws

+ geometry: GM_Primitive

i

[ I ]

«placeholde... «featureTypex aplaceholde...
Geology: FluvialPoint Geology:
SpringOrSeep Vanis hingPoint

afeaturaTypes «featuraTypen
Rapids Falls
wvoidables
=_height Length

Figura 9 — Diagrama UML: Elementé hapsinor (HidroPointOfInteres - PikéHidrikelnteresi) t& ‘Physical
waters’ - ‘Ujrave Fizik’ (pérmban dhe elementé gé lidhen me temat e tjera)

class Hydro - Physical Waters: spatial object types (ManMadeObject)

«featureType» «featureT... «featureT...
Embankment Ford Lock
\ l7 / «featureT...
{yanEiect Slulce
«featureType»
ManMadeObject 1

+ inspireld :identifier
+ levelOMetail :MD_Resolution [0..1]
«widable, lifeCyclelnfo»
+ beginLifespanVersion :DateTime [« | “featureT...
+ endLifespanVersion :DateTime [0..1] DamOrWeir
«widables

+ condition :ConditionOfFacilityValue
+ geometry :GM_Primitive

)

«eatureType» «featureTypen
Crossing ShorelineConstruction
«woidable»
+ type :CrossingTypeValue

Figura 10— Diagrama UML: Elementé hapsinor (Objekte té ndértuara nga njeriu — ManMadeObject) té
Physical waters’ - ‘Ujrave Fizike’ (pérmban dhe elementé qé lidhen me temat e fera).
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class Hydro - Physical Waters: datatypes /

wdataTypes» «dataType»
‘WidthRange HydroOrderCode
+ lower: Length + order: CharacterString
+ upper: Length + orderScheme: CharacterString
+ scope: CharacterString

Figura 11— Diagrama UML: Elementét tabelor té ‘Physical waters — Ujrat Fizike’

class Hydro - Physical Waters: codelists & enumerations /

«enumeratio... acodelists | wcodelisty J wcodeLists
OriginValue CrossingTypeValue istenceVal ‘WaterLev elValue
natural + aqueduct + diy equinoctial SpringLowWater
manMade + bridge + ephemeral higherHighWater
+ culvert + intermittent higherHighWaterLargeTide
+ siphon + perennial highestAgronomical Tide
highestHighWater
highWater

highWaterSprings
indianSpringHighWater
indianSpringLowWater
localDatum
lowerLowWater
lowerLowWaterLargeTide
lowestAstronomical Tide
lowestLowWater
lowestLowWaterSprings
lowWater
lowWaterDatum
lowWaterSprings
‘meanHigherHighWater
‘meanHigherHighWaterSprings
meanHigherLowWater
meanHighWater
meanHighWaterNeaps
meanHighWaterSprings
meanlLowerHighWater
meanlLowerLowWater
meanlLowerLowWaterSprings
meanLowWater
meanlLowWaterNeaps
meanLowWaterSprings
meanSealevel
meanTidelLevel
meanWaterLevel
neardyHighestHighWater
nearlylowestLowWater
tropicHigherHighWater
tropicLowerLowWater

R R

Figura 12— Diagrama UML: Kodlista e ‘Physical Waters — Ujrat Fizike’
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class Hydro - Physical Waters: imported types. /

s«enumerations wcodelists
Base Types: Base Types:
VerticalPositionValue ConditionOfFacilityValue
onGroundSurface + disused
suspendedOrElevated + functional
underground + projected
+ underConstruction
«dataTypes wcodeLists
Base Types:identifier Base Types:
VoidReasonValue
+ localld: CharacterString
+ namespace: CharacterString + Uninown
alifeCycielnfo, voidables + Unpopulated
+ versonld: CharacterString [0..1]
acodeLists wcodeLists
Natural Risk Land Covers
Zones:: ShoreTypeValue
InundationValue
+ boulders
+ controlled + clay
+ natural + gravel
+ mud
+ rock
+ s=and
+ shingle
+ sdone

Figura 13- Diagrama UML: Elementét e importuar nga temat e tjera té ‘Physical Waters — Ujrat Fizike’
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3.1.3. KATALOGU I TIPOLOGIISE - FEATURE CATOLOGUE

1. HIDRO BAzA - (HIDRO BASE)

1.1. OBJEKT HIDRIK — (HYDROOBJECT)

| 1 | Objekt Hidrik
Pérkufizimi:

Pérshkrimi:
Tipi i elementit

Gjeometria
| Lidhet me

Nj& bazg identiteti pér objektet hidrografike né botén reale (pérfshi edhe ‘
| objektet artificiale) |
SHENIM: Objektet hidrografike t& botés reale pérfagésohen nga specifikime né
skema t& tjera aplikimesh; t& gjithé “perfaqésuesit™ e t& nj&jtit objekt ndajné t&
| nj&jtin emertim gjeografik dhe identifikues hidrografik.

| «teatureType»
| Abstrakt

| Atributi: EmértimiGjeografik

| Perkufizimi:

| Pérshkrimi

Njé emertim gjeografik q& pérdoret t& identifikojé njé objekt hidrografik né
botén reale. Identifikuesi siguron njé “gelés™ pér t& lidhur né ményre t&
| papérséritshme pérfagésues t& ndryshém t& objektit. |
SHEMBULL: Njé element “ujra t& ndenjura” né harté mund t& keté t& njéjtin
emértim gjeografik si njé ligen, duke 1&né t& kuptohet q& ato t& dy jang

| perfagésues t€ s& njgjtit objekt n& bot& reale.

Lloji i vlergs

| Emértim gjeografik

| Lloji i verss
| Vleré Shémbull

| Shuméllojshméria:

Detyrueshme

j Vlere Shémbull L=
| Shuméllojshméria: | 0..*
|| Detyrueshme Po
| Atributi: Hidrold |
Pérkufizimi: Njé identifikues q& pérdoret t& identifikoj& njé objekt hidrografik n& botén reale.
Identifikuesi siguron njé “gelés” pér t& lidhur né ményré t& papérséritshme
| | perfagésues t& ndryshem t& objektit. |
Pérshkrimi SHENIM 1: Identifikuesi mund té jeté njé kod nacional hidrografik

identifikimi.
SHENIM 2: Mg shumé s& njé identifikues mund & jeté ¢ nevojshme, pér
shémbull: njé rryme uji mund t& marri identifikues t& ndryshem sipas skemes
koduese nacionale apo Europiane.
SHEMBULL: Njé porté bllokuese né harté mund t& keté t& njgijtin identifikues
si njé nyjé hidrografike né paragitjen e rrjetit hidrografik, duke leng t& kuptohet
| g& ato t& dy jané perfaqésues t€ s& nj&jtit objekt n¢ botén reale.
| Hidroldentifukues
1 0.%
| Po
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1.2. HIDRO IDENTIFIKUES — (HYDROIDENTIFIER)

2 | Hidroldentifikues

Pérkufizimi:

Njé identifikues tematik hidrografik.

Pérshkrimi:

SHENIM: Mund t& perdoret t& mbaje njé kod identifikimi hidrografik
nacional.

Tipi i elementit

«dataType»

Gjeometria

Lidhet me

Atributi: SkemaEKlasifi

kimit — (classificationScheme)

Pérkufizimi: Njé pérshkrim i skemé&s identifikuese g& pérdoret (Nacionale, Europiane etj).
Pérshkrimi -

Lloji i vlerés CharacterString , Numér

Vlere Shémbull -

Shuméllojshméria: | 0..1

Detyrueshme -

Atributi: Id Lokale — (localld)

Pérkufizimi: Njé identifikues lokal i caktuar nga autoritetet.
SHENIM: Mund t& jeté zakonisht njé identidikues hidrografik nacional.
Pérshkrimi -
| Lloji i vlerés CharacterString, Numér
Vlere shémbull -
Shuméllojshméria: | 1
Detyrueshme Po

Atributi: Emertimi lokal — (nameSpace)

Pérkufizimi:

Njé tregues mbi qé&llimin pér identifikuesin lokal.

Pérshkrimi

SHENIM: N& rast t& njé identifikuesi hidrografik nacional duhet & jeté kod
me dy shkronja sipas ISO 3166-1-Alpha-2.

Lloji i vlerés CharacterString , Numér
Vlere Shémbull -

Shuméllojshméria: | 1

Detyrueshme Po
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2. RRIETI UJOR — (HYDRO NETWORK)

Ne ményré skematike paraqitet tipologjia e Rejetit Ujor (fig.13):

Figura 13. Tipologjia e Rrjetit Ujor

2.1. NYJE HIDROGRAF IKE — (HYDRONODE)

3 | NyjeHidrografike

Pérkufizimi: Njé nyje brenda rrjetit hidrografik.

Pérshkrimi: SHENIM - Mund t& pérfaqésojé njé piké fizike bashkimi/degezimi/mbyllje etj

ose mund t& lidhet me nj& piké hidrografike interesi apo objekti.

Tipi i elementit «featureType»

Gjeometria Pike

Lidhet me HidroObjekt, Nyje (Generic Network Model”)* - Imported type
Atributi: KategoriaHidroNyjes - (hydroNodeCategory)

Pérkufizimi: Natyra e nyjeve hidrografike.

Pérshkrimi -

Lloji i vlerés KodList¢ - VleratEKategoriveTéNyjeveHidrografike® — Imported Type

Vlere Shémbull -

Shuméllojshméria: | 1

Detyrueshme -

% Generic Network Model - gjéndet né specifikimet INSPIRE
http://inspire.ec.europa.ew/documents/Data_Specifications/D2.10.1_GenericNetworkModel v1.0rc3.pdf
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2.2. RRJETII RRJIEDHES UJORE — (WATERCOURSELINK)

4 | RrjetiRrjedhésUjore
| Pérkufizimi: | Njé segment i njé rryme uji brenda njé rrjeti hidrografik. |
Pérshkrimi: SHENIM - Njé rrjedhé ujore mund té jeté imagjinare, pa asnjé lidhje me
objektet reale dhe pérfshihet vetem pér t& siguruar njé rrjet t& mbyllur.
Shémbull fiktiv:
- Segmentét e rrjetéve virtual né njé zong ujore bregdetare
- Segmentét ¢ rrjetéve virtual né zong ligeni
- Segmentét e rrjetéve virtual né lumenj q& lidhin brigjet
- Segmentét e rrjetéve virtual né zona ujore né zhvillim

| Tipi i elementit «featureType»
|| Gjeometria Linjé
Lidhet me HidroObjekt, Lidhjet* ~Imported Type
| Atributi: DrejtimilRjedhés — (flowDirection)
Pérkufizimi: Drejtimi i rrjedhés se ujit né segmentin e shqyrtuar krahasuar me gjeometring
- ¢ segmentit t& dixhitalizuar.
| Pérshkrimi -
| Lloji i vlerés KodList¢ - DrejtimilRrjedh&sVlera?— Imported type
| Vlere Shémbull -
| Shuméllojshméria: | 1
| Detyrueshme Po
| Atributi : Gjatésia — (length)
| Pérkufizimi: Gjatésia e njé segmenti & rrjetit.
| Pérshkrimi | -
| Lloji i vlerés | Gjatési
| Vlere Shémbull | -
| Shuméllojshméria: | 1
Detyrueshme Po

2.3. SEKUENCE E RRJETIT TE RRIEDHES UJORE — (WATERCOURSELINKSEQUENCE)
| 5 | SekuenceERrjetitTeRrjedhesUjore

| Pérkufizimi: | Njé sekuencé e rrjedhes ujoré qé pérfagéson njé pjesé té pa degézuar t& rrjetit.
| Pérshkrimi: | -
| Tipiielementit | «featurcType»
| Gjeometria | Linjé
Lidhet me | HydroObjekt, Rénditja ¢ Lidhjeve® — Imported Type

2.4. KALIMET E UJRAVE TE NDARA — (WATERCOURSESEPARATEDCROSSING)

6 Kalimet e Ujrave té Ndara

Pérkufizimi: Njé& element né rrjetin hidrografik q& tregon njé pike kalimi jo-interaktive t&
| | rrjedhés ujore t€ niveleve t€ ndryshme.

Pérshkrimi: | Pika e kalimit mund t& thye;j ligjerisht njé rregull cilésie t& mos-mbivendosjes.
| Tipiielementit | «featureType»
| Gjeometria | Pik&
| Lidhet me | HydroObjekt, Kalimet ¢ klasave t& ndara®- Imported Type
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KODLISTA E “RRJETTHIDROGRAFIK”

2.5. VLERAT E KATEGORIVE TE NYJEVE HIDROGRAF IKE — (HYDRONODECATEGORY VALUE)

| VleratEKategoriveTéNyjeveHidrografike

Perkufizim Percakton kategorité pér llojet ¢ ndryshme t& nyjeve t& rrjetit hidrografik.
| Link | http:/INSPIRE. ec.curopa.eu/codelist/HydroNodeCategory Value
Viera | Vierat ¢ lejuara pér kété kodlisté jang vlerat e specifikuara ng tabelén e
L | meposhtme.
Kufi — (boundary)
|| Bmri: [ Kufi
| Perkufizimi: | Nyje (pike) q& pérdoret pér t& lidhur rrjete & ndryshme.
| NdryshuesRrjedhe — (flowDirection)
| Emri: | Ndryshues rrjedhe
| Perkufizimi: | Njé nyje e rrjetit e pa lidhur me topologjing e rrjetit né vetvete, por ¢ lidhur me ‘

njé piké hidrografike interesi ose objeti, apo njé objekt artificial, q& ndikon né
L1 B | rrjedhén e ujit.
RregulluesRjedhe — (flowRegulation)
Emri: Rregullues rrjedhe
| Perkufizimi: [ Njé nyje e rrjetit e pa lidhur me topologjing e rrjetit né vetvete, por ¢ lidhur me
njé pike hidrografike interesi ose objeti, apo njé objekt artificial, q& rregullon
‘ rrjedhén e yjit.
Kryqézim — (junction)

Emri: Kryqézim
| Perkufizimi: | Nyje ku tre ose mé shume linja jang t& lidhura.
| Grykederdhje — (outlet)
| [ Emi: Grykederdhje
| Perkufizimi: | Nyja ¢ mbarimit t& nj& seri linjash t& nderlidhura me njéra-tjetren.
Burim - (source) )
| | Emri: Burim
Pérkufizimi: | Pika ¢ fillimit t& njé seri linjash t& ndérlidhura me njéra-tjetrén.
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3. UJRAT FIZIKE — (HYDRO PHYSICAL WATERS)

Ne ményré skematike paraqitet tipologjia ¢ Ujrave Fizike (fig.14, fig.15):

Figura 15. Basenet lumore
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3.1. KALIM — (CROSSING)

1 | Kalim, Véndkalim
Pérkufizimi: Njé& objekt i krijuar nga njeriu ¢ cila lejon kalimin e ujit mbi ose nén njé
pengesé.
Pérshkrimi: SHEMBULL: ujésjellésit, uré, kanal nén rrugg, sifon.
Tipi i elementit «featureType»
Gjeometria Piké
Lidhet me ObjektetéNdértuaraNgaNjeriu
Atributi: Lloji — (type)
Pérkufizimi: Lloji i kalimit fizik
 Pérshkrimi -
Lloji i vlerés VleratELlojeveTéKalimeve - Kodlisté
Vleré Shémbull -
Shuméllojshméria | 1
Detyrueshme Po

3.2. DIGA— (DAMORWEIR)

2 | Diga
Pérkufizimi: Njé& pengesé e pérhershme pérgjaté rrymés sé ujit, e cila pérdoret pér ta mbyllur
apo kontrolluar rrjedhjen e saj
Pérshkrimi: BURIMI [Harta ¢ Europés Rajonale].
Tipi i elementit «featureType»
~Gjeometria Pikg ose Linjé
Lidhet me ObjektetéNdértuaraNgaNjeriu

3.3. PELLGU UJEMBLEDHES — (DRAINAGEBASIN)

3 | PellguUjémbledhés
| Perkufizimi: Zona q& ka njé dalje t& zakonshme pér largimet sipérfaqésore.
Pérshkrimi: SHENIM 1: N¢ lidhje me klasifikimet ¢ ndryshme t& kullimit t& baseneve, nuk

ka dallim midis kullimit t& baseneve/nén-baseneve, e cila mund t& ndryshohet
me aplikimin. Fshté e mundur t& ndértohen basene nga basenét e tjera.
SHENIM 2: Dalje ¢ kullimit t& basenit mund t& jeté njé kanal ose njé ligen.
SHENIM 3: Sinonimet pér kullimin ¢ basenit pérfshijng: ujémbledhés; Zona
ujémbledhés; Zona e kullimit; Pellgjeve; Pellgu ujémbledhés

Tipi i elementit

«featureType»

Gjeometria poligon
Lidhet me ObjektHidrik
_Atributi: Sipérfaqe — (area)
Pérkufizimi: Madhési e zongs s& kullimit t& basenit ¢ pellgut ujembledhés
Pérshkrimi -
Lloji i vierés Sipérfaqe
Vleré Shémbull -
~Shuméllojshméria | 1
Detyrueshme Po

Atributi: RendiIPellgut — (basinOrder)
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Pérkufizimi: Numér (ose kod) q& shpreh shkallén ¢ degézimit/ndarjes né njé sistem t&
pellgut ujémbledhés

Pérshkrimi -

Lloji i vlerés RendilHidroKodit — datatype

Vleré Shémbull | -

Shuméllojshméria | 0....1

Detyrueshme Po

Atributi: FillimilJetégjatésisé - (beginLifespanVersion)

Pérkufizimi: Data dhe koha ng t& cilén ky version i objektit hapésinor &shté krijuar ose
ndryshuar né t& dhénat hapsinore.

Pérshkrimi -

Lloji i vlergs Data Ora

Vleré Shémbull -

Shuméllojshméria | 1

Detyrueshme Po

Atributi: MbarimilJetégjatésisé - (endLifespanVersion)

Pérkufizimi: Data dhe koha né t& cilén ky version i objektit hapésinor &shté pérfunduar.
Pérshkrimi -

Lloji i vlerés Data Ora

Vleré Shémbull -

Shuméllojshméria | 0..1

Detyrueshme Jo

Atributi: Gjeometria — (geometry)

Pérkufizimi: Gjeometria ¢ basenit ujémbledhés
Pérshkrimi -
Lloji i vierés -
Vleré Shémbull -
Shuméllojshméria | 1
Detyrueshme Po
Atributi: Inspireld — @inspireld)
Pérkufizimi: Objekti i jashtém indetifikues i objektit hapsinor
Pérshkrimi SHENIM Njé objekt identifikues i jashtém &sht njé identifikues unik i

objektit t& publikuar nga organi pérgjegjés, t& cilat mund t& pérdoren nga
aplikacionet ¢ jashtme t& referimit t& objektit hapésinor. Identifikuesi &shté njé
identifikues i objektit hap&sinor, jo njé identifikues i fenomenit n& botég.

Lloji i vierés

Indetifikues - ID

Vleré Shémbull -
Shuméllojshméria | 1
Detyrueshme Po

Atributi: Origjina — (origin)

Pérkufizimi:

Origjina ¢ basenit ujémbledhés

Pérshkrimi

SH]?MBULL Natyrore, ¢ krijuar nga njériu etj
SHENIM Njé vend kénetor &shté njé pellg me origjing t& krijuar nga njériu

Lloji i vierés

VleraOrigjing - kodlisté

Vleré Shémbull -
Shuméllojshméria | 1
Detyrueshme Po
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3.4. ARGJINATURE — (EMBANKMENT)

4 | Argjinaturé
Pérkufizimi: Njé& objekt i ndérturar, nga dora ¢ njériut, me grumbuj gurésh apo matériale t&
tjera pérgjaté tokés
Pérshkrimi: SHENIM 1 Pérfshin mbajtjen e murit, strehg, pritat.

SHENIM 2 Pércaktohet dhe si objekt hapésinor né Angksin III né temén 'zona
natyrore e rrezikut "pér shkak t& rolit t& saj né kufizimin ¢ pérmbytjeve.

| Tipiielementit «teatureType»
Gjeometria Piké ose Linjé
Lidhet me ObjekteTéNdértuaraNgaNjeriu

3.5, UJBVARE — (FALLS)

5 | Ujévaré
Pérkufizimi: Njé pjesé e rrjedhés s& ujit ku uji bie né drejtim vertikal nga njé lartési.
| Pérshkrimi: SHEMBULL Ujévarat mbi njé shkémb apo njé greming.
Tipi i elementit «featureType»
Gjeometria Piké
Lidhet me PikaKufiriLumor
Atributi: Lartési — (height)

Pérkufizimi: Distanca e matur nga pika mé e ulét e bazés s¢ térrenit ose nivelit t& ujit deri
né pikén e larté t& objektit hap&sinor.

Pérshkrimi -

Lloji i vlerés Lartésia

Vleré Shémbull -

Shuméllojshméria | 1

Detyrueshme Po

3.6. PIKE KALIMI LUMOR — (FLUVIALPOINT)

6 | PikaKufiriLumor
Pérkufizimi: Njé piké hidro q& ndikon n& rrjedhén e njé rrymé ujore.
Pérshkrimi: -
Tipi i elementit «featureType»

| Gjeometria Abstrakt
Lidhet me PikéelnteresitHidrik
3.7. Va—(FoORrD)

7| Va
Pérkufizimi: Njé pjesé e cekét e shtratit t& rrjedhés ujore ku mund t& pérdoret si rrugé kalimi.
Pérshkrimi: -
Tipi i elementit «featureType»
Gjeometria Piké
Lidhet me ObjekteTéNdértuaraNgaNjeriu
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3.8. PIKE E INTERESIT HIDRIK — (HYDROPOINTOFINTEREST)

8 | PikéelnteresitHidrik
Pérkufizimi: Njé& vend natyror ku uji shfaget, zhduket ose ndryshon rrjedhén e saj.
Pérshkrimi: SHEMBULL Piké e kufirit lumor (ujévaré, kaskada, pragje t& lumit,
ndérprerés), burim (burim, vendburim, burim termal, burim natyror, pus,
(oxhak vullkanik), ujérat artezian), grop karstike (grop karstike, humbja e
drenazhit)
SHENIM Njé piké hidro e cila mund t& krijojé né rrjet njé ngushtim t&
- rrjedhjes.
Tipi i elementit «teatureType»
| Gjeometria Abstrakt
Lidhet me -
Atributi: FillimilJetégjatésisé - (beginLifespanVersion)

At

Pérkufizimi: Data dhe koha ng t& cilén ky version i objektit hapésinor &shté krijuar ose
ndryshuar né t& dhénat hapsinore.

Pérshkrimi -

Lloji i vierés DataOra

Vleré Shémbull -

Shuméllojshméria | 1

Detyrueshme Po

ributi: MbarimilJetégjatésisé -(endLifespanVersion)

Pérkufizimi: Data dhe koha né t& cilén ky version i objektit hapé&sinor &shté pérfunduar

Pérshkrimi -

Lloji i vierés Data Ora

Vleré Shémbull -
| Shuméllojshméria | 0...1

Detyrueshme Jo
Atributi: Gjeometria — (geometry)

Pérkufizimi: Gjeometria ¢ pikés, kurbés apo sipérfaqges

Pérshkrimi -

Lloji i vlerés

Vleré Shémbull -

Shuméllojshméria | 0...1

Detyrueshme Po
Atributi: Inspireld — (inspireld)

Pérkufizimi: Objekti i jashtém indetifikues i objektit hapsinor

Pérshkrimi SHENIM Njé objekt identifikues i jashtém &shté njé identifikues unik i

objektit t& publikuar nga organi pérgjegjés, t& cilat mund t& pérdoren nga
aplikacionet ¢ jashtme t& referimit t& objektit hapésinor. Identifikuesi &shté njé
identifikues i objektit hapésinor, jo njé identifikues i fenomenit né boté.

Lloji i vlerés

Indetifikues - ID

At

Vlerg Shémbull -
_Shuméllojshméria | 1
Detyrueshme Po

ributi: NiveliIdetajeve — (levelOfDetail)

Pérkufizimi: Rezolucioni, i shprehur si invers i njé shkalle ose distance né terren
Pérshkrimi SHENIM: rregullat zbatohen pér portretizim dhe vizualizimi.

Lloji i vlergs -

Vleré Shémbull -
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Shuméllojshméria

0.1

Detyrueshme

Jo

3.9. KUFIRI TOKE UJE — (LANDWATERBOUNDARY)

9 | KufiriTokéUjé

Pérkufizimi:

Njé vijé kufitare ku masa e tokés laget nga uji.

Pérshkrimi:

SHENIM: Referenca e planit pér kufirin toké - ujé duhet t& jeté njé fakt (datum
i t& dhéna) i lartésis€ s& ujit, t& tilla si ‘Mesatarja ¢ lastésisé s& burimit ujor’,
‘Lartésia e Ujit” ose Mesatatja ¢ Lastésisé s& Ujit', ku pak ndryshime ka ng
nivelin e ujit / kéndi i baticés bregdetare, 'Niveli Mesatar i Detit' ku mund t&
pérdoret 'Datum Lokal'.

Tipi i elementit «featureType»
Gjeometria Vijé
Lidhet me -

Atributi: FillimilJetégjatésisé - (beginLifespanVersion)

Pérkufizimi: Data dhe koha ng t& cilén ky version i objektit hapésinor &shté krijuar ose
ndryshuar né t& dhénat hapsinore.
Pérshkrimi -
| Lloji i vlerés DataOra
Vleré Shémbull -
Shuméllojshméria | 1
Detyrueshme Po

Atributi: MbarimilJetégjatésisé - (endLifespanVersion)

Pérkufizimi: Data dhe koha né t& cilén ky version i objektit hapé&sinor &shté pérfunduar
Pérshkrimi -

Lloji i vlergs Data Ora

Vleré Shémbull -

Shuméllojshméria | 0...1

Detyrueshme Jo

Atributi: Gjeometria — (geometry)

Pérkufizimi: Gjeometria ¢ kufirit t& toké — ujé si njé kurbé.
Pérshkrimi -

Lloji i vierés -

Vleré Shémbull -

Shuméllojshméria | 0...1

Detyrueshme Po

Atributi: : Inspireld — (inspireld)

Perkufizimi:

Objekti i jashtém indetifikues i objektit hapsinor

Pérshkrimi

SHENIM Njé objekt identifikues i jashtém &shté njé identifikues unik i
objektit t& publikuar nga organi pérgjegjés, t& cilat mund t& pérdoren nga
aplikacionet ¢ jashtme t& referimit t& objektit hapésinor. Identifikuesi &shté njé
identifikues i objektit hapésinor, jo njé identifikues i fenomenit né boté.

Lloji i vierés

Indetifikues - ID

Vleré Shémbull -
Shuméllojshméria | 1
Detyrueshme Po

Atributi: Origjina — (origin)

| Perkufizimi:

Origjina ¢ kufirit toké - ujé
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Pérshkrimi

SHEMBULL Natyrore, ¢ krijuar nga njériu etj; njé barrier detare &shté njé kufi
toké — ujé si objekt i krijuar nga njériu

Lloji i vlerés

VleraOrigjing - kodlisté

Vleré Shémbull -
Shuméllojshméria | 1
Detyrueshme Po

At

ributi: KategoriaENivelitTéUjit - (waterLevelCategory)

Pérkufizimi: Niveli ujor pércakton kufirin toké - ujé
| Pérshkrimi SHEMBULL Niveli i ujit t& larté, niveli i uji t& ulét, etj
| Lloji i vlergs VleraENivelitTéUjit - Kodlisté
Vleré Shémbull -
Shuméllojshméria | 1
Detyrueshme Po
3.10. PORTA BLLOKUESE — (LOCK)
10 | PortaBllokuese
Pérkufizimi: Njé bllok portash q& shérbejné pér t& ngritur ose ulur nivelin e ujrave gé t&
lejojné kalimin e anijeve nga njé nivel uji né tjetrin.
Pérshkrimi: -
Tipi i elementit «featureType»
Gjeometria Piké
Lidhet me Objekte TéNdértuaraNgaNjeriut
311 OBJEKTE T NDERTUARA NGA NJERIU — (MANMADEOBJECT)
11 | ObjekteTéNdértuaraNgaNjeriu (Objekte artificiale)

Pérkufizimi: Njé& objekt artificial q& shtrihet ng bréndesi t& trupit ujor dhe ka njé nga llojet
¢ funksionit si méposht:
= Mban Ujé
= Rregullon sasin e ujit
= Ndryshon rrjedhjen e ujit
— * Lejon kryqézimin e rrjedhjés ujore.
Pérshkrimi: -
Tipi i elementit «featureType»
Gjeometria Abstrakt
Lidhet me ObjektiHidrik
Atributi: FillimilJetégjatésisé - (beginLifespanVersion)
Pérkufizimi: Data dhe koha né& t& cilén ky version i objektit hapésinor &shté krijuar ose
ndryshuar né t& dhénat hapsinore.
Pérshkrimi -
Lloji i vierés Data Ora
Vleré Shémbull -
Shuméllojshméria | 1
Detyrueshme Po

Atributi: Kushtet - Conditions
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Pérkufizimi: Gjendja e planifikimit, ndértimit, riparimit, dhe/ose mirémbajtjen e
strukturave dhe/apo pajisjeve q& pérbéjné njé strukturé dhe/ose vendosur né
njé vend, si njé e t&ré.

Pérshkrimi -

Lloji i vlerés VleraEGjendjeSEObjetit® — kodlisté - Imported

Vleré Shémbull -

Shuméllojshméria | 1

Detyrueshme Po

_Atributi: MbarimilJetégjatésisé - (endLifespanVersion)

Pérkufizimi: Data dhe koha né t& cilén ky version i objektit hapésinor &shté pérfunduar.
Pérshkrimi -
Lloji i vlergs Data Ora
Vleré Shémbull -
Shuméllojshméria | 0...1
Detyrueshme Jo
| Atributi: Gjeometria — (geometry)

Pérkufizimi: Gjeometria ¢ objektit t& ndértuar nga njériu, si njé pike, kurbé ose sipérfaqe.
Pérshkrimi -
Lloji i vlerés -
Vleré Shémbull -
Shuméllojshméria | 1
Detyrueshme Po
Atributi: Inspireld — (Inspireld)

Pérkufizimi:

Objekti i jashtém indetifikues i objektit hapsinor

Pérshkrimi

SHENIM Njé objekt identifikues i jashtém &shté njé identifikues unik i
objektit t& publikuar nga organi pérgjegjés, t& cilat mund t& pérdoren nga
aplikacionet ¢ jashtme t& referimit t& objektit hapésinor. Identifikuesi éshté njé
identifikues i objektit hapé&sinor, jo njé identifikues i fenomenit n& boté.

Lloji i vierés

Indetifikues - ID

Vlerg Shémbull -
Shuméllojshméria | 1
Detyrueshme Po

Atributi: NivelilDetajeve — (levelOfDetail)

Pérkufizimi:

Rezolucioni, ¢ shprehur si invers i njé shkalle ose distancé né térren

Pérshkrimi

SHENIM: rregullat zbatohen pér portretizim dhe vizualizimi.

Lloji i vierés

Vleré Shémbull

0.1

Shuméllojshméria
Detyrueshme Jo

3412, REKE — (RAPIDS)

12 | Réke
Pérkufizimi: Njé pjesé e njé pérroi me rrjedhje t& pérshpejtuar nga ku ajo zbret pa pushuar
né& shtratin ¢ lumit né formén e njé ujévare.

Pérshkrimi:
Tipi i elementit «featureType»
Gjeometria Linjé
Lidhet me PikéKalimilumor
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3.13. BASENI LUMOR — (RIVERBASIN)

13 | BaseniLumor
Pérkufizimi: Sipérfaqja e zonés nga e cila mblidhen t& gjithé ujrat q&¢ mbushin pérren;jt,
lumenijt apo ligenet dhe derdhen né dete népérmjet grykéderdhjeve, lagunave
apo deltave.

: Pérshkrimi:
| Tipiielementit | «featureType»
| Gjeometria Poligon
| Lidhet me | PellguUjémbledhés
3.14. BREGDET - SHORE
| 14 | Bregdet
Pérkufizimi: Rrip i ngushté toke né kontakt t& drejtpérdrejté me trupin e ujit, duke pérfshirg
| | dhe zonén ndérmjet vijave t& larta dhe t€ ulta t& ujit
Pérshkrimi: SHENIM Konsiderohet si njé objekt hapésinor né témén Mbulesa ¢ Tokés'

pér shkak t& mos standartizimit t& pérfshirjes s& bregut né skemat bregdetare
t& klasifikimit t& mbulesés s& tokés
| Tipiielementit | «featureType»

| Gjeometria | Poligon ose Lin¢
Lidhet me | ObjektHidrik
| Atributi: Inspireld — (Inspireld)
Pérkufizimi: Objekti i jashtém indetifikues i objektit hapsinor
| Pérshkrimi | SHENIM Njé objekt identifikues i jashtém éshté njé identifikues unik i

objektit t& publikuar nga organi pérgjegjés, t& cilat mund t& pérdoren nga
aplikacionet ¢ jashtme t& referimit t& objektit hapé&sinor. Identifikuesi éshté njé
identifikues i objektit hapésinor, jo njé identifikues i fenomenit né boté.

| Lloji 1 vierés | Indetifikues - ID
| Vleré Shémbull | -
| Shuméllojshméria | 1
‘ Detyrueshme Po
| Atributi: Gjeometria — (geometry)
| Pérkufizimi: | Gjeometria ¢ bregdetit
| Pérshkrimi | -
| Lloji i vlerés | -
| Vlerg Shémbull | -
| Shuméllojshméria | 1
Detyrueshme Po S
Atributi: LlojilBregut — (composition)
| Pérkufizimi: | Lloji primar i nj& materiali t& kompozuar t& njé objekti hapsinor, sipérfagja.
| Pérshkrimi | -
| Lloji i vlerés | VleraELlojitTeBregut - Kodlisté
| Vleré Shémbull | -
| Shuméllojshméria | 1
| Detyrueshme Po
| Atributi: Treguesi — (deliniationKnown) )
Pérkufizimi: Tregues pér pércaktimin (pér SHEMBULL: limitet dhe informacioni) e njé

| objekti hapésinor gé &shté i njohur.
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Pérshkrimi -
Lloji i vlerés Text
Vlerg Shémbull -
Shuméllojshméria | 1
Detyrueshme Po
Atributi: FillimilJetégjatésisé - (beginLifespanVersion)
Pérkufizimi: Data dhe koha né& t& cilén ky version i objektit hapésinor &shté krijuar ose
ndryshuar ng t& dhénat hapsinore.
Pérshkrimi -
Lloji i vlerés Data Ora
Vlerg Shémbull -
Shuméllojshméria | 1
Detyrueshme | Po
Atributi: MbarimilJetégjatésisé - (endLifespanVersion)

Pérkufizimi: Data dhe koha né t& cilén ky version i objektit hapésinor &shté pérfunduar

Pérshkrimi -

Lloji i vlerés DataOra

Vleré Shémbull -

Shuméllojshméria | 0...1

Detyrueshme Jo

3.15. OBJEKT BREGDETAR — (SHORELINECONSTRUCTION)
15 | ObjektBregdetar

Pérkufizimi: Njé strukturé artificiale e vendosur né toké, ¢ kufizuar me njé trup ujor dhe
fikse.

Pérshkrimi: Zakonisht &shté e fiksuar né fund & trupit ujor (pér SHEMBULL: njé mol),

por heré pas here mund t& jeté lundrues. Ndértimet bregdetare q& jané pérdorur
zakonisht pér banking dhe / ose mbrojtje.

Pérfshin valéprités / skelg; por ka m& shumé fleksibilitét - gjithashtu vien edhe
pér ujérat ¢ bréndshme (p.sh Ligene)

Tipi i elementit «featureType»
Gjeometria Linjé
Lidhet me Objekte TéNdErtuaraNgaNjériu
3.16. PRITE — (SLUICE)
16 | Prité
Pérkufizimi: Njé objekt i ndértuar né rrjedhén e wjit, i pajisur me njé port, pér t& rregulluar
rrjedhén e ujit.
Pérshkrimi: -
Tipi i elementit «featureType»
Gjeometria Piké
Lidhet me ObjekteTéNdertuaraNgaNjériu
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3.17. PELLG— ( STANDINGWATER)
17 | Pellg
| Pérkufizimi: Njé trup ujor q& &shté i rrethuar plotésisht nga toka
Pérshkrimi: Kjo mund t& ndodh& né njé deformim natyror t& terrenit né t& cilin uji

mblidhet, ose mund t& bllokohet nga njé digg, apo i formuar né shtratin e tij
nga rrénimi i tokés ose i formuar nga bllokimi dhe / ose digat natyrore(pér
SHEMBULL: nga njé digé kastoresh). Ajo mund té jeté ¢ lidhur me hyrjen /
rrjedhé&n ujore apo ujéra té tjera jo t& rrjedhshém.

i Tipi i elementit

«featureType»

| Gjeometria

Piké ose Objekt Gjeometrik

| Lidhet me

ObjekteTéNdertuaraN gaNjeriu

Atributi: Lartésia — (elevation)

| Pérkufizimi: Lart&sia mbi nivelin e detit
| Pérshkrimi -

| Lloji i viergs Lartési

| Vlerg Shémbull -

| Shuméllojshméria: | 1

| Detyrueshme Po

Atributi: ThellésiaMesatare — (meanDepth)

| Pérkufizimi: Thellgsia mesatare e trupit ujor
| Pérshkrimi -
| Lloji i vlerés Lartési
| Vleré Shémbull -
| Shuméllojshméria: | 1
| Detyrueshme Po
Atributi: Sipérfaqja — (surfaceArea)
| Perkufizimi: Sipérfaqja ¢ objektit Ujor
| Pershkrimi
Lloji i vierés Sipérfage
Vleré Shémbull -
Shuméllojshméria: | 1
| Detyrueshme Jo
3.18. SIPERFAQE UJORE — (SURFACEWATER)
18 | SipérfageUjore
Pérkufizimi: Cdo objekt ujor i brendshém né toké
Pérshkrimi: Liqén, pellg, rezervuar, lumé, etj Mund t& pérfshijé dhe ishuj, t& pérfaqésuara

si 'vrima' né gjeometring e saj. Ishujt mundet t& jené t& rrethuar nga njé breg
dhe / ose kufi toke.

| Tipi i elementit «featureType»
| Gjeometria Abstrakt
' Lidhet me ObjektHidrik

Atributi: FillimilJetégjatésisé - (beginLifespanVersion)

| Pérkufizimi: Data dhe ora kur ky version i k&saj vlere &shtg hedhur ng sistem
| Pérshkrimi -

| Lloji i vlerss Data Ora

| Vleré Shémbull
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| Shuméllojshméria: | 1
| Detyrueshme Po
Atributi: MbarimilJetégjatésisé - (endLifespanVersion)
| Pérkufizimi: Data dhe ora kur ky version i vlerés &shté hequr nga sistemi
| Pérshkrimi
| Lloji i vlerés Data Ora
| Vleré Shémbull
| Shuméllojshméria: | 0..1
| Detyrueshme Jo
Atributi: Gjeometria — (geometry)
’ Pérkufizimi: Forma e sipérfaqés ujore — mund t& perfaqsojé njé kurbé / sipérfaqe t& rrjedhés
se ujit ose piké / sipérfaqé pér pellgie
| Pérshkrimi
| Llojii vierés GM Primitive
| Vleré Shémbull
| Shuméllojshméria: | 1
| Detyrueshme Po

Atributi: Inspireld — (inspireld)

| Pérkufizimi:

Identifikues i jashtém pér objektin

Pérshkrimi

Eshté njé identifikues unik i objektit, i publikuar nga organi pérgjegjés, i cili
mund t& pérdoret nga aplikacionet e jashtém pér tu referuar objektit hapésinor.

| Lloji i vlerés

Identifikues (ID)

Vleré Shémbull
| Shuméllojshméria: | 1
| Detyrueshme Po
Atributi: Nivelildetajeve — (levelOfDetail)
Pérkufizimi: Rezolucioni, e shprehur si t& kundért t& njé shkalle treguese ose distanca nga
térreni
| Pérshkrimi Objekti kap njé& shkallg t& caktuar t& nivelit t& detajeve zbatohen rregulla pér

portretizim dhe vizualizim.

Lloji i vlergs

MD Resolution

| Vleré Shémbull -
| Shuméllojshméria: | 0..1
‘ Detyrueshme Jo

Atributi: EmértimiLokal - (localType)

| Pérkufizimi: Pércakton términologji dialektore t& objektit
| Pérshkrimi -

| Llojii vierés LocalisedCharacterString - Numér

| Vlerg Shémbull -

| Shuméllojshméria: | 0..1

[ Detyrueshme Jo

Atributi: Origjina — (origin)

| Pérkufizimi:

Origjina ¢ burimit ujor

Pérshkrimi

Shembuj: Natyrore, ¢ béré nga njeriu. Ujérat sipérfaqésore natyrore jang
rrjedha ujore natyrore (p.sh. lumenj, pérrenj) dhe pellgjet ujore (p.sh. Ligene)
t& rujatura né menyré natyrore, dhe q& jané kanalizuar ose jang krijuar diga,
qofté pér lundrim ose mbrojtje nga pérmbytjet.

Njé sipérfaqe ujore ¢ béré nga njériu &shté e krijuar krejtésisht nga njériu pér
arsye kullimi, ruajtje ose transporti, pérfshiré kanale, rezervuare etj.
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| Lloji i vlerés

VleraOrigjing — kodList&

Vlerg Shémbull

Shuméllojshméria: | 1

Detyrueshme Po
Atributi: Zgjatje — (persistence)

Pérkufizimi: Niveli i zgjatjes se ujit
Pérshkrimi
Lloji i vierés HydrologicalPersisténceValue - kodlisté
Vleré Shémbull
Shuméllojshméria: | 1
Detyrueshme Jo
Atributi: Baticé — (fidial)

Pérkufizimi: Pércakton nése toka preket nga batica
Pérshkrimi -
Lloji i vierés text
Vlerg Shémbull -
Shuméllojshméria: | 1
Detyrueshme Po
3.19. RRIEDHA UJORE — (WATERCOURSE)
19 | Rrjedha Ujore
Pérkufizimi: Njé rrjedhe ujore natyror ose artificial, ose lumé.
Pérshkrimi:
Tipi i elementit «featureType»
Gjeometria Linjé
Lidhet me SipérfageUjore

Atributi: Kushtet

Pérkufizimi: Gjendja e planifikimit, ndértimit, riparimit, dhe / ose mirémbajtjes
Pérshkrimi Me r&ndési vetdm pér rastét e rrjedhave artificiale
Lloji i vierés VleraEGjendjeSEEODbjetit® — kodlists - Imported
Vleré Shémbull -
Shuméllojshméria: | 0..1
Detyrueshme Jo
Atributi: Treguesi — (deliniationKnown)
Pérkufizimi: Njé tregues i pérshkrimit (SHEMBULL: kufijté dhe informacion) i njé objekti
hapésinor t& njohur.
Pérshkrimi Pércaktimi nuk mund t& jet& i njohur né& situatat ¢ méposhtme: njé kanal

néntokésor segment rrjeti néntoksor (tubacion ose seksion i njé rrjeti natyror)
Zona e tranzicionit midis njé lumi t& gjeré dhe njé degé t& vogel t& tij

Lloji i vierés

Text

Vleré Shémbull
Shuméllojshméria: | 1
| Detyrueshme Jo
Atributi: Niveli — (level)
| Pérkufizimi: Niveli vertikal i rrjedhés né lidhje me nivelin e tokés
Pérshkrimi

Lloji i vierés

VleraEpozicionitVertikal? — kodlisté — Imported
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| Vlerg Shémbull
Shuméllojshméria: | 1

| Detyrueshme Jo

Atributi: RendilLumit - (streamOrder)

| Parkufizimi: Numer (ose kod) shprehur shkallén e rrjedhés né njé sistem rrjedhés
Pérshkrimi
Lloji i vierés RendilHidroKodit — datatype
Vleré Shémbull
Shuméllojshméria: | 0..1
Detyrueshme Po

Atr

ibuti: Gjerési — (width)

| Parkufizimi: Gjerésia e rrjedha e ujit (si njé varg) pérgjaté gjithé gjatésisé sé saj
Pérshkrimi
Lloji i vierés VleraEgjerésiséSétrupitUjor - datatype
Vleré Shémbull -
Shuméllojshméria: | 1
| Detyrueshme Jo
3.20. TOKE E LAGUR — (WETLAND)

20

Toké e lagur

Pérkufizimi: Njé& zoné ¢ keq drenazhuar ose q& pérmbytet né ményré periodike, ku toka
&shté e ngopur me ujé, dhe ka bimési.

Pérshkrimi: Shembuj: Kénet&, Mogal

Tipi i elementit «featureType»

Gjeometria poligon

Lidhet me ObjektHidrik

Atr

ibuti: Inspireld — (inspireld)

Pérkufizimi:

Identifikues i jashtém pér objektin

Pérshkrimi

Fshté njé identifikues unik i objektit, i publikuar nga organi pérgjegjés, i cili
mund t& pérdoret nga aplikacionet ¢ jashtme pér tu referuar objektit hapésinor.

Lloji i vierés

Identifikues (ID)

Vlerg Shémbull
Shuméllojshméria: | 1
Detyrueshme Po
Atributi: Gjeometria — (geometry)
Pérkufizimi: Forma gjeometrike e sipérfaqés s& objektit.
Pérshkrimi -
Lloji i vlerés Sipérfaqe
Vlerg Shémbull -
Shuméllojshméria: | 1
Detyrueshme Po
Atributi: EmértimiLokal

Pérkufizimi: Pércakton terminologji dialektore t& objektit.
Pérshkrimi -

Lloji i vierés Character String

Vleré Shémbull

Shuméllojshméria: | 0..1
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| Detyrueshme

|Jo

Atributi: Baticé — (tidal)

Pérkufizimi: Pércakton nése toka preket nga batica.
Pérshkrimi -
Lloji i vierés Tekst
Vleré Shémbull -
Shuméllojshméria: | 1
Detyrueshme Po
Atributi: FillimilJetégjatésisé - (beginLifespanVersion)
Pérkufizimi: Data dhe ora kur ky version i késaj vlere &shté hedhur né sistém
Pérshkrimi -
Lloji i vlerés Data Ora
Vleré Shémbull -
Shuméllojshméria: | 1
Detyrueshme Po
Atributi: MbarimilJetégjatésisé - (endLifespanVersion)
Pérkufizimi: Data dhe ora kur ky version i vlerés &shté hequr nga sistémi.
Pérshkrimi -
Lloji i vierés Data
Vleré Shémbull -
Shuméllojshméria: | 0..1
Detyrueshme Jo
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DATATYPE E UIRAVE FIZIKE

RENDII HIDRO KODIT - HYDROORDERCODE

RendilHidroKodit

Pérkufizimi:

Njé rregull kuptimploté pér emértimin e rendit hierarkik t& rrjedhés ujore dhe
basencve.

Pérshkrimi:

| Tipi i elementit

«dataType »

Atributi: Rendi— (order,

Pérkufizimi: Numér ose kod q& shpreh shkallén ¢ degés ose t& ndarjes né njé lumé apo
sistem t& sistemit t& drenazhimit.
Lloji i vlergs CharacterString
Vlerg Shémbull -
Shuméllojshméria: | 1
Atributi: SkemaFrendit — (orderScheme)
Pérkufizimi: Njé& pérshkrim mbi konceptin ¢ renditjes
Lloji i vlerés CharacterString
Vleré Shémbull -
Shuméllojshméria: | 1
Atributi: Qéllimi — (scope)
Pérkufizimi: Njé tregues pér qéllimin apo origjinén e njé kodi t& rendit.
Lloji i vierés CharacterString
Vleré Shémbull -
Shuméllojshméria: | 1
8:.22. VLERA E GJERESISE SE TRUPIT UJOR - WIDTHRANGE
VleraEgjerésiséSétrupitUjor
Pérkufizimi: Rendi i gjerésisé horizontale t& tupit t& rrugés pérgjaté gjatésisé sé tij.
Pérshkrimi: -
| Tipi i elementit «dataType »
Atributi: Ulét
| Perkufizimi: Gjerési e rendit t& ulét
Lloji i vlerés Gjatesi
Vlerg Shémbull -
Shuméllojshméria: | 1
Atributi: Larté
Pérkufizimi: Gijerési e rendit t& lartg
Lloji i vierés Gjatési
Vlerg Shémbull -
Shuméllojshméria: | 1
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KODLISTA E UIRAVE FIZIKE

3.23. VLERA ORIGJINE - ORIGINVALUE
VleraOrigjiné
Pérkufizim Njé vleré e paracaktuar & tregon origjinén e objekteve té ndryshme hidrografike.
Link -
Vlera -

Natyrale — (natural)

Emri:

Natyrale

Pérkufizimi:

Njé objekt krijuar nga shkaqe natyrore

NgaNjeriu — (manMade)

Emri: Nga njeriu
Pérkufizimi: Njé objekt i krijuar nga dora e njeriut
3.24. VLERAT E LLOJEVE TE KALIMEVE — (CROSSINGTYPEVALUE)

VleratELlojeveT eKalimeve

Pérkufizim Llojet e objekteve fizike t& ndertuar nga njériu (objekt artificial) pergjaté rrjedhés
s& ujit.

Link http://INSPIRE .ec.europa.eu/codelist/Crossing Type Value

Vlera Vlerat e lejuara pér kété kodlisté jané vlerat e specifikuara né tabelén e méposhtme.

Kanal — (aqueduct)

Emri:

kanal

Pérkufizimi:

Njétub ose kanal atrtificial, qé éshté projektuar pér té transportuar ujé nga njé burim
i largét, zakonisht me rrjedhje té liré, pér furnizim té ujérave té émbla, bujqésore,
dhe / ose pérdorim industrial.

Urk — (bridge)

Emri:

uré

Pérkufizimi:

Njé strukture qé lidh dy vendodhje ose siguron njé kalim.

Tombino — (culvert)—

Emri: tombino
Pérkufizimi: Njé kanal 1 mbyllur qé shérben pér kalimin e ujrave nén rrugé.
Sifon — (siphon)

Emri: sifon

Pérkufizimi: Njé strukture tubacioni qé shérben pér té pércjellé léngje nga njé nivel mé i larté né
njé mé té ulét, duke shfrytézuar presionin diferencial qé té detyrojé njé koloné léngu
t& njé niveli mé té larté para se té derdhet né dalje.

3.25. VLERA E GJENDJES HIDROLOGJIKE — (HIDROLOGICALPERSISTENCEVALUE)

VleraEGjendjesHidrologjike

Pérkufizim Kategorité e gjendjes hidrologjike t& zakonshme e njé trupi ujor
Link http://INSPIRE .ec.europa.eu/codelist/HydrologicalPersistenceValue
Vlera Vlerat e lejuara pér kété kodlisté jané vlerat e specifikuara né tabelén e méposhtme

E thaté — (dry)
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Emri: E thaté

Pérkufizimi: E mbushur dhe/ose e rrjedhshme shumé rrallg, pérgjithésisht vetem dhe/ose menjéheré
pas reshjeve té rénda.

Pérkohshme — (ephemeral)

Emri: Pérkohshme
Pérkufizimi: E mbushur dhe/ose e rrjedhshme gjaté dhe menjéheré pas reshjeve.
Pérhershém — (perennial)
Emri: Pérhershém
Pérkufizimi: E mbushur dhe/ose e rrjedhme vazhdimisht gjaté gjithé vitit.
3.26. VLERA E LLOJIT TE BREGUT — (SHORETYPEVALUE)
VleraELIlojitTéBregut
Perkufizim Kategorité e pérbérjes s& zonés té bregut.
Link http://INSPIRE .ec.europa.eu/codelist/ShoreTypeValue
Vlera Vlerat e lejuara pér kété kodlisté jané vlerat e specifikuara né tabelén e méposhtme
Shkémbor — (boulders)
Emri: Shkémbor
Pérkufizimi: Shkémbinjé t& médhenj gjysém té zhytur né uje.
Argjilor — (clay)
Emri: Argjilor
Pérkufizimi: Njé siperfaqe e krijuar nga shkembinjé argjilor té& forté dhe ngjités, té cilét nén ndikimin

e yjrave béhen mé shumé plastike dhe mund té thermohen dhe t& shkriftohen.

Zhavor — (gravel)

Emri: Zhavor
Pérkufizimi: Siperfage e formuar nga guré té vegjél né forme zhavori.
Balté — (mud)
Emri: Balté
Pérkufizimi: Toké e buté me lagéshti, réré, pluhur, dhe / ose me element tjetér toke.
Réré - (sand)
Emri: Rére
Pérkufizimi: Materiale t& grimcuar t& pérbéré nga fragmenté t& vogla té gérryer nga shkémbinj

(kryesisht silicore), mé t& vegjél se zalli dhe mé t& médha se balte.

Zall — (shingle)

Emri: Zall

Perkufizimi: Siperfage e formuar nga guralecé té vegjél, t& liré dhe té rrumbullakuar, t& akumuluar
zakonisht né bregun e detit.

Guré — (Stone)

Emri: Gure

Pérkufizimi: Siperfage e krijuar nga copa té shkémbit ose substanca minerale (t& tjera nga metali) t&
percaktuara né formé dhe madhési, zakonisht né ményré artificiale, dhe pérdoret pér
qéllime t& vecanta.
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3.27. VLERA E NIVELEIT TE UJRAVE — WATERLEVELVALUR

VleraENiveleitT eUjrav

(]

NivelilulétiUjraveNéEkujnoksiPranveror — (equinoctialSpringLowWatér)

| Emri: NivelilulétUjit EkujnoksiPranveror

J Pérkufizimi: Niveli 1 ulét i ujrave né periudhen e ekujnoksit pranveror
NiveliLarté — (high Water)
F TEE:i | kulmiiBaticés

| Péerkufizimi: Niveli mé i larté i arritu né njé vend me sipérfagé té ujit né njé cikél té baticés.
DatumiLokal — (locadD atum)

| Emri: DatumiLokal

Pérkufizimi: Njé reference fillestare e pércaktuar nga njé autoritét i njé porti lokal, nga té cilat nivelet

dhe lartésité e baticés jané matur nga ai autoritét

NiveliUlet — (lowWater)

| Emri: NiveliUlét
Pérkufizimi: Njé siperfaqe pérafruese e nivelit t& ulet mesatare t& ujrave, e cila perdoret si nivel
referimi pér njé rajon té kufizuar, pavarésisht nga pércaktimet mé t& mira qé mund té
béhen mé voné.
DatumiiNivelitT éUlét — (lowWaterDatum)
| Emri: DatumiiNivelitTeUlét
Pérkufizimi: Njé siperfaqé pérafruese e nivelit t& ulét mesatare, e cila &shté pershtatur si njé standart

reference pér njé zoné té caktuar.

NiveliMesatariDetit — (meanSeaLevel)

| Emri:

NiveliMesatariDetit

Pérkufizimi:

Niveli mesatar i detit, 1 marré nga matjet shumévjecare t& njé stacion Mareografik, 1
paracaktuar si nivel reference.
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‘ Perkufizim Niveli baticor i siperfaqes referencé t& ujrave né té cilén referohen lartésité dhe ’
thellésité.

| Link http://INSPIRE .ec.europa.euw/codelist/WaterLevelValue

| Vlera Vlerat e lejuara pér kété kodlisté jané vlerat e specifikuara né tabelen e méposhtme
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3.1.4. METADATA

Tabelat pérshkruajné elementét metadata t& cilat pérmbajé informacionin e méposhtém:

» Kolona ¢ paré siguron njé referencé pér njé pérshkrim mé t& detajuar.

* Kolona e dyté specifikon emrin ¢ elementit metadata.

* Kolona e treté specifikon shuméllojshméring.

« Kolona ¢ katért specifikon kushtet, nén t& cilat elementi i dhéné béhet i detyrueshem.

N& ményré specifike, metadatat pér témén Hidrografi jepen té tabeluara mé poshté:

Specifikimi i té
dhénave pér Elementi Metadata Kushtet
Temén Hidrografia
3141 Refere_nca_e Sistemit 1 -
T Koordinativ
0..* | T detyrueshém, nése grupi i t& dhénave hapésinore ose njé
3142 ?grfligehr;;jneee nga tipet e ve(;orive_ té t) qé pérmban_ informa_cion té
o Sistemit pérkohshme qé& nuk i referohen kalendarit gregorian apo
CoordinatedUniversal Time.
3.1.43 Kodimi L -
31.4.4 Karkteri i Kodimit 0... I detyrueshém, né qofté se njé kodim me bazé jo XML éshté
o pérdorur gé té mos suportojé UTE-1
3145 Lloji i Pérfagésimit 1..% | Metoda e pérdorur hapsinore paragésin informata
T Hapsinor gjeografike

3.1.4.1. REFERENCA E SISTEMIT KOORDINATIV

Emri I Elementit Metadata

Referenca e Sistemit Koordinativ

Pérkufizimi

Pérshkrimi 1 Referencés t& Sistemeve Koordinativ té pérdorur né grupin e té
dhénave hapsinore

Iso 19115 Numri dhe Emértimi

13. referenceSystemInfo

ISO/TS 19139

referenceSystemInfo

INSPIRE I
kushtézuar

detyrueshém /i

I detyrueshem

INSPIRE Shuméllojshméria

1

Lloji 1 t&¢ dhénave (ISO 19115
no.)

186. MD_ReferenceSystem

Vlera e fushés

Pér  t¢  identifikuar  referencé  sistemin  duhet t&  sigurchet
IdentifikuesiReferencéSistemit (RS Identifikues). SHENIM udhézime mé
specifike, né veganti né vlerat e paracaktuara pér plotésimin e atributeve té
IdentifikuesiReferencéSistemit duhet t& bihet dakord mes shteteve anétare gjaté
fazés s& zbatimit t& mbéshtetjes sé ndérveprimit.

Instruksionet e implementimit

Shémbull

referenceSystemIdentifier: code: ETRS 89 codeSpace: INSPIRE RS registry

Shémbull i kodimit XML

<gmd:referenceSystemInfo>
<gmd:MD ReferenceSystem>
<gmd:reference SystemIdentifier>
<gmdRS Identifier>
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<gmd:code>
<gco:Character String=ETRS89 </gco:CharacterString>
</gmd:code>
<gmd:codeSpace>
<gco:CharacterString>=INSPIRE RS registry</gco:CharacterString>
</gmd:codeSpace>
</fgmd:RS_Identifier>
</gmd:referenceSystemIdentifier>
</gmd:MD_ReferenceSystem>
</gmd:referenceSystemInfo>

Komente

3.1.4.2. REFERENCA E PERKOHSHME E SISTEMIT KOORDINATIV

Emri i Elementit Metadata

Reference e Pérkohshme e Sistemit

Pérkufizimi

Pérshkrimi i sistemeve t& pérkohshme té referencés t& pérdorura né setin e té
dhénave

Is0 19115 Numri dhe Emértimi

13. referenceSystemInfo

ISO/TS 19139

referenceSystémInfo

INSPIRE I detyrueshém /i | I detyrueshém, nése grupi i té dhénave hapésinore ose njé nga tipet e vecorive t&

kushtézuar tij qé pérmban informacion t& pérkohshém qé& nuk i referohen kalendarit
Gregorian.

INSPIRE Shuméllojshméria 0.%

Lloji 1 t& dhénave (ISO 19115
no.)

186. MD_ReferenceSystem

Vlera e fushés

Asnjé tip specific nuk &shté pércaktuar né ISO 19.115 pér sistemet e referimit t&
pérkohshme. Késhtu, elementet gjenerik MD ReferenceSystem dhe referencé
SystemlIdentifier (RS Identifier) do t& ofrohen.

Instruksionet e implementimit

Shémbull

referenceSystemIdentifier:
code: GregorianCalendar
codeSpace: INSPIRE RS registry

Shémbull i kodimit XML

<gmd:referenceSystemInfo>
<gmd:MD_ReferenceSystem>
<gmd:reference SystemIdentifier>
<gmdRS Identifier>
<gmd:code>
<gco:CharacterString>GregorianCalendar
</geo:CharacterString>
</gmd:code>
<gmd:codeSpace>
< gco:CharacterString>INSPIRE RS
Registry </gco:CharacterString™>
</gmd:codeSpace>
</gmd:RS_Identifier>
</gmd:referenceSystemIdentifier>
</gmd:MD_ReferenceSystém>
</gmdreferenceSystemInfo>

Komente
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3.1.4.3. KODIMI

Emri i Elementit Metadata

Kodimi

Pérkufizimi

Pérshkrimi 1 konstruktit t& gjuhés kompjuterike gé specifikon pérfagésimin e
objekteve t& t& dhénave né njé rekord, fotografi, mesazh, pajisje ruajtje ose né
kanalin e transmetimit

Is0 19115 Numri dhe Emertimi

271. distributionFormat

ISO/TS 19139

distributionInfo/MD _Distribution/distributionFormat

INSPIRE 1
kushtézuar

detyrueshém /i

I detyrueshém,

INSPIRE Shuméllojshméria

1. %

Lloji 1 t& dhénave (ISO 19115
no.)

284. MD_Format

Vlera e fushés

Vlerat e pronés (emri, version, specifikim) e specifikuar né nenin 5, do té pérdoret
pér t& dokumentuar pérzgjedhjen dhe alternativat e kodimit.

Instruksionet e implementimit

Shémbull

Emri: <Emri i skemés sé aplikuar> GML skemé aplikimi version: specifikim
version 3.1rcl: D2.8.1.8 Data Specifikimet pér Hidrografia - Udhézime teknike

Shémbull i kodimit XML

<gmd:MD_Format>
<gmd:name>
<gco:CharacterString>SomeApplicationSchema GML
application schema</gco:CharacterString™>
</gmd:name>
<gmd:version>
<gco:CharacterString>3. 1rc1</gco:CharacterString>
</gmd:version>
<gmd:specification>
<gco:CharacterString>D2.8.1.8 Data Specification on Hydrography —
Technical Guidelines</gco:CharacterString>
</gmd:specification>
</gmd:MD Format>

Komente

3.1.4.4. KARAKTERET E KODIMIT

Emri i Elementit Metadata

Karakteret e Kodimit

Pérkufizimi

Karakteri I kodimit p&rdoren né setin e t& dhénave.

Iso 19115 Numri dhe Emertimi

ISO/TS 19139

INSPIRE i detyrueshém /i kushtézuar

I detyrueshém, né qofté se njé kodim i pérdorur nuk &shté i bazuar né UTF-8.

INSPIRE Shuméllojshméria

0™

Lloji i t& dhénave (ISO 19115 no.)

Vlera e fushés

Instruksionet e implementimit

Shémbull

Shémbull i kodimit XML

<gmd:characterSet>
<gmd:MD_CharacterSetCode
codeListValue="8859part2"
codeList="http://standards.iso.org/ittf/PubliclyAvailableStandards/ISO_19139
_ Schemas/resources/Codelistt ML _gmxCodelists. xml#Character SetCode">885
9-2</gmd:MD_CharacterSetCode>
</gmd:characterSet>

Komente
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3.1.4.5. LLOJII PERFAQESIMIT HAPSINOR

Emri i Elementit Metadata

Lloji i Pérfagésimit Hapsinor

Pérkufizimi

Metodat e pérdorur hapsinore paragésin informata gjeografike

Iso 19115 Numri dhe Emertimi

37. spatialRepresentationType

ISO/TS 19139

INSPIRE i detyrueshém /i kushtézuar

I detyrueshém

INSPIRE Shuméllojshméria

1%

Lloji i t& dhénave (ISO 19115 no.)

B.5.26 MD_SpatialRepresentationTypeCode

Vlera e fushés

Instruksionet e implementimit

I vlerave t& pérfshiré né listén e koduar né ISO 19115 (vektor, mrjetit, textTable, TIN,
stéreoModel, video), vetém vektor, rrjetit dhe TIN duhet t& pérdoret.
SHENIM vlerat Lista kodi shtesé mund t& pércaktohet bazuar né reagimet nga zbatimi

Shémbull

Shémbull i kodimit XML

Komente
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3.1.5. REFERENCE SISTEMET, NJESITE E MATJEVE DHE RRJETAT GIEOGRAFIKE

3.1.5.1. SISTEMET STANDARTE T REFERIMIT, NJESITE E MATJEVE DHE RRIETET

Sistemet ¢ referencés, njésité ¢ matjeve dhe sistemet e rrjeteve gjeografike t& pérfshira né kété nén-seksion
jang standartet q& do t& pérdoren pér t& gjitha grupet ¢ t& dhénave INSPIRE, pérveg kur ka pérjashtime
specifike t& temés dhe/ose kérkesa té tjera t& pércaktuara né seksionin 6.2.

A. KORNIZA REFERUESE GJEODEZIKE E SHQIPERISE

Korniza Referuese Gjeodezike Shqiptare qé do t& pérdoret né Republikén e Shqipérisé do t& quhet:

“Korniza Referuese Gjeodezike Shqiptare 2010 ose shkurt (KRGISH-2010 — kodi EPSG: 6870 %), ku
20107 &shté indeksi q& lidhet me “epokén” né t& cilén jang pércaktuar koordinatat ¢ pikave gjeodezike t&
monumentalizuara né territorin ¢ Republikés s& Shqipérisé. KRGISH-2010 do t& pércaktohet duke u
mbéshtetur né Kornizén Referuese Gjeodezike Europiane. KRGISH-2010 do t& pérdoret né t& gjitha
aplikacionet q& lidhen me pérdorimin ¢ koordinatave né territorin ¢ vendit. Lidhja midis KRGISH-2010
dhe sistemeve t& tjera t& pérdorura ng vendin tong do t& béhet duke pérdorur parametrat e transformimit t&
llogaritura pér ¢do rast.

KRGISH-2010 pérfshin:

a) parametrat gjeodeziké bazé t& pércaktuar né Sistemin Referues Gjeodezik 1980 (GRS-80) si me
poshte:
= Rrezja ¢ ckuatorit t& tokés: a = 6 378 137m;
= Konstantja gravitacionale gjeocentrike ¢ tokés duke pérfshiré edhe atmosferén: GM = 3 986 005
x 108 m’s 2,
= Faktori dinamik i figurés s& tokés pa pérfshiré baticén ¢ qéndrueshme: J2 = 108 263 x 10°%,;
= Kétij faktori i korrespondon shtypja né pole: 1/f = 298.257222100882711,
= Shpejtésia kéndore e rrotullimit t& tokés: o =7 292115.0 x 10 'rad.sek™

b) sistemin koordinativ gjeodezik ETRS 89;

¢) sistemin e lartésive q& realizohet népérmjet reperave t& rrjetit shtetéror t& nivelimit t& pérfshiré né
Rrjetin Unik Europian t& Nivelacionit (UELN) dhe t& pércaktuara ng Sistemin Referues Vertikal
Europian (EVRS) me ndihmén ¢ t& dhénave pér forcén ¢ réndesés t& unifikuara né sistemin
International Gravity Standardization Network 1971 (IGSN 1971).

d) sistemin ¢ koordinatave né plan, i cili mundésohet nga dy projeksione hartografike:
= Projeksioni Térthor Zonal i Merkatorit (TMzn) pér harta ng shkallé mé t& madhe se 1:500.000 me
parametrat e meposhtme:

- Elipsoidi referencé: GRS80

- Meridiani fillestar: Grinuig

- Meridiani gendor (MQ): 20°

- Shkalla ¢ shformimit n& meridianin gendror (ko): 1

- Fallco ¢ lindjes: 500 000 m
3 Shiko Ancks 4.3
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- Fallco e veriut: Om

= Projeksioni Konik Konform i Lambertit (LCC) pér harta ng shkallg 1:500 000 dhe mé t& vogla.

B. REFERENCE SISTEMET KOORDINATIVE SIPAS INSPIRE

1.2 Datumi

Datumi pér referencé sistemet koordinative dy-dimensionale dhe tre-dimensionale

Pér referencé sistemet koordinative dy-dimensionale dhe tre-dimensionale dhe komponentja horizontale
e reference sistemeve koordinative t& kombinuara t& pérdorura pér t& béré t& disponueshme grupin e t&
dhénave hapésinore, si datum do te jeté datumi i Referencé Sistemit Tokésor Evropian 1989 (ETRS89)
n& zona brenda kufijve gjeografik t& tij, ose datumi i Referencé Sistemit Tokésor Ndérkombétar (ITRS)
ose referencé sisteme koordinative gjeodezike t& tjera t& pérputhura me ITRS, né zona q& ndodhen jashté
kufijve gjeografik t&¢ ETRS89. T& pérputhura me ITRS do t& thoté q& pérkufizimi i sistemit bazohet ng
pérkufizimin e ITRS dhe ka njé marrédhénie t& miré-dokumentuar mes dy sistemeve, sipas EN ISO
19111.

1.3 Referencé sistemet koordinative

Referencé sistemet koordinative

Grupet e t& dhénave hapésinore do t& béhen t& disponueshme duke pérdorur t& paktén njé prej reference
sistemeve koordinatave t& caktuara né seksionet 1.3.1, 1.3.2 dhe 1.3.3, pérveg kur géndron njéri prej
kushteve t& caktuara né seksionin 1.3.4.

1.3.1 Referencé sistemet koordinative tre-dimensionale

- Koordinatat karteziane tre-dimensionale bazohen né njé datum t& caktuar né seksionin 1.2 dhe
pérdorin parametrat e elipsoidit GRS80 (Reference Sistemi Gjeodezik 1980).

- Koordinatat gjeodezike tre-dimensionale (gjerésia, gjatésia dhe lartésia elipsoidike) bazohen né
njé datum t& caktuar né seksionin 1.2 dhe pérdorin parametrat ¢ elipsoidit GRS80.

1.3.2 Referencé sistemet koordinative dy-dimensionale

- Koordinatat gjeodezike dy-dimensionale (gjerésia dhe gjatésia) bazohen né njé datum t&
caktuar né& seksionin 1.2 dhe pérdorin parametrat e elipsoidit GRS 80.

- Koordinatat n& plan pérdorin referencé sistemin koordinativ ETRS89 me projeksion LAEA
(Lambert Azimuthal Equal Area) pér analiza hapé&sinore dhe raportime, ku duhet t& pasqyrohen
sipérfaqget ¢ vérteta.

- Koordinatat n& plan pérdorin referencé sistemin koordinativ ETRS89 me projeksion LCC
(Lambert Conformal Conic) pér hartografime konforme né territorin ¢ Evropés né shkallg t&
barabarta ose mé t& vogla se 1:500 000.
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- Koordinatat n& plan pérdorin referencé sistemin koordinativ ETRS89 me projeksion TM
(Transverse Mercator) pér hartografime konforme né territorin ¢ Evropés ng shkallg t&
barabarta ose mé t& médha se 1:500 000.

1.3.3 Referencé sistemet koordinative té kombinuara

1. Pér komponenten horizontale t& referencé sistemit koordinativ t& kombinuar, njé prej referencé
sistemve koordinative t& caktuara né seksionin 1.3.2 do t& pérdoret.
2. Pér komponenten vertikale, do t& pérdoret njé prej referencé sistemve koordinative t& méposhtme:

- Pér komponenten vertikale ng sipérfagen tokésore, do t& pérdoret Referencé Sistemi Vertikal
Evropian (EVRS) pér t& shprehur lartésité e lidhura me gravitetin brenda kufijve gjeografik t&
keétij sistemi. N& zona t& cilat ndodhen jashté kufijve gjeografik t& EVRS, do t& pérdoren
referencé sisteme vertikale t& tjera t& lidhura me fushén e gravitetit Tokésor pér t& shprehur
lartésité e lidhura me gravitetin.

- Pér komponenten vertikale ng atmosferen ¢ liré, presioni barometrik i konvertuar né lartési
duke pérdour ISO 2533:1975 Atmosferen Standarte Ndérkombétare, ose do t& pérdoren
referencé sisteme té tjera lineare ose parametrike. Aty ku jang pérdorur referencé sisteme
parametrike t& tjera, ato do t& pérshkruhen né njé referencé t& kuptueshme duke pérdorur EN
ISO 19111-2:2012.

- Pér komponenten vertikale ng zonat detare ku ka njé rang t& ndjeshém batice (ujéra baticor), si
sipérfaqe referencé do t& pérdoret Batica mé ¢ ulét Astronomike (LAT).

- Pér komponenten vertikale ng zonat detare ku nuk ka njé rang t& ndjeshém batice, né oqeanet e
hapura dhe efektivisht né ujera me t& thella se 200 metra, si sipérfaqe referencé do t& pérdoret
niveli mesatar i detit (MSL) ose njé nivel reference i miré-pércaktuar i afért me MSL.

1.3.3 Referencé sistemet koordinative té tjera

Si pérjashtime, ku mund t& pérdoren referencé sisteme t& tjera nga ato t& listuarané 1.3.1, 1.3.2 0se 1.3.3,
jang:
1. Referencé sisteme koordinative t& tjera mund t& caktohen pér temat ¢ te dhenave hapésinore
specifike né kété Aneks.

2. Pér zonat (regjionet) q& ndodhen jashté kontinentit t& Evropés, Shtetet Anétare (MS) mund t&
pércaktojné reference sisteme koordinative t& pérshtatshme.

Kodet gjeodezike dhe parametrat ¢ nevojshém pér pérshkrimin e kétyre referencé sistemeve koordinative
dhe t& cilat lejojné veprimet ¢ konvertimit dhe transformimit duhet t& dokumentohen dhe duhet t& krijohet
nj& identifikues, sipas EN ISO 19111 dhe ISO 19127.

1.4 Paraqitja

Referencé sistemet koordinative té pérdorura né shérbimin e shikimit té rrjetit

Pér shfagjen e grupeve té t& dhénave hapésinore népérmjet shérbimit t& shikimit té rrjetit si¢ specifikohet
né rregulloren nr. 976/2009, sé paku referencé sistemi koordinative pér koordinatat gjeodezike dy-
dimensionale (gjerésia, gjatésia) do t& jené t& disponueshme.
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1.5 Identifikuesit pér referencé sistemet koordinative

Identifikuesit e referencé sistemeve koordinative

1. Parametrat dhe identifikuesit e referencé sistemit koordinativ do t& menaxhohen né njé ose disa
regjistra t& pérbashkét pér referencé sistemet koordinative.

2. Vetém identifikuesit q& pérmban njé regjistér i pérbashkét do t& pérdoren pér referimin tek
referencé sistemet koordinative t& listuara né kété seksion.

3. Identifikuesit ¢ listuar né tabelén 2 do t& pérdoren pér referimin tek reference sistemet koordinative
t& pérdorura né njé grup t& dhénash.

Kéto udhézuese teknike propozojné pérdorimin ¢ http URI-t& t& ofruara nga Open Geospatial Consortium
si identifikues t& referencé sistemit koordinativ (shiko identifikuesit pér CRS-t& standart mé& poshté). Kéto
jangé t& bazuara dhe t& drejtojné tek pérkufizimi né regjistrin e parametrave gjeodezik EPSG
(http://www.epsg-registry.org/).

Shénim: Identifikuesit ¢ CRS mund t& pérdoren prsh né:

- Kodimin e t& dhénave,
- Metadatat ¢ grupeve dhe shérbimeve t& t& dhénave, dhe
- Kérkesat pér shérbimet e rrjetit t& INSPIRE.

Tabela 2. http URI-t& pér referencé sistemet koordinative standart:

Referencé sistemi koordinativ | Shkurtimi Identifikuesi http URI

Korniza Referuese Gjeodezike http://www.epsg-

Shqiptare. ETRS89/ Abania | KRGJSH_2010 registry. org/export. htm?gml=urn:ogc:def:cr
2010 s:EPSG::6870

Kartezian 3D né ETRS89 ETRS89-XYZ http://www.opengis.net/def/crs/EPSG/0/4936

Gjeodezike 3D né ETRS89 mbi | ETRS89-GRS80h

GRSS0 http.:// www.opengis.net/deficrs/EPSG/0/4937

Gjeodezike 2D né ETRS89 mbi | ETRS89-GRS80

GRSS0 http.:// www.opengis.net/deficrs/EPSG/0/4258

Projeksion LAEA 2D né | ETRS89-LAEA

ETRS89 mbi GRS80 http:// www.opengis.net/deficrs/EPSG/0/3035

Projeksion LCC 2D né ETRS89 | ETRS89-LCC

mbi GRSS0 http.:// www.opengis.net/deficrs/EPSG/0/3034
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Projeksion TM 2D né ETRS89 | ETRS89-TM34N

mbi GRS80, zona 34N (18°W http:// www.opengis.net/deficrs/EPSG/0/3046
deri 24°W)

Lartési n& EVRS EVRS http:// www.opengis.net/def/crs/EPSG/0/5730
3D t& kombinuara: Gjeodezike | ETRS89-GRS80-EVRS

2D n& ETRS89 mbi GRS80, dhe http:// www.opengis.net/deficrs/EPSG/0/7409
lartésite EVRS

C. REFERENCE SISTEMET E PERKOHSHME

Referencé sistemet e pérkohshme

1. Reference sistemi standart i pérkohshém i referuar tek pika 5 e pjesés B t& Aneksit tek Rregullorja e
Komisionit (EC) nr. 1205/2008 (*) do t& pérdoret, pérveg rastit kur jang caktuar referenc sisteme
koordinative t& pérkohshme t& tjera pér tema t& t& dhénave hapésinore specifike né Ancksin II.

Shénim 1: Pika 5 e pjesés B e Ancksit te Rregullores sé Komisionit (EC) nr. 1205/2008 (IR-t& e metadatave
t& INSPIRE) thekson g referencé sistemi standart do t& jeté kalendari Gregorian, me datat ¢ shprehura né
pérputhje me ISO 8601.

Shénim 2: ISO 8601 Elementet e té dhénave dhe formatet e shkémbimit — Shkémbimi i informacionit —
Pasqyrimi i datés dhé orés &shté njé standard ndérkombétar & mbulon shkémbimin ¢ t& dhénave t& lidhura
datén dhe orén. Q&llimi i kétij standardi &shté q& t& sigurojé njé metodé t& qarté dhe t& mirg-pércaktuar pér
pasqyrimin ¢ datés dhe orés, né ményré q& t& shmangen keqinterpretimet ¢ pasqyrimeve numerike t& daté
dhe orés, veganérisht kur t& dhénat transmetohen ndérmjet shteteve me konventa t& ndryshme pér shkrimin
numerik t& datés dhe orés. Standardi organizon t& dhénat n& ményré q& termi mé i madh i pérkohshém (viti)
shfaqet fillimisht n& t& dhéna varg dhe vazhdon deri te termi mé i vogél (sekondi). Ajo gjithashtu ofron njé
metodé t& standardizuar pér komunikimin informacionit t& bazuar né kohé& ndérmjet zonave kohore duke
duke i dhéné njé spostim te Kohés Universale t& Koordinuar (UTC).

Shémbull: 1997 (viti 1997); 1997-07-16 (16 Korrik 1997); 1997-07-16T 19:20:30+01:00 (16 Korrik 1997,
192 20min 30, zona kohore UTC+1).

D. NJESITE E MATJEVE

Kérkesa dhe rregulla té tjera

2. Té gjitha vlerat ¢ matjeve duhet t& shprehen népérmjet njésive SI ose jo-SI & pranuara pér pérdorim
me Sistemin Ndérkombétar t& Njésive, pérveg kur specifikohet ndryshe pér tema apo tipe specifiket
t& t& dhénave hapésinore.
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3.3.1. CILESIA E TE DHENAVE

Ky kapitull perfshin njé p&rshkrim mbi cilésing e t& dhénave t& clementéve dhé nén elementéve si dhe
cilésing e matjes s& t& dhénave, q& duhen pérdorur pér t& vlerésuar dhe dokumentuar cilésing e t& dhénave

pér data setet q& lidhen me t& dhénat hapsinore t& temés Hidrografia.

Kérkesé

Saktésia e materialeve hartografike, té cilat lidhen me ftipologjiné e temés Hidrografia, duhet té
plotésojné saktésiné ekzistuese té krijimit té kétyre materialeve, deri né momentin e krijimit dhe
pércaktimit té saktésisé sé Hartés pér Kadastrén Multifunksionale. Ndérsa, harta bazé pér elementét
e rinj qé do krijohen do té jeté produkti i krijuar nga fotografimi ajror i vitit 2015.

Cilésia e t& dhénave t& elementéve, nén-clementéve dhe matjeve duhet t& pérdoret pér t&:

= Specifikuar kérkesat apo rekomandimet lidhur me cilésing e t& dhénave t& rezultateve target t&
aplikueshme pér data setet q& lidhen me t& dhénat hapsinore pér temén Hidrografia.

= Vierésuar dhe dokumentuar cilésing e elmenentéve t& metadatave t& t& dhénave t& dataseteve.

Né& tabelén ¢ méposhtme paraqet t& gjithé kérkesat pér cilésing e t& dhénave t& clementéve dhe nén
elementéve qé pérmenden né kété standart. Informacioni 1 cilésisé s& t& dhénave vlerésohet né nivelin ¢

objekteve hapsinore, llojet ¢ objekteve hapsinore, setet e t& dhénave dhe serité e seteve.

Rekomandim:
Ku éshté e pamundur pér té shprehur vierésimin e njé element cilésisé sé té dhénave né ményré sasiore,
vierésimi i elementit duhet té shprehet me njé deklaraté tekstuale si rezultat pérshkrues i cilésisé sé té

dhénave.

3.3.1.1. KOMPLETUAR — KOMISION. (COMPLETENESS — COMMISSION)

Rekomandim:
Komisioni duhet t& vierésohet dhe té dokumentohet duke pérdorur Normén e artikujve té tepért té

pércaktuara né tabelat e méposhtme.

Emri Norma e artikujve té tepért

Emri alternativ -

Cilésia e t& dhénave té elementéve Kompletuar

Cilésia e t& dhénave té nén-elementéve Komision

Cilésia e t& dhénave matjeve themelore Shkalla e gabimit

Pérkufizim Numri i artikujve t& tepérta né setet e té dhénave né lidhje me
numrin e artikujve qé duhet t& ishin t& pranishém.

Pérshkrim -

Fusha vlerésimit Objektet hapsinore
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Fusha raportimit

Llojet e objekteve hapsinore, Setet e t& dhénave.

Parametér

Cilésia e t& dhénave té llojeve té vlerave

Real, pérqgindje, raport

Cilésia e t& dhénave té strukturés té vlerave

Burimi reference

ISO/DIS 19157 Geographic information — Data quality

Shémbull

0,0189;98.11% ;11:582

Masa identifikuese

3

3.3.1.2. KOPLETUAR — PERJASHTIMI. (COMPLETENESS — OMISSION)

Rekomandim:

Pérjashtimi duhet té vierésohet dhe té dokumentohet duke pérdorur Normén e artikujve té tepért té

pércaktuara né tabelat e méposhtme.

Emri Norma e artikujve té tepért
Emri alternativ -

Cilésia e t& dhénave té elementéve Kompletuar

Cilésia e t& dhénave té nén-elementéve Pérjashtimi

Cilésia e t& dhénave matjeve themelore Shkalla e gabimit

Pérkufizim

Numri 1 artikujve t& hequr né setet e t& dhénave né lidhje me
numrin e artikujve qé duhet t& ishin t& pranishém.

Pérshkrim -

Fusha vlerésimit Objektet hapsinore

Fusha raportimit Llojet e objekteve hapsinore, Setet e t& dhénave.
Parametér -

Cilésia e t& dhénave té llojeve t& vlerave

Real, pérgindje, raport

Cilésia e t& dhénave té strukturés té vlerave

Burimi reference

ISO/DIS 19157 Geographic information — Data quality

Shémbull

0,0189;98,11% ; 11:582

Masa identifikuese

7

3.3.1.3. LOGJIKA E QENDRUESHMERISE — KONCEPTI I QENDRUESHMERISE. (LOGICAL CONSISTENCY —

CONCEPTUAL CONSISTENCY)

Rekomandim:

Pér testet né géndrueshmériné konceptuale, rekomandlohet pér té pérdorur cilésiné e té dhénave té nén

elementéve té ‘Logjika e géndrueshmérisé— Koncepti i géndrueshmérisé’ dhe masat e ‘Numri i artikujve

Jjo né pérputhje me rregullat e skemés konceptuale’ dhe ‘Numri i mbivendosjeve paviefshme té

sipérfageve’ té pércaktuara né tabelat e mé poshté:

Emri

Numri i artikujve jo né pérputhje me rregullat e skemés
konceptuale

Emri alternativ

Cilésia e t& dhénave té elementéve

Logjika e gé¢ndrueshmérisé

Cilésia e t& dhénave té nén-elementéve

Koncepti i g¢ndrueshmérisé

52|Faqe





image53.jpeg
m AUTORITETI SHTE

Cilésia e t& dhénave matjeve themelore

Numri i gabimit

Pérkufizim

Numérimin e t& gjitha artikujve né setet e t& dhénave cilat nuk
jané né pérputhje me rregullat e skemés konceptuale.

Pérshkrim

Neése skema konceptuale né ményré té qarté ose t& padyshimté
pérshkruan rregullat, kéto rregulla do t& ndigen. Shkeljet kundér
rregullave té tilla mund té jené, pér Shémbull, vendosja e
pavlefshme e tipologjive brenda njé tolerancé t& caktuar,
dublikimi i elementve dhe mbivendosjet t& pavlefshme té tyre.

Fusha vlerésimit

Objektet hapsinore, llojet e objekteve hapsinore

Fusha raportimit

Setet e t& dhénave

Parametér

Cilésia e t& dhénave té llojeve t& vlerave

Integer

Cilésia e t& dhénave té strukturés té vlerave

Burimi reference

ISO/DIS 19157 Geographic information — Data quality

Shémbull

Masa identifikuese
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Emri

Numri i mbivendosjeve té pavlefshme té sipérfageve

Emri alternativ

Mbivendosja e sipérfageve

Cilésia e t& dhénave té elementéve

Logjika e gé¢ndrueshmérisé

Cilésia e t& dhénave té nén-elementéve

Koncepti i gé¢ndrueshmérisé

Cilésia e t&¢ dhénave matjeve themelore

Numri i gabimit

Pérkufizim

Cilat sipérfaget mund t& pérputhen dhe t& cilat nuk do t& jeng

aplikim i varur. Jo t& gjitha sipérfaget q&é mbivendosen jang

domosdoshmérisht t& gabuara.

Kur e raportoni kété masé té cilésisé t& t& dhénave, duhet té

raportohen gjithashtu llojet e tipologjive 1 pérkatésin

mbivendosjeve té sipérfageve té paligjshme.

Rregullat e méposhtme mbi ményrén se si siperfaget mund té

mbivendosen t& aplikuara né temén Hidrografia t& Direktivés

INSPIRE:

= Digat nuk duhet t& mbivendosen ndérmjet tyre dhe ujévarat,
pérrenjt apo burimet ujore.

= Sipérfaget ujore nuk duhet t& mbivendosen ndermjet tyre
dhe rrejdhés ujore.

= Sipérfaget e tokés sé& lagur nuk duhet &8 mbivendosen
ndérmjet tyre dhe rrjedhés ujore apo sipérfaget ujore.

= Rrjedha ujore nuk duhet t&¢ mbivendosen ndérmjet tyre apo
sipérfaget ujore.

Pérshkrim Objekt hapsinor

Fusha vlerésimit Llojet e objekteve hapsinore, setet e t& dhénave.
Fusha raportimit -

Parametér Integer

Cilésia e t& dhénave té llojeve t& vlerave

Cilésia e t& dhénave té strukturés té vlerave

Burimi reference

ISO/DIS 19157 Geographic information — Data quality
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Shémbull

1<

Fa 2

/
3/

Celés:

1 —sipérfage 1

2 —sipérfaqe 2

3 —sipérfaqja e mbivendosjes

Masa identifikuese
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3.3.1.4. LOGJIKA E QENDRUESHMERISE — FUSHA E QENDRUESHMERISE. (LOGICAL CONSISTENCY — DOMAIN

CONSISTENCY)

Rekomandim:

Pér testet mbi fushén e géndrueshmérisé, rekomandohet pér té pérdorur cilésiné e t& dhénave té nén

elementéve té ‘Logjika e géndrueshmérisé— Fusha e qéndrueshmérisé’ dhe masat e ‘Numri i artikujve

Jo né pérputhje me fushén e tyre té vierave’ dhe ‘Shkalla e pérputhjes sé vierave pér fushat’ si¢ éshté

specifikuar né tabelén e méposhtme:

Emri Numri i artikujve jo né pérputhje me fushén e tyre té vlerave
Emri alternativ -

Cilésia e t& dhénave té elementéve Logjika e géndrueshmérisé

Cilésia e t& dhénave té nén-elementéve Fusha e géndrueshmérisé

Cilésia e t&¢ dhénave matjeve themelore

Numri i gabimit

Pérkufizim

Numérimi i t& gjitha artikujve né setin e t& dhénave qé nuk jang
né pérputhje me fushén e tyre té vlerave

Pérshkrim -

Fusha vlerésimit Objektet hapsinore, llojet e objekteve hapsinore
Fusha raportimit Setet e t& dhénave

Parametér -

Cilésia e t& dhénave té llojeve t& vlerave

Integer

Emri

Shkalla e pérputhjes sé vlerave pér fushat

Emri alternativ

Cilésia e t& dhénave té elementéve

Logjika e gé¢ndrueshmérisé

Cilésia e t& dhénave té nén-elementéve

Fusha e géndrueshmérisé

Cilésia e t&¢ dhénave matjeve themelore

Shkalla e saktésisé sé elementéve

Pérkufizim

Numri i elementéve né setet e t& dhénave qé jané né pérputhje
me fushén e tyre t& vlerave né raport me numrin e pérgjithshém
té artikujve né setin e t& dhénave.

Pérshkrim -

Fusha vlerésimit Objektet hapsinore

Fusha raportimit Llojet e objekteve hapsinore, setet e t& dhenave
Parametér -

Cilésia e t& dhénave té llojeve t& vlerave

Real, pérgindje, raport

Cilésia e t& dhénave té strukturés té vlerave
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Shémbull
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3.3.1.5. LOGJIKA E QENDRUESHMERISE — TOPOLOGJIA E QENDRUESHME. (LOGICAL CONSISTENCY —

TOPOLOGICAL CONSISTENCY)

Rekomandim:

Topologjia e géndrueshme duhet té vierésohet dhe té dokumentohet me ané té: Numri i lidhjeve té

gabuara piké-kurbé, Numri i lidhjeve té munguara pér shkak té mos-mbivendosjes, Numri i lidhjeve té

munguara pér shkak té kalimit té njé ure/rruge, Numri i lidhjeve té munguara pér shkak té

mbivendosjes, Numri i gabimeve té vete-ndérprerjeve, Numri i gabimeve té vete-mbivendosjes, Numri

i lidhjeve té rrjedhés wore poshté gjatésisé sé pragut, Numri i lidhjeve té rrjedhés ujore poshté gjatésisé

sé pragut, Numri i lidhjeve té mbyllura té rrjedhés ujore, Numri i lidhjeve té shuméanshme té rrjedhés

wjore té specifikuara né tabelat e méposhtme.

Cilgsité e topologjisé sé¢ géndrueshme t& nén-clemntéve rekomandohen me qéllim & t& ndértojné nje rrjet

t& mbyllur hidrologjik t& ‘pastér’.

Emri Numri i lidhjeve té gabuara piké-kurbé
Emri alternativ Pika pa lidhje

Cilésia e t& dhénave té elementéve Logjika e géndrueshmérisé

Cilésia e t& dhénave té nén-elementéve Topologjia e géndrueshme

Cilésia e t&¢ dhénave matjeve themelore

Numri i gabimit

Pérkufizim

Numri i lidhjeve t& gabuara té pike-kurbé né setin e t& dhénave.

Pérshkrim

Ekziston njé lidhje piké-kurbé ku kthesat e ndryshme preken.
Kéto kthesa kang njé marrédhénie t& brendshme topologjike qé
do t& pasqyrojé formén e vérteté. Nése lidhja piké-kurbé éshté
né kundérshtim me rrjedhén e pérgjithshme, lidhja piké-kurbé
&shté i gabuar né lidhje me kété masé e cilésisé sé té dhénave.
Cilésia e té dhénave numéron numrin e gabimeve t8 kétij lloji.

Fusha vlerésimit

Objektet hapsinore,

Fusha raportimit

Llojet e objekteve hapsinore, Setet e t& dhénave

Parametér

Cilésia e t& dhénave t& llojeve t& vlerave

Integer

Cilésia e t& dhénave té strukturés té vlerave

Burimi reference

ISO/DIS 19157 Geographic information — Data quality

Shémbull

Shémbull:

Sistemi automatikisht vendos njé piké-kurbé né bazé té limitit t&
kulmeve t& ndértuar sipas kodit t& software, ku nuk ekziston
asnjé justifikim hapésinor pér kéto pika.
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Emri Numri i lidhjeve t¢ munguara pér shkak té€ mos-mbivendosjes
Emri alternativ mos-mbivendosjes

Cilésia e t& dhénave té elementéve Logjika e géndrueshmérisé

Cilésia e t& dhénave té nén-elementéve Topologjia e géndrueshme

Cilésia e t&¢ dhénave matjeve themelore

Numri i gabimit

Pérkufizim

Numri i elementéve né setin e t& dhénave, qé pérputhen pér shkak
t& mos-mbivendosjes, jepet me parametrin e Toleranca e lidhjes

Pérshkrim

Mungesat e lidhjes qé tejkalon Tolerancen e lidhjes konsiderohen
si gabime né qofté se tipologjité reale jané lidhur né rrjetin
hidrografik.

Fusha vlerésimit

Objektet hapsinore

Fusha raportimit

Llojet e objekteve hapsinore, Setet e t& dhénave

Parametér

-Emertimi : Toleranca e lidhjes
-Perkufizim: Distanca e kérkuar nga fundi i njé té veguar.
-Pérshkrim:
Ky parametér éshté specifike pér ¢do set t& dhénash té ofruesve
té t& dhénave dhe duhet té raportohen si metadata pér t& siguruar
krijimin automatik dhe t& qarté t& topologjisé sé lidhjes pér
rrjetin hidrografik.
Toleranca lidhjes duhet té specifikohet nga ofruesi i t& dhénave
duke pérdorur elementét e méposhtme t& metadatatave
DQ Topological Consistency pér masén aktuale:
= 102.measureDescription (lloji: tekst I lire)
Percaktuar si ‘Pershkrimi i matjeve’
= 107 Result (lloji DQ Result)
Pércaktuar si ‘vlera (ose grup vlerash) té marra nga
aplikimi 1 cilésisé sé t& dhénave apo rezultati 1 fituar 1
vlerésimit ti vlerave kundrejté nje niveli t& géndrueshém
cilésie specifike.
Né t& shumtén e rasteve, tolerance pércaktohet me dy
elemnté:
= 130,specifikeme
= 131.shpjegime
Nga klasa DR result.

Shénim: Elemntét e metadatave pércaktohen ne ISO
19115

Cilésia e t& dhénave té llojeve t& vlerave

Integer

Cilésia e t& dhénave té strukturés té vlerave

Burimi reference

ISO/DIS 19157 Geographic information — Data quality
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1 —tolerance e lidhjes
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jané té kapura né nyje dhe jo t& shképutura.
Tot Leceptable Aecentable
st W

ot

Linjat e rrjedhes ujore nuk duhet t& jené t& shképutura, por
gjithmoné t& bashkohet me njé linje tjetér né pike. Njé gabim 1
zakonshém i dixhitalizimit &shté t& kapésh fundin e njé lidhje me
njé lidhje tjetér, por jo né nyje. Kéto linja ndérpriten por nuk béjné
pjesé né topologjing e rrjetit.

Masa identifikuese
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Emri

Numri i lidhjeve té munguara pér shkak té kalimit té njé
ure/rruge

Emri alternativ

Cilésia e t& dhénave té elementéve

Logjika e géndrueshmérisé

Cilésia e t& dhénave té nén-elementéve

Topologjia e géndrueshme

Cilésia e t&¢ dhénave matjeve themelore

Numri i gabimit

Pérkufizim

Numri 1 t& gjithé elementéve té rrjetit lumor né t& dhénat q&
shképuten pér shkak té kalimit t& njé rruge apo ure.

Pérshkrim -

Fusha vlerésimit Objektet hapsinore

Fusha raportimit Llojet e objekteve hapsinore, Setet e t& dhénave
Parametér -

Cilésia e t& dhénave té llojeve t& vlerave

Integer

Cilésia e t&¢ dhénave té strukturés té vlerave

Burimi reference

ISO/DIS 19157 Geographic information — Data quality

Shémbull

Nuk duhet t& jeté asnjé hapésiré/shképutje né rrjetin e rrjedhés
ujore ku ura apo rruga kalon mbi lumin. Kjo éshté e nevojshme
té pérshkruhet si objekt 1 ndértuar nga njeriu dhe t& lidhet me
piké.

Masa identifikuese
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Emri Numri i lidhjeve té munguara pér shkak t¢ mbivendosjes
Emri alternativ Mbivendosje

Cilésia e t& dhénave té elementéve Logjika e géndrueshmérisé

Cilésia e t& dhénave té nén-elementéve Topologjia e géndrueshme
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Cilésia e t& dhénave matjeve themelore

Numri i gabimit

Pérkufizim

Numri i elementéve né setin e t& dhénave, q& pérputhen pér
shkak t& mbivendosjes, jepet me parametrin e Toleranca e
lidhjes

Pérshkrim

Mungesat e lidhjes qé& tejkalon Tolerancén e lidhjes
konsiderohen si gabime né qofté se tipologjité reale jang lidhur
né rrjetin hidrografik.

Fusha vlerésimit

Objektet hapsinore

Fusha raportimit

Llojet e objekteve hapsinore, Setet e t& dhénave

Parametér

-Emertimi : Toleranca e lidhjes
-Perkufizim: Distanca e kérkuar nga fundi 1 njé t& veguar.
-Pérshkrim:
Ky parametér éshté specifike pér ¢do set té dhénash té
ofruesve t& t& dhénave dhe duhet té raportohen si metadata pér
t& siguruar krijimin automatik dhe t& qarté t& topologjisé sé
lidhjes pér rrjetin hidrografik.
Toleranca lidhjes duhet té& specifikohet nga ofruesi i t&
dhénave duke pérdorur elementét e méposhtme té
metadatatave DQ Topological Consistency pér masén
aktuale:
= 102.measureDescription (lloji: tekst I lire)
Percaktuar si ‘Pershkrimi i matjeve’
= 107 Result (lloji DQ_Result)
Pércaktuar si ‘vlera (ose grup vlerash) t& marra nga
aplikimi 1 cilésisé sé t& dhénave apo rezultati i fituar 1
vlerésimit ti vlerave kundrejtt nje niveli t&
qéndrueshém cilésie specifike.
Né té shumtén e rasteve, tolerance pércaktohet me dy
elemnté:
= 130,specifikeme
= 131.shpjegime
Nga klasa DR _result.

Shénim: Elementét e metadatave pércaktohen ne ISO 19115

Cilésia e t& dhénave té llojeve t& vlerave

Integer

Cilésia e t& dhénave té strukturés té vlerave

Burimi reference

ISO/DIS 19157 Geographic information — Data quality

Shémbull
River
i
1
River
Celés:
1- Toleranca e lidhjes =3 m
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Emri Numri i gabimeve t€é veté-ndérprerjes
Emri alternativ Unazor

Cilésia e t& dhénave té elementéve Logjika e géndrueshmérisé

Cilésia e t& dhénave té nén-elementéve Topologjia e géndrueshme

Cilésia e t&¢ dhénave matjeve themelore

Numri i gabimit
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Pérkufizim Numérimi 1 t& gjithé elementéve né t& dhénat qé né ményré &
paligishme ndérpritet me vetveten.

Pérshkrim -

Fusha vlerésimit Objektet hapsinore

Fusha raportimit Llojet e objekteve hapsinore, Setet e t& dhénave

Parametér -

Cilésia e t& dhénave té llojeve t& vlerave

Integer

Cilésia e t& dhénave té strukturés té vlerave

Burimi reference

ISO/DIS 19157 Geographic information — Data quality

Shémbull

2

/

1
Celés:
1 — Rrjeti i rrjedhés ujore
2 — Veté-ndérprerje ilegale (unazore)
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Emri Numri i gabimeve t¢é veté-mbivendosjes
Emri alternativ Mbivendosje

Cilésia e t& dhénave té elementéve Logjika e gé¢ndrueshmérisé

Cilésia e t& dhénave té nén-elementéve Topologjia e géndrueshme

Cilésia e t&¢ dhénave matjeve themelore

Numri i gabimit

Pérkufizim

Numérimi 1 t& gjithé elementéve né t& dhénat qé né ményré &
paligjshme mbivendosen me vetveten

Pérshkrim -

Fusha vlerésimit Objektet hapsinore

Fusha raportimit Llojet e objekteve hapsinore, Setet e t& dhénave
Parametér -

Cilésia e t& dhénave té llojeve t& vlerave

Integer

Cilésia e t& dhénave té strukturés té vlerave

Burimi reference

ISO/DIS 19157 Geographic information — Data quality

Shémbull 1
17— » 2
I —m - 4
overlap
L & & L

‘\ ] V

a - vertekset
Shémbull 2 Linjat nuk duhet té kalojné apo té z&né t& njéjtén hapésiré me até

té njé linje tjetér, me pérjashtim shumé té rrallé kur njé kanal
transferimi kalon né njé kanal tjetér por nuk bashkohet me té.
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Emri

Numiri i lidhjeve té rrjedhés ujore poshté gjatésisé sé pragut.

Emri alternativ
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Cilésia e t& dhénave té elementéve

Logjika e géndrueshmérisé

Cilésia e t& dhénave té nén-elementéve

Topologjia e géndrueshme

Cilésia e t&¢ dhénave matjeve themelore

Numri i gabimit

Pérkufizim

Numérimi 1 t& gjithé elementéve t& rrjedhés ujore né té dhénat
Q& jané nén gjatésisé sé pragut.
Gjatésia e pragut ndryshon né varési té nivelit t& detajeve:

= Lokale—1m

= Rajonale — 10m

= Kombétare — 100 m

Pérshkrim -

Fusha vlerésimit Objektet hapsinore

Fusha raportimit Llojet e objekteve hapsinore, Setet e t& dhénave
Parametér -

Cilésia e t& dhénave t& llojeve t& vlerave

Integer

Cilésia e t& dhénave té strukturés té vlerave

Burimi reference

ISO/DIS 19157 Geographic information — Data quality

Shémbull

Lidhjet mund té futen si shénime né setet e t& dhénave hapsinore
(FeatureClass) si njé rresht né tabelé. Ky shénim mund té ketg
atributet q¢ lidhen me t&. Lidhjet e rrjedhave t& wit nuk duhet t&
jené me gjatési zero.

Masa identifikuese

Emri

Numri i lidhjeve té€ mbyllura té rrjedhés ujore

Emri alternativ

Cilésia e t& dhénave té elementéve

Logjika e gé¢ndrueshmérisé

Cilésia e t& dhénave té nén-elementéve

Fusha e géndrueshmérisé

Cilésia e t& dhénave matjeve themelore

Numri i gabimit

Pérkufizim

Numérimi i té gjitha elemntéve té rrjedhés yjore né té dhénat qé
jané t& mbyllura.

Pérshkrim -

Fusha vlerésimit Objektet hapsinore

Fusha raportimit Llojet e objekteve hapsinore, Setet e t& dhénave
Parametér -

Cilésia e t& dhénave té llojeve t& vlerave

Integer

Cilésia e t& dhénave té strukturés t& vlerave

Burimi reference

ISO/DIS 19157 Geographic information — Data quality

Shémbull

Lidhjet e rrjedhave t& wjit nuk mund té jené t& mbyllura duke
dité q& njé lumé rrjedh nga burimi deri né grykéderdhje. Ajo
mund t& ndahet apo t& devijohet pér shkage natyrore apo
artificiale. Njé linjé nuk duhet t& pérfundojé aty ku nisi.

Masa identifikuese

Emri

Numri i lidhjeve té shumé-pjeséshe té rrjedhés ujore

Emri alternativ

Cilésia e t& dhénave té elementéve

Logjika e gé¢ndrueshmérisé

Cilésia e t& dhénave té nén-elementéve

Fusha e géndrueshmérisé

Cilésia e t& dhénave matjeve themelore

Numri i gabimit

Pérkufizim

Numérimi i t& gjitha elementéve té rrjedhés ujore gé jané té
pérbéré nga shumé pjesé.

Pérshkrim -
Fusha vlerésimit Objektet hapsinore
Fusha raportimit Llojet e objekteve hapsinore, Setet e t& dhénave
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Parametér

Cilésia e t& dhénave t& llojeve t& vlerave

Integer

Cilésia e t& dhénave té strukturés té vlerave

Burimi reference

ISO/DIS 19157 Geographic information — Data quality

Shémbull

Lidhjet duhet t& jené element t& vetém (nuk duhet t& jeté shumé-
pjesésh). Lidhjet shumé-pjeséshe jané lidhje t& pérbéra nga mé
shumé se njé lidhje. Ata mund t& duket t& t& lidhura, por jang
elements t& rrjetit t& pavlefshém
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3.3.1.6. SAKTESIA E POZICIONIMIT — SAKTESIA ABSOLUTE APO JASHTME. (POSITION ACCURACY — ABSOLUTE OR

EXTERNAL ACCURACY)

Rekomandim:

Saktésia absolute dhe e jashtme duhet té vierésohet apo té dokumentohet duke pérdoré Viera mesatare

e pasigurive pozicionale e cila specifikohet si né tabelé:

Emri

Vlera mesatare e pasigurive pozicionale

Emri alternativ

Cilésia e t& dhénave té elementéve

Saktésia e pozicionimit

Cilésia e t& dhénave té nén-elementéve

Saktésia absolute dhe e jashtme

Cilésia e t&¢ dhénave matjeve themelore

E pa aplikueshme

Pérkufizim

Vlera mesatare e pasigurive pozicionale pér njé grup té
pozicioneve ku pagartésité pozicionale jané pércaktuar si
distanca mes njé pozicion té matur dhe até qé konsiderchet si
pozicioni i vérteté

Pérshkrim Shiko ISO/DIS 19157 Geographic information — Data quality
Fusha vlerésimit Objektet hapsinore

Fusha raportimit Llojet e objekteve hapsinore, Setet e t& dhénave

Parametér -

Cilésia e t& dhénave té llojeve t& vlerave

Integer

Cilésia e t& dhénave té strukturés té vlerave

Burimi reference

ISO/DIS 19157 Geographic information — Data quality

Shémbull
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3.3.1.7. SAKTESIA E POZICIONIMIT — SAKTESIA
RELATIVE OR INTERNAL ACCURACY)

Rekomandim:

REIATIVE APO E BRENDSHME. (POSITIONAL ACCURACY —

Saktésia relative apo e brendshme duhet té vierésohet apo té dokumentohet duke pérdoré Gabimet

realative horizontale e cila specifikohet si né tabelé:

Emri

Gabimet realative horizontale

Emri alternativ

Rel CE90

Cilésia e t& dhénave té elementéve

Saktésia e pozicionimit
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Cilésia e t& dhénave té nén-elementéve

Saktésia relative dhe e jashtme

Cilésia e t& dhénave matjeve themelore

E pa aplikueshme

Pérkufizim

Vlerésimi 1 gabimeve té rastit né pozicion horizontal t& njé
elementi né njé tjetér né t& njéjtén set t& dhénash ose né té njéjtén
harté / tabele

Pérshkrim Shiko ISO/DIS 19157 Geographic information — Data quality
Fusha vlerésimit Objektet hapsinore

Fusha raportimit Llojet e objekteve hapsinore, Setet e t& dhénave

Parametér -

Cilésia e t& dhénave té llojeve té vlerave

Integer

Cilésia e t& dhénave té strukturés té vlerave

Burimi reference

ISO/DIS 19157 Geographic information — Data quality

Shémbull
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3.3.1.8. SAKTESIA TEMATIKE — KORREKTESIA JO-SASIORE E ATRIBUTEVE. (THEMATIC ACCURACY — NON-

QUANTITATIVE ATTRIBUTE CORRECTNESS)

Rekomandim:

Korrektésia jo-sasiore e atributeve duhet té vierésohet apo té dokumentohet duke pérdoré Numri i

vierave jo korrekte té atributeve e cila specifikohet si né tabelé:

Emri

Numri i vlerave jo korrekte té atributeve

Emri alternativ

Cilésia e t& dhénave té elementéve

Saktésia tematike

Cilésia e t& dhénave té nén-elementéve

Korrektésia jo sasiore e atributeve

Cilésia e t& dhénave matjeve themelore

Numri i gabimit

Pérkufizim

Numri 1 pérgjithshém i vlerave t& gabuara té atributeve brenda
setit t& t& dhénave pérkatés.

Pérshkrim Shiko ISO/DIS 19157 Geographic information — Data quality
Fusha vlerésimit Objektet hapsinore

Fusha raportimit Llojet e objekteve hapsinore, Setet e t& dhénave

Parametér -

Cilésia e t& dhénave té llojeve t& vlerave

Integer

Cilésia e t& dhénave té strukturés té vlerave

Burimi reference

ISO/DIS 19157 Geographic information — Data quality

Shémbull
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3.3.1.9. SAKTESIA TEKNIKE — SAKTESIA SASIORE E ATRIBUTEVE. (TEMATIC ACCURACY — QUANTITATIVE

ATTRIBUTE ACCURACY)

Rekomandim:

Saktésia sasiore e atributeve duhet té vierésohet apo té dokumentohet duke pérdoré Niveli i rendésisé

sé vierave té atributeve me 95% pasiguri e cila specifikohet si né tabelé:
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Emri

Niveli i rendésisé sé vlerave té atributeve me 95% pasiguri

Emri alternativ

Cilésia e t& dhénave té elementéve

Saktésia tematike

Cilésia e t& dhénave té nén-elementéve

Saktésia sasiore e atributeve

Cilésia e t& dhénave matjeve themelore

LE95 ose LE95(r), ne varési té procedurés sé vlerésimit

Pérkufizim

Gjysma e gjatésisé s& intervalit t& pércaktuar nga njé kufi i
sipérme dhe 1 poshtém, né & cilén vlera e vértetd pér cilésie
sasiore shtrihet me probabilitet 95%

Pérshkrim

Numri i t& gjithé vlerave t& atributeve ku vlera &shté gabim

Fusha vlerésimit

Objektet hapsinore

Fusha raportimit

Llojet e objekteve hapsinore, Setet e t& dhénave

Parametér

Cilésia e t& dhénave té llojeve té vlerave

Integer

Cilésia e t& dhénave té strukturés té vlerave

Burimi reference

ISO/DIS 19157 Geographic information — Data quality

Shémbull

Masa identifikuese
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4. ANEKSE

4.1.

1.1
12

2.1
22
23

2.4

2.5
31
32
33
34
35
36
37
38
39
3.10
311
312
313
3.14
3.15
3.16
317
3.18
3.19
3.20
321

KATALOGU I TIPOLOGIJISE

Tabelé shpjeguese mbi lidhjen ¢ tipologjisé né temén Hidrografia né Shqip dhe t& asaj Hidrography né
Anglisht.

Emri I elementit
Anglisht

HydroObject
Hydroldentifier
HydroNode

watercourseLink

watercourseLinkSequenc
e
watercourseSeparatedCr
ossing
HydroNodeCategoryVal
ue

Crossing
DamOrweir
DrainageBasin
Embankment

Falls

FluvialPoint

Ford
HydroPointOflnterest
LandwaterBoundary
Lock
ManMadeObject
Rapids

RiverBasin

Shore
ShorelineConstruction
Sluice
Standingwater
Surfacewater
‘Watercourse
Wetland
HydroOrderCode

Emri I elementit Shqip
ObjektHidrik
Hidroldentifikues
NyjeHidrografike

RrjetiRrjedhesUjore

SekuenceERrjetitTeRrjedhes
Ujore

KalimetEUjraveTeNdara
KategoriaHidroNyjeVlere
Mbi/Nen-Kalim

Dige

PellguUjémbledhés
Argjinaturé

Ujevaré
PikeKalimiLumore

Va
PikaInteresiHidrografike
KufiriUjeToke

PortaBllokuese

ObjekteTéNdertuaraNgaNjeri
u

Rreke
BasenLumor
Bregdet
ObjektBregdetar
Prité

Pellg
SiperfageUjore
RrjedhaUjore
ZonatELagura
RendilhidroKodit

Package

Hydro - base
Hydro - base
Hydro - Network
Hydro - Network

Hydro - Network
Hydro - Network

Hydro - Network

Hydro - Physical waters
Hydro - Physical waters
Hydro - Physical waters
Hydro - Physical waters
Hydro - Physical waters
Hydro - Physical waters
Hydro - Physical waters
Hydro - Physical waters
Hydro - Physical waters
Hydro - Physical waters
Hydro - Physical waters
Hydro - Physical waters
Hydro - Physical waters
Hydro - Physical waters
Hydro - Physical waters
Hydro - Physical waters
Hydro - Physical waters
Hydro - Physical waters
Hydro - Physical waters
Hydro - Physical waters
Hydro - Physical waters

Stereotypes
«featureType» Astrakt
«dataType»
«featureType»
«featureType»

«featureType»
«featureType»
«codeList»
«featureType»
«featureType»
«featureType»
«featureType»
«featureType»
«featureType» Abstrakt
«featureType»
«featureType» Abstrakt
«featureType»
«featureType»

«featureType» Abstrakt

«featureType»
«featureType»
«featureType»
«featureType»
«featureType»
«featureType»
«featureType» Abstrakt
«featureType»
«featureType»
«dataType»
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322 | WidthRange

3.23 | OriginValue

3.24 | CrossingTypeValue

325 Hydrological PersistentV
alue

3.26 | ShoreTypeValue

3.27 | WaterLevel Value

ANEKSE

A ConditionOfFacilityValu
e

B VerticalPositionValue

C GeneralisedLink

D GradeSeparatedCrossing

E Link

F LinkSequence

G NetworkElement

H Node

1 LinkDirection

4.2. IMPORTED TYPE

{OHAPESINOR

m AUTORITETI SHTETEROR PER INFORMACIONIN G
N

VleraGjeresiaE TrupitUjor
VeraOrigjing
VleraEllojeveTéKalimeve

VleraEgjendjesHidrologjike

VleraEllojitTéBregut

VleraEnivelitT&éUjrave

VleraEgjendjesSEObjektit
VleraEpozicionitVertikal
LidhjeePérgjithésuar
KalimetEklasaveTéNdara
Lidhjet

RénditjaElidhjeve
ElementétErrjetit

Nyje

Drejtitmillidhjeve

Hydro - Physical waters
Hydro - Physical waters
Hydro - Physical waters

Hydro - Physical waters

Hydro - Physical waters
Hydro - Physical waters

Generic Conceptual Model

Generic Conceptual Model
Generic Network Model

Generic Network Model
Generic Network Model
Generic Network Model
Generic Network Model
Generic Network Model

Generic Network Model

«dataType»
«codeList»

«codeList»
«codeList»

«codeList»

«codeList»

«codeList» imported

«codeList» imported

«featureType» imported

«featureType» imported
«featureType» imported
«featureType» imported
«featureType» imported
«featureType» imported

«dataType» imported

A. Vlera e gjéndjes sé objektit — (ConditionOfFacilityValue) - Kodlisté

| VleraEGjéndjesS¢Objektit

Perkufizim | Statusi injé objekti né lidhje me pérfundimin e tij dhe pérdorimin.

| Link | urn:x-inspire def:codeList: INSPIRE:ConditionOfFacility Value
| | Viera | Vlerat e lejuara pér kéts kodlists jans vlerat e specifikuara né tabelén e méposhtme.
| TéPashfrytézueshme — (disused)
[ Emri: Té&Pashfrytézueshme

| Perkufizimi: | Objektit nuk éshté mé i shfytézueshém por nuk &shté akoma nxjerrs jashté pérdorimit.
| Funksionale — (functional) ‘
|| Emri: | Funksionale
|| Perkufizimi: Objekti éshté funksional.
‘ Projektuar — (projected)
| Emri: Projektuar

| Perkufizimi: | Objekti po projektohet. Konstruksioni nuk éshté 1 ndértuar akoma.

| NéKonstruksion — (unde;'Constru ciion)

Emri:

NéKonstruksion
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| Pérkufizimi: | Objekti éshté né konstruksion e sipér por akoma jo funksional.
JashtéPérdorimit — (decommissioned)
Emri: JashtéPérdorimit
Pérkufizimi: Objekti nuk éshté mé né pérdorim ose éshté jashté pérdorimit.

B. Vlera e Pozicionit Vertikal — (VerticalPositionValue) - Kodlistg

VleraEpozicionitVertikal

Perkufizim Pozicioni relativ vertikal i njé objekti hapsinor.
Link -
Vlera Vlerat e lejuara pér kété kodlisté jang vlerat e specifikuara né tabelén e méposhtme.

NéSipérfaqe — (onGroundSurface)

Emri: NéSipérfage

Pérkufizimi: Objekti hapsinor ndodhet né sipérfage.
PezullOseNgritur — (suspendedOrElevated)

Emri: PezullOseNgritur

Pérkufizimi: Objekti hapsinor ndodhet pezull apo 1 ngritur.
NénToké — (underground)

Emri: NénT oké

Pérkufizimi: Objekti hapsinor éshté nén toké.

C. Lidhje e Pérgjithésuar — (GeneralisedLink)

LidhjeEpérgjithésuar
Pérkufizimi: Njé lloj baze abstrakte qé pérfagéson njé element linear ré rrjetit q& mund té pérdoret
sinjé objektiv né referenca lineare.
Pérshkrimi: -
Tipi i elementit <<featureType>>
Gjeometria Abstrakt
Lidhet me ElementetErrjetit

D. Kalimet e Klasave t§ Ndara — (Grade Separated Crossing)

KalimetEklasaveTeNdara

Peérkufizimi:

Tregues, ku dy ose mé shumé elementé q& ndérpriten jané poshté dhe lart, i cili
pérdoret nése kuota nuk &shté e pércaktuar apo e besueshme.

Pérshkrimi:

Shénim 1:

Né shumicén e rasteve, numri i elementéve éshté dy

Shénim 2:

Zakonisht, kjo éshté kur elementét ndrpriten me koodrinata plane xy kur vlera e
koordinatés y nuk éshté e pércaktuar apo nuk éshté mjaftueshém e sakté.

Tipi i elementit <<featureType>>
Gjeometria Abstrakt
Lidhet me ElementétErrjetit
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E. Lidhjet - (Link)

Lidhjet
Pérkufizimi: Njé element linear 1 lakuar i rrjetit g& lidh dy pozicione dhe pérfagéson njé rruggé
homogjene né rrjet. Pozicionet e lidhura perfagésohen si nyje.
Pérshkrimi:
Tipi i elementit <<featureType>>
Gjeometria Abstrakt
Lidhet me LidhjeEpérgjithésuar

Atributi: GeometriaEaksit - (centerlineGeometry)

Pérkufizimi:

Gjeometria gé pérfagéson aksin e lidhjes

Pérshkrimi

Lloji i vlerés

Linjé - GMCurve

Vlerg Shémbull

Shuméllojshméria

1

Detyrueshme

Po

Atributi: Fiktiviteti — (fictitious)

Pérkufizimi: Tregues se gjeometria e aksit té lidhjes éshté njé vijé e drejté pa pikat e kontrollit t&
ndérmjetme - pérveg nése vijé t& drejté pérfagéson gjeografing né zgjidhjen e t&
dhénave té pércaktuara né ményré t& pérshtatshme.

Pérshkrimi -

Lloji i vlerés Text

Vleré Shémbull -

Shuméllojshméria: 1

Detyrueshme Po

F. Rénditja e Lidhjeve — (LinkSequence)

Lidhjet
Peérkufizimi: Nje element 1 rrjetit, i cili pérfagéson njé rrugé té vazhdueshém né rrjet pa asnjé
degézim. Elementi ka njé fillim dhe fund t& pércaktuar dhe ¢do pozicion né rénditjen
e lidhjes &shté e identifikueshme me njé parametér t& vetém té tilla si gjatésia.
Pérshkrimi: Shémbull: Njé rénditje lidhjeje mund té pérfagésojé njé rrugé.
Tipi i elementit <<featureType>>
Gjeometria Abstrakt
Lidhet me LidhjeEpérgjithésuar
Atributi: Lidhje - (link)
Pérkufizimi: Rénditja e lidhjeve t& drejtuara gé konsistojné né rendin e lidhjes.
Pérshkrimi

Lloji i vlerés

Drejtimillidhjeve - datatype

Vlerg Shémbull

Shuméllojshméria:

1

Detyrueshme

Po

67|Faqe





image68.jpeg
AS'@ AUTORITETI SHTETEROR PER INFORMACIONIN GJEOHAPESINOR

G. Elementet e Rrjetit — (NetworkElement)

ElementetErrjetit
Pérkufizimi: Njé lloj baze abstrakte qé pérfagéson njé element né rrjet. Cdo element né njé rrjet
siguron njé funksion q& éshté me interes.
Pérshkrimi: -
Tipi i elementit <<featureType>>
Gjeometria Abstrakt
Lidhet me -

Atributi: FillimilJetégjatésisé - (beginLifespanVersion)

Pérkufizimi: Data dhe ora kur ky version i késaj vlere éshté hedhur ng sistem.
Pérshkrimi -

Lloji i vlerés Data Ora

Vleré Shémbull

Shuméllojshméria: 1

Detyrueshme Po

Atributi: MbarimilJetégjatésisé - (endLifespanVersion)

Pérkufizimi: Data dhe ora kur ky version i vlerés éshté hequr nga sistemi.
Pérshkrimi
Lloji i vlerés Data Ora
Vleré Shémbull
Shuméllojshméria: 0.1
Detyrueshme Jo
Atributi: Inspireld — (inspireld)
Pérkufizimi: Identifikues i jashtém pér objektin
Pérshkrimi Eshté njé identifikues unik i objektit, i publikuar nga organi pérgjegjés, i cili mund

té pérdoret nga aplikacionét e jashtém pér tu referuar objektit hapésinor.

Lloji i vlerés

Identifikues (ID)

Vlerg Shémbull

Shuméllojshméria:

0.1

Detyrueshme

Po

H. Nyje — (Node)

Nyje
Pérkufizimi: Pérfaqéson njé pozicion té réndésishém né rrjet qé gjithmoné ndodh né fillim apo né
fund t8 njé lidhje.
Pérshkrimi: Nyja éshté njé element pérfagésues 1 topologjisé sé rrjetit, pér bashkimin e dy apo mé

shumé lidhjeve. N& topologjing e njé rruge nyjet pérfagésohen me pika apo forma
gjeometri té tjera respektive.

Tipi i elementit <<featureType>>
Gjeometria Abstrakt
Lidhet me -

Atributi: gjeometria — (geometry)

Pérkufizimi: Pozicionimi i nyjes
Pérshkrimi -

Lloji i vlerés Piké (GM-point)
Vleré Shémbull -
Shuméllojshméria: 1

Detyrueshme Po
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I. Drejtimi i Lidhjeve — (DirectedLink)

Drejtimillidhjeve
Pérkufizimi: Drejtimi i lidhjes si né dretjim pozitiv apo negativ.
Pérshkrimi: -
Tipi i elementit <<datatype>>
Gjeometria Abstrakt
Lidhet me -
Atributi: Drejtimi — (direction)
Pérkufizimi: Pércakton nése drejtimi 1 lidhjeve pérshtatet (pozitive) apo nuk pérshtatet (negative)
me dretjimin e linjés
Pérshkrimi -
Lloji i vlerés Shenjé
Vleré Shémbull -
Shuméllojshméria: 1
Detyrueshme Po
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43.

KODI EPSG PER KRGJSH 2010

Intemafional Assoclation of Detailed Report on Projected
Oll and Gas Producers .
EPSG geodatic paviueters Coordinate Reference Systems
data set version 854 Search Criteria: 6870
#1  Code: 6570 Name: ETRS89 / Albania 2010
Albania alternative identifier: KRGISH-2010
Base GeogCRS: ETRSS9 e
Geodetic Datum: European Terrestrial Reference System 1989 Order  Axis Name Abbr Axis Units Orientation
Ellipsoid: GRS 1980 1 Northing X metre north
2 Easting ¥ metre cast
CS remarks: Used in projected and engineering coordinate reference systems.
Semi-major axis @) = 378137 metre

Inverse flattening (1/f) = 298 257222101 Map Projection:  Albania 2010
Projection Method: Transverse Mercator
Prime Meridian: Greenwich
L ¢ Parameter Name or Value Init of Meas
Datum origin: Fixed to the stable part of the Eurasian continental plate and Laramerer Value Lnit of Measure
consistent with ITRS at the epoch 1989.0. Latitude of natural origin o 0 L R ]
Datum remarks: The distinction in usage between ETRFS9 and ETRSE9 is Longitude of natural origin 20° 0 0" E
confused: although in principle conceptually different in Seale factor at natural origin 1 unity
practice both are used for the realisation.
Falsc casting 500000 metre
CRS scope. Large and medium scale topographic mapping. cadastral False northing 0 metre
and engineering survey.
CRS remarks: Planimetric component of Albanian Geodetic Reference Framework
(KRGJSH) 2010.
Projection remarks: Planimetric component of Albanian Geodetic Reference Framework
(KRGISH) 2010.
CRS info. source: State Authority for Geospatial Information (ASIG). Data source: OGP Revision date: 18-Sep-14  Change id: 2014.008 2014.065
CRS area of use: 3212 Albania - onshore.

EPSG geodesy parameters. Version: 854 of 18 Scptember 2014

Projected Coordinate Reference Systems (detailed)

Printed on:

28-Oct-14
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