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VENDIM
Nr. 321, datë 27.4.2016

PËR MIRATIMIN E DOKUMENTIT “STANDARDET SHTETËRORE PËR SPECIFIKIMET TEKNIKE TË INFORMACIONIT GJEOHAPËSINOR NË SHQIPËRI - TEMA: PARCELAT KADASTRALE”

Në mbështetje të nenit 100 të Kushtetutës dhe të neneve 11, pika 2, shkronja “e”, dhe 16, pika 1, të ligjit nr.72/2012, “Për organizimin dhe funksionimin e Infrastrukturës Kombëtare të Informacionit Gjeohapësinor në Republikën e Shqipërisë”, me propozimin e ministrit të Shtetit për Inovacionin dhe Administratën Publike, Këshilli i Ministrave

VENDOSI:

1. Miratimin e dokumentit “Standardet shtetërore për specifikimet teknike të informacionit gjeohapësinor në Shqipëri - Tema: Parcelat kadastrale”, sipas tekstit që i bashkëlidhet këtij vendimi dhe është pjesë përbërëse e tij.
2. Ngarkohen ministri i Shtetit për Inovacionin dhe Administratën Publike, Autoriteti Shtetëror për Informacionin Gjeohapësinor (ASIG) dhe autoritetet përgjegjëse për krijimin, ruajtjen dhe përditësimin e të dhënave gjeohapësinore, për ndjekjen dhe zbatimin e këtij vendimi.
Ky vendim hyn në fuqi pas botimit në Fletoren Zyrtare.
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1. PERSHKRIM MBI STANDARDIN

Ky dokument pérmban standardet e specifikimeve teknike té té dhénave gjeohapésinore pér ndértimin e NSDI, duke
u mbéshtetur né Direktivén INSPIRE. Autori i kétij produkti éshté Autoriteti Shtetéror pér Informacionin
Gjeohapésinor (ASIG) dhe né bashképunim me INSTAT, Drejtoriné ¢ Pérgjithshme 8 Gjendjes Civile,
ZQRPP dhe ALUIZNI-n. Data e publikimit t& versionit Nr.1 éshté Tetor 2015. Emértimi i dokumentit éshté:
ASIG_Standard NSDI 2015 PK v.1 ku:

ASIG — Autoriteti pérgjegjés pér krijimin e standardit

Standard — Lloji 1 dokumentit

NSDI - Qéllimi 1 dokumentit

2015 — Viti 1 krijimit

PK — Tema pér t& cilén éshté krijuar standardi: Parcelat Kadastrale.
v.1 — Numri i versionit t& standardit

2. HYRJE

2.1. SILEXOHET DOKUMENTI

Ky material &shtg i strukturuar ng katér kapituj kryesoré:

1-
2-

B
4-

Pérshkrim mbi standardet — N& kété pjesé jepen emértimi dhe autori i standardeve.

Hyrje — N& kété pjesé jepen pérshkrime dhe shpjegime pér t& kuptuar ményrén si organizohet i
gjithg informacioni dhe si mund t& kuptohet mé lehté.

Tema — N& kété pjesé jepen specifikimet teknike pér secilén temé.

Anekse — N& kété pjesé jepen informacione shtesé shpjeguese né ndihmé t& lexuesve.

Pérmbajtja ¢ Kapitullit 3 &shté strukturuar ng 6 pjesé kryesore:

1-
2-
3-
4-
5-

6-

Pérshkrimi i temés — Kétu flitet né ményré t& pérgjithshme pér pérmbajtjen e temés.
Diagramat UML — Kétu jepet pérmbajtja e Katalogut t& Tipologjive pérkthyer sipas gjuhés UML.
Katalogu i Tipologjive — Kétu shpjegohet struktura ¢ temés me t& gjithe elementét e saj pérbérés.
Metadata — Kétu jepen specifikimet teknike pér metadata-t ¢ temés pérkatése.

Sistemi Koordinativ referencé — Kétu pécaktohet sistemi koordinativ referencé q& &shté i
miratuar sipas vendimit Nr,669 daté 7/8/2013 .
Cilésia e té dhénave —Kétu jepet njé pérshkrim mbi cilésing e t& dhénave t& elementéve dhe matjes
s€ tyre.

Diagramat UML ofrojné njé¢ ményré t& shpejté pér t& paré clementst kryesoré t& specifikimeve dhe
marrédhéniet mes tyre. Pérkufizimi mbi llojin ¢ objektit hapésinor, atributet dhe marrédhéniet jang t&
pérfshira né Katalogun ¢ Tipologjive (Feature Catalogue). Personat t& cilét kang ekspertizé tematike por
nuk jang t& familjarizuar me UML-n& mund t& kuptojné plotésisht pérmbajtjen ¢ modelit t& t& dhénave duke
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u fokusuar tek Katalogu i Tipologjive. Pér pérdoruesit, Katalogu i Tipologjive mund t& jeté veganérisht i
dobishém pér t& kontrolluar n&se ai pérmban t& dhénat ¢ nevojshme pér aplikacionet q& ata pérdorin.

N& tabelat e m&poshtme jepet njé shpjegim mbi pérmbajtjen dhe ményrén e organizimit t& informacionit né
tabelat e t& dhénave né Katalogun e Tipologjive.

Tabela Nr.1, 2, me ané t& njé shablloni, shpjegon ményrén e organizimit t& informacionit n& tabelén e
tipologjive dhe t& atributeve t& tyre.

Tabela Nr.3, me ané t& njé shablloni, shpjegon ményrén ¢ organizimit t& informacionit né tabelén ¢ kod

list&s.

Tabela 1

Emri - Emértimi 1 tipologjisé

Pérkufizimi:
Pérshkrimi:
Tipi 1 tipologjisé

Gjeometria

Shuméllojshméria:

Detyrueshme

Lidhjet

Pérkufizimi sipas direktives INSPIRE pér tipologjiné.

Shénime dhe pérshkrime t& tjera pér tipologjing.

Tipi i elementit i cili mund t& jets i kétyre llojeve:

«featureType» - njéelement i cili mund té jeté real né terren apo njé fenomen abstrakt

«dataType» - njé element tabelor i cili shérben vetém si tabelé atributesh pér tu
lidhur me njé element tjetér. N& document gjendet e shqipéruar si
‘tipet e t& dhénave’

«enumeration» - listé e parapérgatitur vlerash ku elementi duhet t& marré vleré.
«codeList» Enumeration nénkupton “renditje vlerash”, ndérsa codeList nénkupton

“listé vlerash ose ndryshe kod lists”. Né dokument gjenden e
shqipéruara ‘Numértimet dhe kod listat’

«Imported» - t& dhéna té specifikuara né tema té tjera t& direktivés INSPIRE. Né
document gjendet e shipéruar si ‘Té dhénat e importuara’

Gjeometria e elementit sipas formatit vektor mund t& gjendet né tre forma: piké, linjé
ose poligon.
Abstrakt — kur elementi nuk &shté element real né terren por konsiderohet vetém si
fenomen.
Lloji dhe numri i vlerave qé mund t& marré atributi:
0..* - mund t& marré shumé lloje vlerash ose asnjé vleré
1% - mund té marré minimum 1 vleré ose shumé vlera
0..1 - mund t& mos marré asnjé vleré ose nése merr vleré, duhet t& marré vetdm 1 vleré té
vetme.
1 - duhet t& marré detyrimisht 1 vleré
Po —nése atributi &shté i detyrueshem té plotésohet
Jo —nése atributi nuk &shté 1 detyrueshém t& plotésohet
Né tabelén e lidhjeve “LIDHIET” tregohen marrédhéniet hierarkike ndérmjet elementéve
té ndryshém né kété temé po ashtu dhe né temat e tjera. Kéto marrédhénie pasqyrojné
lidhjet gé realizohen né skemat UML.
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Tabela 2

ATRIBUTET

-- Emri --
Emértimi i atributit.

- Pérkufizimi --
Pérkufizimi sipas direktivés INSPIRE té elementéve.

-- Pérshkrimi --

Shénime dhe pérshkrime t& tjera pér elementin.

[ Detyrueshme : Detyrueshméria nése atributi duhet t& marré vleré p.sh: PO]

Tabela 3
ATRIBUTET

¢ Vlera e paré e listés sé gatshme p.sh: Ligjor

-- Emri --
Emértimi i vlerés.

- Pérkufizimi --
Pérkufizimi sipas direktives INSPIRE té elementéve.

¥ Vlera e dyté (etj) e listés sé gatshme p.sh: Jo Ligjor

-- Emri --
Emértimi i vlerés.

- Pérkufizimi --
Pérkufizimi sipas direktivés INSPIRE té elementéve.

2.1.1. KARAKTERISTIKAT E <<VOIDABLE>> DHE SHUMELLOJSHMERIA.

Stereotipi <<voidable>> pérdoret pér t& pérshkruar ato pérkatési t& objekteve hapésinore té cilat mund t&
jené ose mund t& mos jené prezenté né grupet e t& dhénave hapésinore, edhe pse ato mund t& ekzistojné né
botén reale. Kjo nuk do t& thoté q& kétyre pérkatésive duhet ti jepet njé vlers.

Pér t& gjitha pérkatésité e pércaktuara pér objektet hapésinore duhet té paraqitet njé vleré — ose vlera
pérkatése (nése éshté e disponueshme né grupin ¢ t& dhénave q& mirémbahet nga ofruesi i t& dhénave) ose
vlera ‘void’. Njé vleré& void nénkupton q& nuk ekziston njé vlerg pérkatése né grupet ¢ t& dhénave hapésinore
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q& mirémbahen nga ofruesi i t& dhénave ose q& asnjé vleré pérkatése nuk mund t& nxirret nga vlerat
ekzistuese me kosto t& arsyeshme.

Arsyeja e pérdorjes s& vlerés void duhet t& paraqitet kurdo t& jeté e mundur duke pérdorur njé nga vlerat e
listuara n& kod listén VleraE ArsyesSéPavlefshmérisé (VoidReasonValue).

Stereotipi <<voidable>> nuk jep informacion nése karakteristika ekziston ose nuk ckziston né botén reale.
Kjo shprehet duke pérdorur shuméllojshméring:

Nése njé karakteristike mund t& ckzistojé apo mund t& mos ekzistojé né botén reale, vlera minimale do t&
pércaktohet si 0. Psh nése njé adresé ka apo nuk ka nj& numér shtépie, shuméllojshméria pérkatése do t&
jet& 0..1.

Nése pér njé karakteristiké t& caktuar ekziston t& paktén njé vleré né botén reale, vlera minimale do t&
pércaktohet si 1. Psh nése njé njési administrative ka gjithmoné t& paktén njé emér, shuméllojshméria
pérkatése do t& jete 1..*.

2.1.2. RENDITJET DHE KOD LISTAT (ENUMERATION AND CODELIST).

Kod listat modelohen si klasa né skemat e aplikimit por vlerat e tyre menaxhohen jashté skemave t&
aplikimit.N& kod list&, ‘vlera t& tjera’ pércakton llojin ¢ pérmbajtjes s& kod listés pércaktuar specifikisht si
m& poshts:

‘jo’ pérfaqéson kod lista q& pérmbajné vetém vlera té specifikuara ng kétg rregullore.

‘té kufizuara’pérfagéson kod lista t& pérmbajné vlera t& specifikuara né kété rregullore dhe vlera té tjera t&
limituara t& pércaktuara nga ofruesi i t& dhénave.

‘6 hapura’ pérfaqéson kod lista q& pérmbajné vlera t& specifikuara ng kété rregullore dhe vlera shtesé né
cdo nivel, t& pércaktuara nga ofruesi i t& dhénave.

‘po’ pérfagéson kod lista q& pérmbajné vlera t& pércaktuara nga ofruesi i t& dhénave.

Vlerat shtesé t& pércaktuara nga ofruesit ¢ t& dhénave nuk duhet t& z&véndésojné apo modifikojné vlerat
ekzistuese t& pércaktuara né rregullore.

N& rastin kur ofruesit e t& dhénave do & pérdorin kod lista me vlera jo t& pérmbajtura né rregullore, ofruesit
jang t& detyruar ti b&jné kéto vlera bashké me pérkufizimet e tyre, t& disponueshme né njé regjistér. Kjo do
t& mundésojé q& dhe pérdoruesit e tjeré ti kuptojné kéto vlera dhe t& kené mundési t’i pérdorin.

2.1.3. PARAQITJAE ASPEKTIT KOHOR.

Skemat e aplikimit pérdorin atributin “FillimilTetégjatésise” dhe “MbarimilJetégjatésise™ pér t& regjistruar
jetégjatésing e njé objekti hapésinor.

Atributi “FillimilJetégjatésise™ specifikon datén kur versioni i objektit hapé&sinor &shté futur apo ndryshuar
né grupin e t& dhénave hapésinore (ng sistem). Atributi “MbarimilJetégjatésise” specifikon datén kur
versioni 1 objektit hap&sinor &shté zévéndésuar apo térhequr nga grupi i t& dhénave hapésinore (né sistem).
Kéto vlera kohore nuk kang t& b&jné me karakteristikat kohore t& objektit né botén reale.
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Ndryshimet q& b&hen né atributin “MbarimilJetégjatésisé” nuk shkaktojné ndryshime né atributin
“FillimilJetégjatésise™.

g Shénim i réndésishém:

Disa terma né katalogun e tipologjive si p.sh: tipi i tipologjisé, etj, nuk jané pérkthyer qéllimisht né gjuhén
Shqipe. Qéllimi parésor &shté q& t& mos humbasé kuptimi gjaté pérkthimit dhe s& dyti t& pérdoret njé gjuhé
unike sipas termave t& Direktivés INSPIRE.





image7.jpg
2.2. DETYRIMET LIGJORE

Né bazé t& ligjit Nr 72/2012, neni 16, “Pér organizimin dhe funksionimin e Infrastrukturés Kombétare t& Informacionit
Gjeohapésinor né Republikén e Shqipérisé”, ASIG é&shté pérgjegjés pér krijimin e standardeve pér secilén nga temat
e pércaktuara né ligj (neni 11), né pérputhje me standardet europiane (direktiva INSPIRE).

Standardet teknike t& t& dhénave gjeohapésinore pér krijimin e NSDI né Shqipéri, jané pérshtatur nga specifikimet
teknike t& temave pérkatése né direktivén INSPIRE. Pér implementimin e direktivés, kérkohet qé té gjithé aktorét t&
implementojné disa standarde té pérbashkéta, té cilat mundésojné ndérveprimin e shérbimeve dhe harmonizimin e t&
dhénave.

Standardet (Rregullat e Implementimit (IR)) duhet t& krijohen pér fushat e méposhtme:

o Metadata — né kété fushé direktiva pércakton standardet sesi duhet té jené metadata-t. Ky standard éshté
unik dhe 1 aplikueshém pér té gjithé institucionet ose palét e treta (si¢ éshté e pércaktuar né fushén e veprimit té késaj
direktive), t& cilét do implementojné kété direktive.

0 Specifikimi i té¢ dhénave — standardet e késaj kategorie pérfshijné té gjitha atributet e objekteve té ndryshme
té cilat do t& publikohen. INSPIRE ka pércaktuar disa atribute si bazé e cila do té shérbejé pér publikimin e t& dhénave
té ndryshme. Vendet e ndryshme, né varési t& ligjeve ose nevojave té brendshme mund té shtojné atribute té tjera, pér
ti béré sa mé té pérdorshme t& dhénat. T& gjitha t& dhénat q& do t& shtohen duhet t& jené t& dokumentuara dhe t&
aprovuara nga autoritetet pérgjegjése lokale.

2.3. FUSHAE VEPRIMIT
Té& gjithé autoritetet publike, kompani private apo individét, té& cilét mbajné ose pérpunojné t& dhéna gjeohapésinore
pér llogari t& Institucioneve Publike, jané t& detyruar ti nénshtrohen késaj rregulloreje.

Bazuar né modelet e proceseve té biznesit, sistemi i propozuar nga direktiva INSPIRE ka proceset dhe ciklin jetésor
si mé poshté:

Shpemdarja Analizimi
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Figura 1

Planifikimi — Eshté procesi gjaté té cilit krijohen strukturat e té dhénave t& nevojshme pér té publikuar informacionin
né portal. Rezultatet e kétij procesi jané modelet e ndryshme té t& dhénave.

Vlerésimi — Eshté procesi gjaté té cilit té dhénat ekzistuese testohen kundrejt modelit. Rezultati i kétij procesi do jeté
certifikimiité dhénave ose nevoja pér té modifikuar t& dhénat pér tu pérshtatur me modelet e pércaktuara gjaté procesit
té vlerésimit.

Procesimi — Eshté procesi gjaté té cilit mblidhen dhe manipulohen atributet e té dhénave pér té prodhuar informacion
kuptimploté. Manipulimi i tyre béhet kundrejt modeleve té pércaktuar gjaté planifikimit. Rezultatet e kétij procesi,
jané bashkési t& dhénash t& cilat jang gati pér tu publikuar.

Shpérndarja — Eshté procesi gjaté té cilit té dhénat vihen né dispozicion pér pérdoruesit (Qytétarét, Autoritetet
publike, Organizatat ose Palét e treta). Pérdoruesi mund té shkarkojé, pérdoré, analizojé ose té citojé ato. Publikimi 1
té dhénave bazohet né modelet e ndryshme t8 pérdorimit.

Zbulimi — Eshté procesi i vazhdueshém mbi té dhénat e publikuara, gjaté té cilit zbulohen té dhéna té reja ose té dhéna
jo cilésore.

Analiza - Eshté procesi i analizimit té t& dhénave té evidentuara né fazén e zbulimit. Gjaté kétij procesi merret vendimi
cfaré do béhet mé té dhénat qé jané evidentuar.

Pérditésimi — Eshté procesi kur propozohet shtimi, modifikimi ose fshirja e té dhénave. Ky proces rregjistrohet nga
procesi i analizimit t& t& dhénave ekzistuese dhe t& publikuara.

Arkivimi - Eshté procesi gjaté té cilit, bashkésité e té dhénave qé nuk nevojiten té aksesohen, arkivohen duke u bazuar
né standarde lokale dhe n€ legjislacionin né fuqi t& vendeve ku implementohet. Rezultati i kétij procesi jané t& dhénat
té cilat béhen té pa aksesueshme pér publikun, me akses vetém nga autoritetet specifike. Kéto t& dhéna vazhdojné té
ruhen pér arsye té pérputhshmérisé me kuadrin ligjor né fuqi ose standardet specifike.

Shkatérrimi — Eshté procesi gjaté té cilit, t& dhénat béhen té pa rikuperueshme. Ky proces bazohet né standarde lokale
ose legjislacione né fuqi.
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3. TEMA

31 PARCELAT KADASTRALE
3.1.1. PERSHKRIMI I TEMES

Tema ‘Parcelat kadastrale’ sipas direktivés INSPIRE &shté pérfshiré ng Aneksin I, ndérsa sipas Ligjit
Nr 72/2012 &shté prioritet, g€ nénkupton se konsiderohen si t& dhéna referencé, d.m.th. t& dhéna g8 pérbéjng
kornizén hapésinore pér lidhjen dhe/ose orientimin tek informacione té tjera, q& i pérkasin fushés specifike
tematike si mjedisi, dheu, pérdorimi i tok&s dhe shumé té tjeré.

Procesi

Specifikimet teknike ¢ t& dhénave gjeohapésinore pér parcelat kadastrale jané pérgatitur duke
ndjekur parimin ¢ pjesémarrjes né procesin ¢ ndértimit t& konsensusit. Palét e interesuara, sipas grupit t&
punés, patén mundésing pér t& paraqitur kérkesat e pérdoruesve dhe materiale referencash, propozimet e
ekspertéve pér krijimin e specifikimeve dhe t& mermmin pjesé né rishikimin e kétyre specifikimeve t& t&
dhénave. Grupi Tematik i Punés pérgjegjés pér zhvillimin e specifikimit pérbéhej nga eksperté, & vinin
nga institucionet pérgjegjése.

Themeli i zhvillimit t& specifikimit ishte pércaktimi i Direktivés pér parcelat kadastrale: “zonat e
pércaktuara nga parcelat kadastrale ose t& barasvlershme me to”. N& p&rputhje me sistemin ligjor ¢do Shtet
Anétar mban njé regjistér pérkatés nén pérgjegjésing e qeverisé. Regjistra t& tille quhen regjistri i pasurisé
& paluajtshme, ku njésia bazg &shté parcela kadastrale. Parcelat kadastrale zakonisht formojné njé ndarje
t& vazhdueshme t& territorit kombétar me pérjashtim t& rasteve kur disa toka nén zotérimin e qeverisé nuk
i nénshtrohen regjistrimit.

Pérkufizimi i pérgjithshém i parcelave kadastrale &shté plotésuar nga Grupi Tematik i Punés pér t’u
pérshtatur mé miré me kérkesat ¢ pérdoruesit sipas ményrés vijuese: parcelat kadastrale, aty ku &shté e
mundur, duhet t& jeng zona t& vetme t& sipérfaqes s& tokés (toké dhe/ose ujé) sipas t& drejtave t& pasurive
t& paluajtshme homogjene dhe pronésisé unike, ku t& drejtat e pasurive t& paluajtshme pércaktohen nga
ligjet kombétare.

Ky dokument nuk synon t& harmonizojé parimet e pronésisé dhe t& drejtat q& lidhen me parcelat, por
pérqendrohet ng aspektet gjecometrike si¢ paragiten né sistemin kombétar.

Modeli i t& dhénave pér parcelat kadastrale &shté pérgatitur né njé ményré, qé mbéshtet pérputhshméring
me standardin ndérkombétar t& ardhshém mbi Modelin e Sferés s& Administrimit t& Tokés. Modeli i Sferés
s& Administrimit t& Tok&s (MSAT) siguron njé kontekst mé & gjeré pér Parcelat Kadastrale sepse MSAT
pérfshin informacione shtesé mbi t& drejtat (t& detyrueshme pér legjislacionin kombétar) dhe pronarét.

Elementi thelbésor i modelit t& parcelave kadastrale t& kétij standardi &shté vet parcela kadastrale. Ajo
pérshkruhet nga disa elementé t& detyrueshém si gjeometria, identifikuesi unik, referenca kadastrale dhe
etiketimi i parcelave, q&¢ mbéshtet identifikimin e tyre né hartat ¢ shtypura.
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Si konkluzion, vlera kryesore e modelit t& Parcelave Kadastrale &shté struktura e saj e thjeshté, por
fleksibél q& iu mundéson ofruesve t& t& dhénave publikimin e t& dhénave ckzistuese né ményrén mé té
volitshme t& mundshme.

Pér temén ‘Parcelat Kadastrale’, termat vijues jané pérkufizuar né ményré specifike si méposhté:

= Boshlléku kadastral

Zong q& nuk &shté menduar t& mbulohet me parcela kadastrale pér shkak t& rregullave kombétare.
*Shénim: Nuk duhet ngatérruar me zona ende t& pastudivara dhe t& paregjistruara.

SHEMBULL: né shumé vende, deti tj.

L] Mbivendosja kadastrale

Zong q& mund t& mbulohet me disa parcela kadastrale pér shkak té rregullave kombétare.

SHEMBULL: N& Mbretéring ¢ Bashkuar, parcelat e mbivendosura mund t& ndodhin aty ku jang regjistruar
t& drejta t& ndryshme né t& nj&jtén hapésirg, d.m.th. njé e drejté absolute dhe njé proné e dhéné me qira.

. Boshllgku topologjik
Zong q& &shté e mbuluar me parcela kadastrale né terren, por jo né dataset-in hapésinor.

SHEMBULL: Boshlléqet topologjike mund t& ndodhin kur kryhet grumbullimi i parcelave kadastrale nga
disa sipérfaqe kadastrale ose pas shndérrimit t& formatit.

Ll Mbivendosja topologjike

Zong q& &shté ¢ mbuluar vetém me njé parcelé kadastrale né terren, por nga disa parcela né setin ¢ t&
dhénave hapésinore.

SHEMBULL: Mbivendosjet topologjike mund t& ndodhin kur kryhet grumbullimi i parcelave kadastrale
nga disa sipérfaqe kadastrale ose pas shndérrimit t& formatit.
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3.1.2. DIAGRAMAT UML

3121

«applicationSchema»
Parcelat Kadastrale

SKEMA E APLIKIMIT TE ‘PARCELAT KADASTRALE’

«applicationSchema»
Emértimet Gjeografike

E + KufijtéKadasgtral
a + NjésiaBaz&EPronés

g + ParcelatKandagtrale
a + ZonaKadasdrale

S + VleraENivelitT éZonésKadastrale

S + EmértimetGjeografike

g + EmértimilVedit

g + GermézimilEmrit

g + VleraEPrejardhjes

g + VleraE StatusitT éEmrit

S + VleratEGjiniséGramatikore
+ VleraT em &sS&Emrit

S + VleratENumritGram atikor

N
«applicationSchema»
Lloji Bazé

7
(from Emértimet Gjeografike)

g + TeDhé&natHapsinore

g + VleraEKushtitT éObjekit
+ VleraEPozicionimitVertikal

S + VleraEArsyesSéPaviefshmériss

(from Lioji Bazé)

Figura 2 - Lidhja e Skemés sé aplikimit sé Parcelat Kadastrale’ me té tierat.

3.1.22. NUMERTIMET DHE KOD LISTAT

«codelist»
Parcelat Kadastrale::
VleraENiv elitTéZonésKadastrale

+ o+ o+ o+

Rendi1
Rendi2
Rendi3
Rendi4

Figura 2 - Enumerations & codelists
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3.1.23. TIPOLOGIJIA E TEMES ‘PARCELAT KADASTRALE’

+NivelilNjésissM&TéL arté
«voidable» 0..1

feature Type»
Parcelat Kadastrale:ParcelatKandastrale «feature Type»
Parcelat Kadastrale:ZonaKadastrale

+ Gjeometria: Poligon
+ Inspireld: Identifikues + Gjeometria: Poligon
+ NumrilPasurisé: CharacterString + Inspireld: Identifilues [0..1]
+ ReferencaKombétareKadastrale: CharacterString + NumrilPasurisé: CharacterString
«voidable» + ReferencaKombétareEZonésKadastrale: CharacterString|
+ EvlefshmeDeri: Daté [0..1] «voidable»
+ EvlefshmeNga: Daté [0..1] ‘+Z°"6Kada% + EméntesaEHartésNgShkallénOrigjinale: Integer [0..1]
+ PikaReferené: Piké [0..1] «oidable» o 1|+ Eméttimi: EménimetGjeografike [0..]
+ VleraEsipétfages: Sipéifage [0..1] [+ EmriNiveli: Characterstring [1..]
«lifeCyclelnfo, voidable» + EVlefsnmeDeri: Daté-Oré [0..1]
+ Fillimiljetsgjatésisé: Daté + EVlefshmeNga: Daté-Oré [0..1]
+ Mbarimiljetégjatésis: Dats [0..1] + Niveli: VieraENivelitTéZonésKadastrale

“ + PikaReferencé: Piké [0..1]

+ SakésaELlogaritur: Gjatési [0..1]

«lifeCyclelnfo, voidable»
+ Fillimil Jetégjatésisé: Daté
+ Mbarimil Jetégjat

+Parcela 1.2
«voidable»

«feature Type»
Parcelat Kadastrale::KufijtéKadastral

+ Gjeometria: Linjé

+ Inspireld: Identifikues[0..1]
«voidable»

+ EvlefshmeDeri: Dats-Oré [0..1]

+ EvlefshmeNga: Daté-Oré [0..1]

+ SaMésaELlogaritur: Gjatési [0..1]
«lifeCyclelnfo, voidable»

+ FillimilJetégjatésiss: Daté

+ MbarimilJetégjatésisé: Daté - Oré [0..1]

Figura 3 - Feature type — Tipologjia e temés ‘Parcelat Kadastrale’
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3.1.24. TE DHENAT E IMPORTUARA

«featureType»
Parcelat Kadastrale::Parcelatiandastrale

+NjesteAdminisrative
«oidable»

Gjeometria: Poligan

Inspireld: Identifilues

NumiilPasurise: CharacterString

ReferencakombetareKadastrale: CharacterSting
«voidable»

EvlefshmeDeri: Date [0..1]

EvlefshmeNga: Date [0..1]

PikaReferene: Pike [0..1]

VleraEsiperfanes Siperfage [0.1]

o

«lifeCydlelnfo, voidable»
+ Fillimiljetegjatesise: Date
+ Mbarimiljetegjatesise: Date [0..1]

constraints
{LiojilGjeametrise}
leraESiperfagesoM}
{EVlefshmeDer}
MbarimilJetegjatesise)

+Parcela
«oidahle»

N

o

«featureType»
Parcelat Kadastrale::KufijtéKadastral

+ Gjeometia: Linje

+ Inspireld: Identifilues[0..1]
«aidablen

+  EvlefsimeDeri: Date-Ore [0..1]

+ EvlefsimeNga: Date-Ore [0..1]

+ SakesaELlogaritur Gjatesi [0.1]
«lifeCyclelnfo, vaidable»

+ Fillimil etegjatesise: Date

+ MhanimilJetegjatesiss: Date - Ore [0..1]

constraints
{SakesiaELlogaritutJoM}
EViefsmeDer}
Mbarimilletegjatesiss}

+ZonaKadasrale
«oidable»

i

I
;
B
| Tl
i
i
)
i

+Parcelé
«aidahle»

«featureType»
Njésité Administrative:Nj&sitéAdministrative

+ Emertimi: EmertimetGjeografike [1.7]

+ Gjeometia: Poligan

+ |dAltemative: ldLokale

+ Inspireld: Identifilues

+ KodiKombetar. CharacterString

+ NiveliNacional: Hierard aENjesiveAdministative
+ Shteti: KodilShtetit
«aidablen

+  Autoriteti Gendror. AutoritetiQendror [1.7]

+ EmertimiNacionallnivelit CharacterSting [1.7]
«aidable, lifeCyclelnfoy

+ Fillimil Jetegjatesis¢: Date

+ Mhanimilletegjatesise: Date [0.1]

constraints
iveliMelLartelNesissAdministrative}
NiveliMelUletiNjesissAdminisrative}

«leatureTypen
Parcelat Kadastrale:ZonaKadastrale

Gjeometria: Poligan
Inspireld: |dentifilues(0..1]

NumiilPasurise: CharacterString
ReferencakombetareEZoneskadastrale: CharacterSting

=
5
o
.

«oidable»
EmertesaEHartesNeShkallenOrigjinale: Integer [0..1]
Emertimi: EmertimetGjeagrafike [0.7]

ErmnrilNiveli: CharacterSting [1.7]
EVlefshmeDeri: Date-Ore [0..1]
EVlefshmeNga: Date-Ore [0..1]

Niveli: VieraENivelitTeZongsKadasrale
PikaReference: Pike [0.1]
SakiesiaELlogaritur: Gjatesi [0..1]

difeCyclelnfo, voidable»

+ Fillimilletegjatesiss: Date

+ MhbarimilJetegjatesise: Date [0..1]

1

constraints
{Hierari aENivelitT eZonesadastrale}
{SaktesiaELlogariturUoM}
{EVlefshmeDeri}
MbarimilJetegjatesiss)

+NivelilNjesiseM eTeLarte

waidable» 0.1

eatureTypen
SistemilAdresav e:Adresa

+ Inspireld: |dentifilues
+ Lokalizues IdentifiluesilAdresss[1.7] fordered)
+ Pozicionimi: PazicionimiGjeografik[1.7]
«oidable, lifeCyclelnfay

+ FillimilJetegjatesise: Date

+ MbarimilJetegjatesis2: Date [0..1]

«oidabler

+ Identifikuesaltemativ: CharacterString [0..1]
+ Statusi: VieraEStatusit [0..1]
+ validFrom: Date-Ore
+ validTa: Date-Ore [0..1]

constraints
VendodhjaEAdreses
Mbarimilletegjatesiss}
{OytetiAdreses)

Figura 4 - Lidhja e Parcelave Kadastrale me Adresat dhe Njesité Administrative.
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«dataType»

dataT:
Emértimet Gjeografike::EEmértimetGjeografike “iaalnee

Emértimet Gjeografike::GermézimilEmrit

+ Gemézimi: GermézimilEmrit [1..%] + Teksti: CharacterString
«voidable»

+ SkemaEKonvertimit: CharacterString [0..1]

+ SkiptilAlfabetit: CharacterString

«voidable»
GjiniaGramatikore: VleratEGjinisé Gramatikore [0..1]
Gjuha: CharacterString
NumriGramatikor: VleratENumritGramatikor [0..1]
OrigjinaEEmrit: CharacterString

Prejardhja: VleraEPrejardhjes
StatusilEmrit: VleraEStatusitT€Emrit

+ o+ o+ o+ o+ o+

Figura 5 — T¢ dhénat e importuara nga tema: Emértimet Gjeografike
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3.1.25. STRUKTURA E TEMES ‘PARCELAT KADASTRALE’

feature Type»
ParcelatKandastrale

Gjeometria: Poligon

Inspireld: Identifikues

NumrilPasurisé: CharacterString
ReferencaKkombétareKadastrale: Characterstring

+ 4+ o+

«voidable»
EviefshmeDeri: Daté [0..1]
EviefshmeNga: Daté [0..1]
PikaReferené: Piké [0..1]
VleraEsipérfaqes: Sipérfaqe [0..1]

+ o+ o+ o+

«lifeCyclelnfo, voidable»
+ Fillimiljetégjatésiss: Daté
+ Mbarimiljetégjatésiss: Daté [0..1]

+ZonaKadasirale
«voidable»

+NivelilNj
«voidable» 0..1

TéLarté

«feature Type»
ZonaKadastrale

constraints
{LlojilGjeometrisé}
{VleraESipérfagesUoM}
{EVlefshmeDeri}
{MbarimilJetégjatésiss} .

+Parcela 1.2
«voidable»

«featureType»
KufijtéKadastral

+ Gjeometria: Linjé
+ Inspireld: Identifikues[0..1]
«voidable»

+ EvefshmeDeri: Daté-Oré [0..1]

+ EviefshmeNga: Daté-Oré [0..1]

+ SakésaELlogaritur: Gjatési [0..1]

«lifeCyclelnfo, voidable»
+ FillimilJetégjate Daté
+ MbarimilJetégjatésisé: Daté - Oré [0..1]

constraints
{SaktésiaELlogariturUoM}
{EVlefshmeDeri}
{Mbarimil Jetégjatésis&}

Gjeometria: Poligon
Inspireld: Identifikues[0..1]
NumrilPasurisé: CharacterString

+ 4+ o+

«voidable»

EmértesaEHartésNéShkallénOrigjinale: Integer [0..1]
Eméttimi: EmértimetGjeografike [0..7]

EmrilNiveli: CharacterString [1.."]

EVlefshmeDeri: Dal ré [0..1]

Niveli: VieraENivelitTéZonésKadastrale
PikaReferencé: Piké [0..1]
SaktésiaELlogaritur: Gjatési [0..1]
«lifeCyclelnfo, voidable»

+ FillimilJetégjatésisé: Daté

+ MbarimilJetégjatésisé: Daté [0..1]

+ ottt

constraints
{HierarkiaENivelitTéZonésKadastrale}
{SakésiaELlogariturUoM}
{EVlefshmeDeri}
{MbarimilJetégj atésiss}

«codeList»
VieraENivelitTéZonésKadastrale

Rendi1
Rendi2
Rendi3
Rendi4

+ 4+ o+

Figura 6 - Struktura e temés ‘Parcelat Kadastrale’

ReferencakombétareEZonésKadastrale: CharacterString
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3.1.3. KATALOGU I TIPOLOGIJISE — FEATURE CATALOGUE

3.1.3.1. PERSHKRIM

Njé& ZK &shté njésia bazé pér administrimin e regjistrit t& pasurive t& paluajtshme dhe pérfagéson njé pjesé
t& sipérfaqes sé tokés e pércaktuar gjeografikisht (pa shképutje territoriale), zakonisht njé fshat, njé qytet,
njé lagje né qytetet e médha , ose njé sipérfaqe toke q& pérfshin 4000-5000 pasuri. Cdo ZK ka njé numér
unik té pérbéré nga 4 shifra (p.sh. ZK 1111) i cili vendoset ng bazg t& renditjes s& emrave t& ZK sipas rendit
alfabetik.

Cdo pasuri brenda njé ZK merr njé numér unik (t& vecantg) i cili nuk pérséritet brenda késaj ZK.

e NéZK rurale: vendosja e numrit t& pasurive né njé ZK béhet duke filluar nga skaji veriperéndimor
isaj dhe vazhdon nga peréndimi né lindje dhe né rendin e dyt& nga lindja n& peréndim ¢ késhtu me
rradhé. Numérohen né vazhdimési t& gjitha poligonet pavarésisht nga 1loji i tyre, me pérjashtim t&
pyjeve, kullotave, rrugéve, kanaleve, pérrenjve, lumit, etj, q& mund t& shtrihen pérbri parcelave ose
gjaté gjithé ZK, t& cilat numértohen t& fundit.N& pasurité e paluajtshme t& 1lojit toke bujqésore (aré,
pemtore, vreshté, ullishte) numri i pasurisé pérb&het nga dy njési t& ndara me fraksion (shembull:
123/7). Pjesa ¢ paré ¢ numrit tregon numrin ¢ parcelés kadastrale t& pa ndarg (123 "parcela mémé")
sipas hartave kadastrale t& krijuara para vitit 1991, dhe pjesa e dyté&, pas fraksionit, tregon numrin
e nén-ndarjes (7) s& "parcelés mémé". Nén-ndarjet fillojné me numrin 1. Kur pasuria "mémé" ka
numér me fraksion, pasurité e krijuara do t& kené numér me dy fraksione. Ka edhe pasuri q& nuk
jané ndaré nga privatizimi t& cilat mbajné ish numrin kadastral.

e NéZK urbane: 7K t& qytetit ndahen né blloge t& kufizuara nga rrugét. Madhésia ¢ bllokut varet
nga numri i pasurive dhe sipérfaqja. Rekomandohet q& blloku t& ket& jo mé& shumé se 400 parcela
dhe sipérfaqe jo mé shumé se 7ha. Numértimi i bllogeve brenda njé ZK béhet nga e majta né t&
djathtg, duke filluar me numrin 1. Numrat ¢ bllogeve nga njéri tek tjetri jang ng vazhdimési. Numri
i bllokut &shtg pjesé pérbérése e pasurisé.

¢ Numértimi i parcelave (pasurive) brenda cdo blloku b&het me t& njejtin kriter si mé sipér. Numri i
pasurisé formohet me numrin ¢ bllokut / numrin ¢ parcelés. (Shembuj: numri i pasurisé s& paré t&
bllokut t& paré t& ZK &shté 1/1 dhe numri i pasurisé sé treté t& bllokut t& pesté t& ZK &shté 5/3.)

¢ Parcelat q& priten prej rrugéve, hekurudhave etj, marrin numra t& vecantg sipas pjeséve & jang
ndarg.

¢ Nérast kur parcela ndahet prej njé vije uji ose prej njé rruge kémbésorésh, pjesét lidhen me shenjén
e posedimit (shih shenjat konvencionale) dhe nuk marrin numra t& vecanté. Po késhtu, ndértesat
dhe pjesét e parcelave qé i pérkasin njé pronari, lidhen me shenjén ¢ posedimit dhe nuk marrin
numra t& vecante.

¢ Rrugét kryesore t& njé ZK, si rregull, marrin vetém njé numér derisa t& mos priten brenda asaj ZK
prej rrugéve té tjera kryesore, lumenjéve ose pérrenjéve. Vazhdimi i t& njéjtés rrugé né ZK kufitare
merr numgér tjetér.
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¢ Lumenjté e pérren;jté t& cilét kufizojné dy zona kadastrale, sipas aksit t& njé lumi, marrin né& cdo
zon€ numér t& vecante.

Lulishtja publike n& t& gjitha rrugicat dhe vendet ¢ shétitjeve merr njé numér t& vetém. Ndértesat q& ndodhen
né lulishte marrin numér t& vecanté vetém pér sipérfagen g ato z&né.

3.1.3.2. KUFITE KADASTRALE
-- Emri --

Kufijté kadastralé

-- Pérkufizimi --

Kufiri brenda t& cilit shtrihet njé parcelé kadastrale. Njé kufi kadastral mund t& ndahet me dy parcela kadastrale fqinje.

-- Pérshkrimi --
Né kontekstin e INSPIRE, kufijté kadastralé do t& béhen té disponueshém nga shtetet anétare ku informacioni 1
saktésisé absolute t& pozicionimit regjistrohet pér kufirin kadastral (saktésia e pérllogaritur e atributit).

Tipi i elementit — FeatureT ype

Lidhje ndihmése
b OCL. SaktésiaELlogariturUoM

/* Vlera e SaktésiaELlogaritur duhet t& jepet né metra (m). */
inv: self.estimated Accuracy.uom.uomSymbol="m'

9% OCL. EVlefshmeDeri

/* Nése vendoset vlera EVlefshmeDeri, ajo duhet t& jeté mé e voné se E VlefshmeNga */
inv: selfvalidTo .isEqual(self.validFrom) or self. validTo .isAfter(self validFrom)

9B OCL. MbarimilJetégjatésisé

/* Nése vendoset, vlera MbarimilJetégjatésisé duhet t& jeté mé e voné se FillimilJetégjatésisé */
inv: self.endLifespanVersion .isAfter(self beginLifespanVersion)

Atributet

# EvlefshmeDeri : Dat&-Oré
Shuméllojshméria: [0..1]

-- Emri -
E vlefshme deri.
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Atributet

-- Pérkufizimi -
Data dhe koha né t& cilén kufiri kadastral pérfundon/ose do t& pérfundojé sé pérdoruri ligjérisht.

-- Shénim --
Kjo &shté data dhe ora e referencés kadastrale kombétare e cila nuk mund t& pérdoret mé né veprimet ligjore.

[ Detyrueshme : JO |
¢ EvlefshmeNga : Dat&-Oré
Shuméllojshméria: [0..1]

-- Emri -
E vlefshme nga.

-- Pérkufizimi -
Data dhe koha zyrtare e kufirit kadastral q& ishte/do t& vendoset ligjérisht.

-- Shénim --
Kjo &shtg data dhe koha kur mund t& pérdoret referenca kadastrale kombétare né veprimet ligjore.

[ Detyrueshme : PO |

 FillimilJetégjatésisé : Daté

-- Emri -
Fillimi i jetégjatésisé

-- Pérkufizimi -
Data né té cilén ky Versioni i objektit hapésinor &shtg krijuar ose ndryshuar né t& dhénat hapésinore.

[ Detyrueshme : PO ]

¥ Gjeometria : Linjé

-- Emri -
Gjeometria

-- Pérkufizimi -
Gjeometria e kufirit t& parcelés kadastrale

[ Detyrueshme : PO |
 Inspireld : Identifikues
Shuméllojshméria: [0..1]

-- Emri -
Inspire Id

-- Pérkufizimi --
Identifikues i jashtém i objektit hapésinor.

-- Pérshkrimi -
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Atributet
Njé objekt identifikues i jashtém &shté njé identifikues unik i objektit t& publikuar nga autoriteti pérgjegjés, I cili t& mund t&
pérdoret nga aplikacionet e jashtme t& referimit t& objektit hapésinor. Identifikuesi &shté njé identifikues i objektit hapésinor, jo
njé identifikues i fenomenit né boté.

[ Detyrueshme : PO |

¥ MbarimilJetégjatésisé : Daté - Oré
Shuméllojshméria: [0..1]

-- Emri -
Mbarimi i jetégjatésisé

-- Pérkufizimi -
Data né té cilén ky Versioni i objektit hapésinor &shté pérfunduar.

[ Detyrueshme : JO |

¥ SaktésiaELlogaritur : Gjatési
Shuméllojshméria: [0..1]

-- Emri -
Saktésia llogaritur

-- Pérkufizimi -

Saktésia absolute e pérllogaritur e pozicionimit t& kufirit kadastral né sistemin e pérdorur t& referencave t& koordinatave té&
INSPIRE. Saktésia absolute e pozicionimit &shté vlera mesatare e pozicionimit t& pasigurive pér njé grup pozicionesh, ku
pasiguria pozicionale &shté largésia mes njé pozicioni t& matur dhe asaj ¢faré konsiderohet si pozicioni i vérteté pérkatés.

-- Pérshkrimi --
Kjo vler& mesatare mund t& vijé nga matjet cilésore né njé popullsi homogjene t& kufijve kadastralé ose nga njé pérllogaritje e
bazuar né njohurité e proceseve t& prodhimit dhe saktésisé sé tyre.

[ Detyrueshme : PO |

LIDHJET
#  Lidhjet (drejtimi:Origjina -> Objektivi)

-- Pérkufizim -
The cadastral parcel(s) outlined Nga this cadastral boundary. A cadastral boundary may outline one or two cadastral parcels.

Origjina: (Class) KufijtéKadastralé «featureType» Objektivi: «voidable»  Parcela (Class)
ParcelatKandastrale «featureType»
Shuméllojshméria: [1..2]

- Pérkufizim -

Parcela kadastrale konturohet nga ky kufi kadastral.
Njé kufi kadastral mund t& konturojé njé ose dy
parcela kadastrale.
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3.1.33. VLERA E NIVELIT TE ZONES KADASTRALE
-- Emri --
Vlera e nivelit té zonés kadastrale.

-- Pérkufizimi --
Nivelet e hierarkisé t& zonave kadastrale.

-- Pérshkrimi --
Nivelet mé té larta t& hierarkisé sé temés kufijté e njésive administrative (shteti) nuk pérsériten né kété listé kodesh.

Tipi i elementit — Enumeration & CodeList

Atributet

# Rendil :

-- Emri -
Rendi i paré

-- Pérkufizimi --
Niveli mé i larté (sipérfaget mé t& médha) né hierarking e zonave kadastrale, t& barabarta ose t& barasvlershme me zonat e
rregjistrimit. Regjistrimit eshte territori ge perfshin nga disa zona kadastrale ge ndodhen ne administrim te nje ZVRPP-je.

¥ Rendi2 :

-- Emri -
Rendi i dyté

-- Pérkufizimi --
Niveli i dyté né hierarking e zonave kadastrale, t& barabarta ose t& barasvlershme me zonen kadastrale.

¥ Rendi3:

-- Emri -
Rendi i treté

-- Pérkufizimi —
Niveli i treté né hierarking e zonave kadastrale, t& barabarta ose t& barasvlershme me bllokun kadastral.
# Rendi4 :

-- Emri -
Rendi i katért

-- Pérkufizimi —
Niveli i katért né hierarking e zonave kadastrale, t& barabarta ose t& barasvlershme me parcelen kadastrale.
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3.1.3.4. PARCELAT KADASTRALE

- Emri --
Parcelat kadastrale

-- Pérkufizimi --
Parcela kadastrale éshté njé sipérfaqe tokésore (toké dhe/ose ujé) mbi té cilén ekzistojné té drejta juridike pronésie

homogjene sipas njé titulli t& vertetuar nga njé akt bazuar né legjislacionin kombétar.

-- Shénim --
Né kontekstin e INSPIRE, parcelat kadastrale duhet té formojné, aq sa té jeté e mundur, njé ndarje t& territorit
kombétar-

Tipi i elementit — FeatureT ype

Lidhje ndihmése
95 OCL. LlojilGjeometrisé

/* Lloji i gjeometrisé mund t& jeté sipérfaqge ose shumé-sipérfagéshe */
inv: geometry.oclIsKindOf{GM_ Surface) or geometry.oclIsKindOf{lGM_MultiSurface)

98 OCL. VleraE SipérfagesUoM

/* Vlera e VleraESipérfaqes duhet t& jepet né metér katror (m2). */
inv: selfareaValue.uom.uomSymbol='m2'

9B OCL. EVlefshmeDeri

/* Nése vendoset vlera EVlefshmeDeri, ajo duhet t& jeté mé e voné se E VlefshmeNga */
inv: selfvalidTo .isEqual(self.validFrom) or self validTo .isAfter(self validFrom)

@B OCL. MbarimilJetégjatésisé

/* Nése vendoset, vlera MbarimilJetégjatésisé duhet t& jeté mé e voné se FillimilJetégjatésisé */
inv: self.endLifespanVersion .isAfter(self beginLifespanVersion)

Atributet

# NumrilPasurisé : CharacterString

-- Emri -
Numui [ pasurisé

-- Pérkufizimi -
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Atributet
Teksti i pérdorur gjerésisht pér t& shfaqur identifikimin e parcelés kadastrale.

-- Shénim -
Numii [ pasurisé zakonisht éshté pjesa e fundit e referencés kadastrale.

[ Detyrueshme : PO |
¢ EvlefshmeDeri : Daté
Shuméllojshméria: [0..1]

-- Emri -
E vlefshme deri.

-- Pérkufizimi -
Data dhe koha né t& cilén parcela kadastrale pérfundon/ose do té pérfundojé s& pérdoruri ligjérisht.

-- Shénim --
Kjo &shtg data dhe ora e referencés kadastrale kombétare e cila nuk mund té pérdoret mé né veprimet ligjore.

[ Detyrueshme : JO |
# EvlefshmeNga : Daté
Shuméllojshméria: [0..1]

-- Emri -
E vlefshme nga.

-- Pérkufizimi -
Data dhe koha zyrtare e parcelés kadastrale q& ishte/do t& vendoset ligjérisht.

-- Shénim -
Kjo &shtg data dhe koha kur mund t& pérdoret referenca kadastrale kombétare né veprimet ligjore.

[ Detyrueshme : PO |

 Fillimiljetégjatésisé : Daté

-- Emri -
Fillimi i jetégjatésisé

-- Pérkufizimi -
Data né té cilén ky Versioni i objektit hapésinor &shtg krijuar ose ndryshuar né t& dhénat hapésinore.

[ Detyrueshme : PO ]

¢ Gjeometria : Poligon

-- Emri -
Gjeometria

-- Pérkufizimi -
Gjeometria e parcelés kadastrale
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Atributet

[ Detyrueshme : PO ]

# Inspireld : Identifikues

-- Emri -
Inspire Id

-- Pérkufizimi --
Identifikues i jashtém i objektit hapésinor.

-- Pérshkrimi -
Njé objekt identifikuesi jashtém éshté njé identifikues unik i objektit t& publikuar nga autoriteti pérgjegjés, i cili mund t& pérdoret

nga aplikacionet e jashtme t& referimit t& objektit hapésinor. Identifikuesi &shté njé identifikues i objektit hapésinor, jo njé
identifikues i fenomenit né boté.

[ Detyrueshme : PO ]
¥ Mbarimiljetégjatésisé : Daté
Shuméllojshméria: [0..1]

-- Emri -
Mbarimi i jetégjatésisé

-- Pérkufizimi -
Data né té cilén ky Versioni i objektit hapésinor &shté pérfunduar.

[ Detyrueshme : JO |
¥ PikaRefereng : Piké
Shuméllojshméria: [0..1]

-- Emri -
Pika referencé

-- Pérkufizimi -
Njé piké né parcelén kadastrale (centroidi).

-- Shénim--
P.sh. Qendra e gjeometrisé sé parcelés

[ Detyrueshme : PO |

# ReferencaKombétareKadastrale : CharacterString

-- Emri -
Referenca kombétare kadastrale

-- Pérkufizimi -
Identifikues tematik né nivel kombétar, pérgjithésisht kodi i ploté kombétar i parcelés kadastrale. Duhet t& sigurojé lidhjen me
regjistrin kadastral kombétar ose t& barasvlershém me té.

-- Shénim--
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Atributet

Referenca kadastrale kombétare mund t& pérdoret edhe né kérkesat e métejshme né shérbimet kombétare.

¥ VleraEsipérfaqes : Sipérfaqe
Shuméllojshméria: [0..1]

- Emri --
Vlera e sipérfages

-- Pérkufizimi -

[ Detyrueshme : PO ]

Vleré e regjistruar e zonés q& péreakton sasing e sipérfaqes sé projektuar né rrafshin horizontal t& parcelés kadastrale.

LIDHJET
#  Lidhjet (drejtimi:Origjina -> Objektivi)

-- Pérkufizim -
Parcela kadastrale i pérket njé njésie administrative.

Origjina: (Class) ParcelatKandastrale «featureType»

#  Lidhjet (drejtimi:Origjina -> Objektivi)

-- Pérkufizim —
Zona kadastrale pérmban kété parcelé kadastrale.

Origjina: (Class) ParcelatKandastrale «featureType»

/" Lidhjet (drejtimi:Origjina -> Objektivi)

-- Pérkufizim -

[ Detyrueshme : PO |

Objektivi: «voidabley Njésité Administrative
(Class) Njésitt Administrative «featureType»
Shuméllojshméria: [0..1]

- Pérkufizim -
Njésia administrative e nivelit mé t& ulét pérmban
kété parcelé kadastrale.

Objektivi: «voidable» ZonaKadastrale (Class)
ZonaKadastrale «featureType»
Shuméllojshméria: [0..1]

- Pérkufizim -
Zona kadastrale e njésisé mé t& ulét pérmban kété
parcelé kadastrale.

Parcela kadastrale kufizohet nga ky kufi kadastral. Njé kufi kadastral mund t& kufizojé njé ose dy kufij kadastralé.
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LIDHJET
Origjina: (Class) KufijtéKadastralé «featureType»

# Lidhjet (drejtimi: Origjina -> Objektivi)

Origjina: (Class) Adresa «featureType»

3.1.3.5. ZONAKADASTRALE

-- Emri --
Zona kadastrale

-- Pérkufizim —

Objektivi: «voidable»  Parcela (Class)
ParcelatKandastrale «featureType»
Shuméllojshméria: [1..2]

- Pérkufizimi -

Parcela kadastrale konturohet nga ky kufi kadastral.
Njé kufi kadastral mund t& konturojé njé ose dy
parcela kadastrale.

Objektivi: «voidable»  Parcelé  (Class)
ParcelatKandastrale «featureType»
Shuméllojshméria: [0..%]

- Pérkufizim -
Parcela kadastrale gé kjo adresé éshté e lidhur.

— Pérshkrim -

Njé adresé mund t& keté lidhje me zero, njé ose
shumé parcela kadastrale. Gjithashtu éshté e mundur
qé shumé adresa t& lidhen me njé parcelé kadastrale
(kjo nuk éshté e paraqitur né keto skema aplikimi.

Zona kadastrale éshté sip&rfaqja e tok&s e pércaktuar gjeografikisht (pa shképutje territoriale), zakonisht njé fshat, njé
qytet, njé lagje né qytetet e médha , ose njé sipérfage toke qé pérfshin nje numer te konsiderueshem parcelash

kadastrale, dhe pérdoret pér t& mbartur informacionin e metadatave dhe pér t& leht&suar portretizimin e t& dhé&nave t&

regjistrit t& pasurive t& paluajtshme.

-- Pérshkrim —

Né kontekstin e INSPIRE, zonat kadastrale jané Sipérfaqe terreni (toke dhe/ose uji) t& ndérmjetme qé ndajné territorin
kombétar me gellim administrimin e regjistrit te parcelave kadastrale dhe do t& pérdoren pér t& mbartur informacion
té metadata-ve dhe pér t& lehtésuar portretizimin e t& dhénave. Zonat kadastrale pérgjithésisht pércaktohen kur harta

kadastrale krijohet pér heré t& paré.

Tipi i elementit — FeatureT ype
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Lidhje ndihmése
9B OCL. HierarkiaENivelitTéZonésKadastrale

/*Njé zoné kadastrale e nivelit t& ulét duhet t& jeté pjesé e njé niveli mé t& larté. */
inv: selfnationalLevel <> 'lstOrder' implies selflevel < self.upperLevelUnit.level

9B OCL. SaktésiaELlogariturUoM

/* Vlera e SaktésiaELlogaritur duhet t& jepet né metra (m). */
inv: self.estimated Accuracy.uom.uomSymbol="m'

98 OCL. EVlefshmeDeri

/* Nése vendoset vlera EVlefshmeDeri, ajo duhet t& jeté mé e voné se EVlefshmeNga */
inv: selfvalidTo .isEqual(self.validFrom) or self.validTo .isAfter(self validFrom)

95 OCL. MbarimilJetégjatésisé

/* Nése vendoset, vlera MbarimilJetégjatésisé duhet t& jeté mé e voné se FillimilJetégjatésisé */
inv: self.endLifespanVersion .isAfter(self beginLifespanVersion)

Atributet

¥ EmértesaEHartésNéShkallénOrigjinale : Integer
Shuméllojshméria: [0..1]

-- Emri -
Emértesa e hartés né shkallén origjinale

-- Pérkufizimi -
Emértuesi né shkallé t& hartés origjinale né letér (nése ka) me t& cilén korrespondon zona kadastrale.

-- Shénim--
P.sh. 2000 g& nénkupton harta origjinale kadastrale ishte e shkallés 1:2000

[ Detyrueshme : PO |
¥ Emértimi : EmértimetGjeografike
Shuméllojshméria: [0..*]

-- Emri -

Emértimi

-- Pérkufizimi -

Emértimi i zonés kadastrale

-- Shénim -
Zonat kadastrale g& jané gjithashtu njési administrative ka né pérgjithési njé emértim.
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Atributet

[ Detyrueshme : PO ]
# EmrilNiveli : CharacterString
Shuméllojshméria: [1..*]

-- Emri -
Emri i nivelit

-- Pérkufizimi -
Emri i nivelit t& zonés kadastrale né hierarking kadastrale kombétare né t& paktén njé gjuhé zyrtare t& Bashkimit Evropian.

-- Pérshkrimi --
Psh. pér Spanjén, emri i nivelit mund t& jepet si "municipio” (né Spanjisht) dhe si “municipality” (né anglisht).

[ Detyrueshme : PO ]

 Etiketa : CharacterString

-- Emri -
Etiketa

-- Pérkufizimi -
Tekst i pérdorur gjerésisht pér € shfaqur identifikimin e zonés kadastrale.

-- Pérshkrimi --
Etiketa &sht& zakonisht pjesa e fundit e referencés sé zonés kadastrale kombétare ose veté referencés apo emrit.

[ Detyrueshme : PO ]
¢ EVlefshmeDeri : Daté-Oré
Shuméllojshméria: [0..1]

-- Emri -
E vlefshme deri.

-- Pérkufizimi -
Data dhe koha né t& cilén zona kadastrale pérfundon/ose do t& pérfundojé sé pérdoruri ligjérisht.

-- Shénim -
Kjo éshté data dhe ora e referencés kadastrale kombétare e cila nuk mund t& pérdoret mé né veprimet ligjore.

[ Detyrueshme : JO |
¥ EVlefshmeNga : Daté-Oré
Shuméllojshméria: [0..1]

-- Emri -
E vlefshme nga.

-- Pérkufizimi -
Data dhe koha zyrtare e zonés kadastrale g& ishte/do t& vendoset ligjérisht.
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Atributet

-- Shénim --
Kjo éshtg data dhe koha kur mund t& pérdoret referenca kadastrale kombétare né veprimet ligjore.

[ Detyrueshme : PO |

 FillimilJetégjatésisé : Daté

-- Emri -
Fillimi i jetégjatésisé

-- Pérkufizimi -
Data né té cilén ky Versioni i objektit hapésinor &shtg krijuar ose ndryshuar né t& dhénat hapésinore.

[ Detyrueshme : PO ]

¥ Gjeometria : Poligon

-- Emri -
Gjeometria

-- Pérkufizimi -
Gjeometria e zonés kadastrale.

[ Detyrueshme : PO ]

v Inspireld : Identifikues
Shuméllojshméria: [0..1]

-- Emri -
Inspire Id

-- Pérkufizimi —
Identifikues i jashtém i objektit hapésinor.

-- Pérshkrimi --
Njé objekt identifikuesi jashtém éshté njé identifikues unik i objektit t& publikuar nga autoriteti pérgjegjés, i cili mund t& pérdoret

nga aplikacionet e jashtme t& referimit t& objektit hapésinor. Identifikuesi &shté njé identifikues i objektit hapésinor, jo njé
identifikues i fenomenit né boté.

[ Detyrueshme : PO ]
¥ MbarimilJetégjatésisé : Daté
Shuméllojshméria: [0..1]

-- Emri -
Mbarimi i jetégjatésisé

-- Pérkufizimi -
Data né té cilén ky Versioni i objektit hapésinor &shté pérfunduar.

[ Detyrueshme : JO |
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Atributet

# Niveli : VleraENivelitTéZonésKadastrale

-- Emri -
Niveli

-- Pérkufizimi --
Niveli i zonés kadastrale né hierarking kadastrale kombétare

[ Detyrueshme : PO ]
¢ PikaReferencé : Piké
Shuméllojshméria: [0..1]

-- Emri -
Pika referencé

-- Pérkufizimi -
Njé piké brenda zongs kadastrale.

-- Shénim--
P.sh. Centroidi i gjeometrisé sé& parcelés kadastrale.

[ Detyrueshme : PO ]

¢ ReferencaKombétareEZonésKadastrale : CharacterString

-- Emri -
Referenca kombétare e zongs kadastrale

-- Pérkufizimi -
Identifikuesi tematik né nivel gendror, pérgjithésisht kodi i ploté kombétar i zonés kadastrale.

- Shénim--
P.sh. 03260000AB (Francé), 30133 (Austria), APDOOF (Holands).

[ Detyrueshme : PO ]

¥ SaktésiaELlogaritur : Gjatési
Shuméllojshméria: [0..1]

-— Emri --
Saktésia llogaritur

-- Pérkufizimi -

Saktésia absolute e pérllogaritur e pozicionimit t& parcelés kadastrale né Sistemin Koordinativ referencé té pérdorur nga
INSPIRE. Saktésia absolute e pozicionimit &shté vlera mesatare e pozicionimit t& pasigurive pér njé¢ grup pozicionesh, ku
pasigurité pozicionale jang: largésia mes njé pozicioni t& matur dhe asaj ¢faré konsiderohet si pozicioni i vérteté pérkatés.
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Atributet

-- Pérshkrimi --
Kjo vleré mesatare mund & vijé nga matjet cilésore né njé popullsi homogjene t& parcelave kadastrale ose nga njé pérllogaritje
¢ bazuar né njohurité e proceseve t& prodhimit dhe saktésisé sé tyre.

[ Detyrueshme : PO |

LIDHJET
# Lidhjet (drejtimi: Origjina -> Objektivi)

-- Pérkufizim --
Reflekton hierarking e pércaktimit t& indeksit kadastral né njé vend (rendi i paré mé1i larti)

Origjina: (Class) ZonaKadastrale «featureType» Objektivi:  «voidabley NivelilNjésiséMéTELarté
(Class) ZonaKadastrale «featureType»
Shuméllojshméria: [0..1]

-- Pérkufizimi --
Niveli tjetér mé i larté i zonés kadastrale pérmban
kété zoné kadastrale.

# Lidhjet (drejtimi: Origjina -> Objektivi)
-- Pérkufizim —

Reflekton hierarking e pércaktimit t& indeksit kadastral né njé vend (rendi i paré mé1i larti)

Origjina: (Class) ZonaKadastrale «featureType» Objektivi:  «voidabley NivelilNjésiséMéTELarté
(Class) ZonaKadastrale «featureType»
Shuméllojshméria: [0..1]

-- Pérkufizimi --
Niveli tjetér mé i larté i zonés kadastrale pérmban
kété zoné kadastrale.

# Lidhjet (drejtimi: Origjina -> Objektivi)

-- Pérkufizim -

Zona kadastrale pérmban kété parcelé kadastrale.

Origjina: (Class) ParcelatKandastrale «featureType» Objektivi: «voidable» ZonaKadastrale (Class)

ZonaKadastrale «featureType»
Shuméllojshméria: [0..1]

-- Pérkufizimi --
Zona kadastrale e njésisé mé t& ulét pérmban kété
parcelé kadastrale.
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3.1.4. METADATA.

3.1.4.1. ELEMENTET E METADATA-VE

N& tabelén ¢ méposhtme paraqiten kéto elementé:

= Kolona ¢ paré ofron njé referencé té pjesés pérkatése né Rregulloren e Metadatés, ¢ cila pérmban

njé pérshkrim mé t& hollgsishém.

= Kolona ¢ dyt& specifikon emrin ¢ Metadatés.
= Kolona e treté specifikon shuméllojshméring.
= Kolona ¢ katért specifikon gjendjen, sipas t& cilés elementi béhet i detyrueshém.

Pjesa e

rregullores sé Elementi i Metadata-ve Shuméllejs | Gjendja

metadatave hméria

1.1 Titulli i burimit 1

1.2 Abstrakti 1 burimit 1

13 Lloji i burimit 1

14 Lokalizuesi i burimit 0.% |I detyrueshém, nése nj¢ URL éshté e
disponueshme pér té pérftuar informacione
té tjera né burim, dhe/ose shérbimeve té
aksesit.

1.5 Identifikuesi unik 1 burimit 1

1.7 Gjuha e burimit 0.% |E detyrueshme, nése burimi pérfshin
informacion né tekst.

2.1 Kategoria e temés 1.%

3 Fjalé kyce 1.%x

4.1 Kuti e kornizés gjeografike Lo

S5 Referenca kohore 1.

6.1 Cikli i jetés 1

6.2 Rezolucioni gjeohapésinor 0.% |T detyrueshém pér grupet e t& dhénave dhe
serive t& tyre, nése mund t& specifikohet
shkalla e barasvlershme me to ose njé
distancg.

7 Pérputhshmeéria 1.,
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8.1 Kushtet pér aksesin dhe 1..%
pérdorimin

82 Kufizimet e aksesit 1..%
publik

9 Autoriteti pérgjegjés 1.,

10.1 Pika e kontaktit metadata-ve 1.%x

10.2 Data e metadata-ve 1

10.3 Gjuha e metadata-ve 1

3.1.42. ELEMENTET E METADATA-VE PER NDERVEPRUESHMERINE

Tabelat pérshkruajné elementét ¢ metadata-ve t& cilat pérmbajé informacionin e méposhtém:

= Kolona ¢ parg siguron nj& referencé pér njé pérshkrim mé t& detajuar.

= Kolona ¢ dyt& specifikon emrin ¢ elementit metadata.

= Kolona e treté specifikon shuméllojshméring.

= Kolona ¢ katért specifikon kushtet, nén t& cilat elementi i dhéné béhet i detyrueshém.

N& meényré specifike, metadatat pér temén Parcelat Kadastrale jepen t& tabeluara mé poshté:

Specifikimi i t&
dhénave pér
Temén Parcelat

Elementi Metadata

Kushtet

Kadastrale
Referenca e Sistemit
31421 Koordinativ ! .
R Liden, e gL vt
31422 Pérkohshme ¢ 0. | MEatipee vegorve oty 4° b . .
. . pérkohshém qé nuk i referohen kalendarit gregorian apo
Sistemit ; : ;
CoordinatedUniversal Time.
31423 Kodimi Jieo! -
31424 Karakteri i Kodimit 0. I detﬂyrl{eshém, ne ?Ofté SEI ko.‘%lm e bazd [G XN
&shté pérdorur qé t& mos suportojé UTF-1
31425 Lloji i Pérfagésimit 1 Metoda e pérdorur hap&sinore paraqet informata
T Hapé&sinor " | gleografike
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3.1.4.2.1. Sistemi Koordinativ Referencé

Emri I Elementit Metadata

Sistemi Koordinativ Referencé

Pérkufizimi

Pérshkrimi Sistemeve Koordinativé té Referencés té pérdorur né grupin e té
dhénave hapésinore

Iso 19115 Numri dhe Emértimi

13. referenceSystemInfo

ISO/TS 19139 referenceSystemInfo
INSPIREI detyrueshém /i

Kushtézuar I detyrueshem
INSPIREShuméllojshméria 1

Lloji i t& dhénave (ISO 19115
no.)

186. MD_ReferenceSystem

Vlera e fushés

Pér té identifikuar sistemin referencé duhet té sigurohet
IdentifikuesiReferencéSistemit (RS Identifikues). SHENIM udhézime mé
specifike, né veganti né vlerat e paracaktuara pér plotésimin e atributeve té
IdentifikuesiReferencéSistemit duhet t& bihet dakord mes shteteve anétare gjaté
fazés sé zbatimit t& mbéshtetjes sé ndérveprimit.

Instruksionet e implementimit

Shembull

referenceSystemIdentifier: code: ETRS 89 codeSpace: INSPIRE RS registry

Shembull i kodimit XML

<gmd:referenceSystemInfo>
<gmd:MD_ReferenceSystem>

<gmd:reference SystemIdentifier>
<gmd:RS_Identifier>

<gmd:code>

<gco:CharacterString>ETRS89 </gco:CharacterString>
</gmd:code>

<gmd:codeSpace>

<gco:CharacterString>INSPIRE RS registry</gco:CharacterString>
</gmd:codeSpace>

</gmd:RS_Identifier>

</gmd:reference SystemIdentifier>
</gmd:MD_ReferenceSystem=>

</gmd:reference SystemInfo>

Komente

3.1.4.2.2. Sistemet Koordinative

Referencé, t& pérkohshme

Emri i Elementit Metadata

Sistemi Referencé i Pérkohshém

Pérkufizimi

Pérshkrimi i sistemeve té referencés té pérkohshme té pérdorura né setin e té
dhénave

Is0 19115 Numri dhe Emértimi

13. referenceSystemInfo

ISO/TS 19139

referenceSystémInfo

INSPIREI detyrueshém /i
kushtézuar

I detyrueshém, nése grupi i té dhénave hapésinore ose njé nga tipet e vecorive té
tij q¢ pérmban informacion t& pérkohshém qé nuk i referohen kalendarit
Gregorian.

INSPIRE Shuméllojshméria

0.%

Lloji i t& dhénave (ISO 19115

no.)

186. MD_ReferenceSystem
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Vlera e fushés

Asnjé tip specifik nuk éshté pércaktuar né ISO 19.115 pér sistemet e referimit t&
pérkohshém. Késhtu, elementét gjenerik MD_ReferenceSystem dhe referencé
SystemIdentifier (RS_Identifier) do té ofrohen.

Instruksionet e implementimit

Shembull

referenceSystemIdentifier:
code: GregorianCalendar
codeSpace: INSPIRE RS registry

Shembull i kodimit XML

<gmd:reference SystemInfo>
<gmd:MD_ReferenceSystem>
<gmd:reference SystemIdentifier>
<gmd:RS_Identifier>

<gmd:code>
<gco:CharacterString>GregorianCalendar
</gco:CharacterString>
</gmd:code>

<gmd:codeSpace>

< gco:CharacterString>=INSPIRE RS
Registry </gco:CharacterString>
</gmd:codeSpace>
</fgmd:RS_Identifier>
</gmd:referenceSystemIdentifier>
</fgmd:MD_ReferenceSystém>
</gmdreferenceSystemInfo>

Komente

3.1.4.2.3. Kodimi

Emri i Elementit Metadata

Kodimi

Peérkufizimi

Pérshkrimi i konstruktit t& gjuhés kompjuterike qé specifikon pérfagésimin e
objekteve té t& dhénave né njé rekord, fotografi, mesazh, pajisje ruajtje ose né
kanalin e transmetimit

Iso 19115 Numri dhe
Emertimi

271. distributionFormat

ISO/TS 19139

distributionInfo/MD Distribution/distributionF ormat

INSPIREI detyrueshém /i
kushtézuar

I detyrueshém,

INSPIRE Shuméllojshméria

L™

Lloji i t& dhénave (ISO 19115
no.)

284. MD_Format

Vlera e fushés

Vlerat e pronés (emér, version, specifikim) t& specifikuara, do t& pérdoren pér
té dokumentuar pérzgjedhjen dhe alternativat e kodimit.

Instruksionet e implementimit

Shembull

Emri: <Emri i skemés 8 aplikuar> GML skemé aplikimi version: specifikim
version 3.1rcl: D2.8.1.8 Data Specifikimet pér Parcelat Kadastrale -
Udhézime teknike
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Shembull i kodimit XML

<gmdMD_Format>

<gmd:name>
<gco:CharacterString>SomeApplicationSchema GML
application schema</gco:Character String>
</gmd:name>

<gmd:version>

<gco:CharacterString>3. 1rc1</gco:CharacterString>
</gmd:version>

<gmd:specification>

<gco:CharacterString>D2.8.1.8 Data Specification on Hydrography —
Technical Guidelines</gco:CharacterString>
</gmd:specification>

</gmd:MD Format>

Komente

3.1.4.2.4. Karakteret e kodimit

Emri i Elementit Metadata

Karakteret e Kodimit

Pérkufizimi

Karakteret e kodimit pérdoren né setin e t& dhénave.

Iso 19115 Numri dhe Emértimi

ISO/TS 19139

INSH_RE i detyrueshém /i T detyrueshém, né qofté se njé kodim i pérdorur nuk éshté i bazuar né UTF-8.

kushtézuar

INSPIRE Shuméllojshméria 0.%

Lloji i té dhénave (ISO 19115 no.)

Vlera e fushés

Instruksionet e implementimit

Shembull -
<gmd:characterSet>
<gmd:MD_CharacterSetCode

codeListValue="885%part2"

Shembull i kodimit XML codeList="http://standards.iso.org/ittf/Publicly Available Standards/I
SO _19139 Schemas/reOrigjinas/Codelist/ML,_gmxCodelists.xml#
CharacterSetCode">8859-2</gmd:MD_CharacterSetCode>
</gmd:characterSet>

Komente

3.1.4.2.5. Lloji i pérfagésimit hapé&sinor

Emri i Elementit Metadata

Lloji i Pérfaqgésimit Hapésinor

Pérkufizimi

Metodat e pérdorura hapésinore paraqesin informata gjeografike

Iso 19115 Numri dhe
Emértimi

37. spatialRepresentationType
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ISO/TS 19139

INSPIRE i detyrueshém /i .

kushtézuar Ldetyruestienn

INSPIRE Shuméllojshméria L™

i}gl iiteidhepave IS0 19115 B.5.26 MD_SpatialRepresentationTypeCode

Vlera e fushés

Instruksionet e implementimit

I vlerave té pérfshira né listén e koduar né ISO 19115 (vektor, rrjet,
textTable, TIN, stereoModel, video), vetém vektor, rrjet dhe TIN duhet t&
pérdoren.

SHENIM vlerat Lista kodi shtesé¢ mund té pércaktohen bazuar né reagimet
nga zbatimi

Shembull

Shembull i kodimit XML

Komente
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3.1.5. SISTEMET REFERENCE, NJESITE E MATIES DHE RRIETAT GJEOGRAFIKE.

SISTEMET STANDARDE TE REFERIMIT, NJESITE E MATJEVE DHE RRIETET

Sistemet koordinative referencé, njésité e matjeve dhe sistemet e rrjeteve gjeografike té pérfshira né kété nén-seksion
jané standardet qé do t& pérdoren pér té gjitha grupet e t& dhénave INSPIRE, pérveg kur ka pérjashtime specifike t&
temés dhe/ose kérkesa té tjera té pércaktuara né seksionin 6.2.

A KORNIZA REFERUESE GJEODEZIKE E SHQIPERISE

Korniza Referuese Gjeodezike Shqiptare qé do té pérdoret né Republikén e Shqipérisé do té quhet:

“Korniza Referuese Gjeodezike Shqiptare 20107 ose shkurt (KRGISH-2010 — kodi EPSG: 6870 1), ku “2010” éshté
indeksi qé& lidhet me “epokén” né té cilén jané pércaktuar koordinatat ¢ pikave gjeodezike té monumentalizuara né
territorin e Republikés sé& Shqipérisé. KRGISH-2010 do t& pércaktohet duke u mbéshtetur né Kornizén Referuese
Gjeodezike Europiane. KRGISH-2010 do t& pérdoret né t& gjitha aplikacionet qé lidhen me pérdorimin e koordinatave
né territorin e vendit. Lidhja midis KRGISH-2010 dhe sistemeve té tjera t& pérdorura né vendin toné do t& béhet duke
pérdorur parametrat e transformimit té llogaritura pér ¢do rast.

KRGISH-2010 pérfshin:

a) parametrat gjeodeziké bazé t& pércaktuar né Sistemin Referues Gjeodezik 1980 (GRS-80) si mé poshté:
- Rrezja e ekuatorit t& tokés: a =6 378 137m;
- Konstantja gravitacionale gjeocentrike e tokés duke pérfshiré edhe atmosferén: GM = 3 986 005 x 10 m®s’
2%

- TFaktori dinamik i figurés sé tokés pa pérfshiré baticén e géndrueshme: J2 =108 263 x 10°;
- Katyj faktori i korrespondon shtypja né pole: 1/f = 298.257222100882711;
- Shpejtésia kéndore e rrotullimit t& tokés: @ =7 292115.0 x 10°!'rad sek

b) sistemin koordinativ gjeodezik ETRS 89;

c) sistemin e lartésive qé realizohet népérmjet reperave té rrjetit shtetéror t& nivelimit té pérfshiré né Rrjetin
Unik Europian t& Nivelacionit (UELN) dhe t& pércaktuara né Sistemin Referues Vertikal Europian (EVRS)
me ndihmén e t& dhénave pér forcén e réndesés té unifikuara né sistemin International Gravity
Standardization Network 1971 (IGSN 1971).

d) sistemin e koordinatave né plan, i cili mundésohet nga dy projeksione hartografike:
- Projeksioni Térthor Zonal 1 Merkatorit (TMzn) pér harta né shkallé mé t& madhe se 1:500.000 me parametrat
e meposhtme:

e Elipsoidi referencé: GRS80

e  Meridiani fillestar: Grinuig

e Meridiani gendor (MQ): 200

e  Shkalla e shformimit né meridianin gendror (ko): 1

s Fallco e lindjes: 500 000 m
e Fallco e veriut: Om

! Shiko Aneks 4.3
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- Projeksioni Konik Konform i Lambertit (LCC) pér harta né shkallg 1:500 000 dhe mé t& vogla.

B. SISTEMET KOORDINATIVE REFERENCE SIPAS INSPIRE

1.2 Datumi

Datumi pér sistemet koordinative referencé dy-dimensionale dhe tre-dimensionale

Pér sistemet koordinative referencé dy-dimensionale dhe tre-dimensionale dhe komponentja horizontale e
sistemeve koordinative referencé t& kombinuara t& pérdorura pér t& béré t& disponueshém grupin e t& dhénave
hapésinore, si datum do te jeté datumi i Sistemit Tokésor Referencé Evropian 1989 (ETRS89) né zona brenda
kufijve gjeografiké t& tij, ose datumi i Sistemit Tokésor Referencé Ndérkombétar (ITRS) ose sisteme koordinative
referencé e gjeodezike té tjera t& pérputhura me ITRS, né zona qé ndodhen jashté kufijve gjeografiké t&é ETRSS9.
Té pérputhura me ITRS do té thoté qé pérkufizimi i sistemit bazohet né pérkufizimin e ITRS dhe ka njé marrédhénie
té miré-dokumentuar mes dy sistemeve, sipas EN ISO 19111.

1.3 Sistemet koordinative referencé

Sistemet koordinative referencé
Grupet e t& dhénave hapésinore do t& béhen té disponueshme duke pérdorur té pakten njé prej sistemeve
koordinatave referencé té caktuara né seksionet 1.3.1, 1.3.2 dhe 1.3.3, pérve¢ kur qéndron njéri prej kushteve t&
caktuara né seksionin 1.3.4.
1.3.1 Sistemet koordinative referencé tre-dimensionale

- Koordinatat karteziane tre-dimensionale bazohen né njé datum té caktuar né seksionin 1.2 dhe pérdorin
parametrat e elipsoidit GRS80 (Sistemi Gjeodezik Referencé 1980).

- Koordinatat gjeodezike tre-dimensionale (gjerésia, gjatésia dhe lartésia elipsoidike) bazohen né njé
datum té& caktuar né seksionin 1.2 dhe pérdorin parametrat e elipsoidit GRS80.

1.3.2 Sistemet koordinative referencé dy-dimensionale

- Koordinatat gjeodezike dy-dimensionale (gjerésia dhe gjatésia) bazohen né njé datum té caktuar né
seksionin 1.2 dhe pérdorin parametrat e elipsoidit GRS80.

- Koordinatat né plan pérdorin sistemin koordinativ referencé ETRS89 me projeksion LAEA (Lambert
Azimuthal Equal Area) pér analiza hapésinore dhe raportime, ku duhet t& pasqyrohen sipérfaget e
vérteta.

- Koordinatat né plan pérdorin sistemin koordinativ referencé ETRS89 me projeksion LCC (Lambert
Conformal Conic) pér hartografime konforme né territorin e Europés né shkallé t& barabarta ose mé t&
vogla se 1:500 000.

- Koordinatat né plan pérdorin sistemin koordinativ referencé ETRS89 me projeksion TM (Transverse
Mercator) pér hartografime konforme né territorin e Europés né shkallé té barabarta ose mé té médha se
1:500 000.

1.3.3 Sistemet koordinative referencé té¢ kombinuara

1. Pér komponenten horizontale t& sistemit koordinativ referencé t& kombinuar, njé prej sistemeve koordinative
referencé té caktuara né seksionin 1.3.2 do té& pérdoret.

2. Pér komponenten vertikale, do t& pérdoret njé prej sistemeve koordinative referencé t& méposhtme:

- Pér komponenten vertikale né sipérfagen tokésore, do t& pérdoret Sistemi Vertikal Referencé Europian
(EVRS) pér t& shprehur lartésité e lidhura me gravitetin brenda kufijve gjeografiké té kétij sistemi. N&
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zona t& cilat ndodhen jashté kufijve gjeografiké t&¢ EVRS, do t& pérdoren sisteme vertikale referencé té
tjera té& lidhura me fushén e gravitetit tokésor pér t& shprehur lartésité e lidhura me gravitetin.
- Pér komponenten vertikale né atmosferen e liré, presioni barometrik i konvertuar né lartési duke pérdour
IS0 2533:1975 Atmosferen Standarde Ndérkombétare, ose do t& pérdoren sisteme referencé té tjera
lineare ose parametrike. Aty ku jané pérdorur sisteme referencé parametrike t& tjera, ato do t&
pérshkruhen né njé referencé té kuptueshme duke pérdorur EN ISO 19111-2:2012.
- Pér komponenten vertikale né zonat detare ku ka njé rang té ndjeshém batice (ujéra baticor), si sipérfaqe
referencé do t& pérdoret Batica mé e ulét Astronomike (LAT).
- Pér komponenten vertikale né zonat detare ku nuk ka njé rang t& ndjeshém batice, né ogeanet e hapura
dhe efektivisht né ujéra mé té thella se 200 metra, si sipérfage referencé do t& pérdoret niveli mesatar i
detit (MSL) ose njé nivel referencé i miré-pércaktuar i afért me MSL.
1.3.3 Sistemet koordinative referencé té tjera
Si pérjashtime, ku mund t& pérdoren sisteme referencé té tjera nga ato té listuara né 1.3.1, 1.3.2 ose 1.3.3, jané:
1. Sisteme koordinative referencé t& tjera mund t& caktohen pér temat e t& dhénave hapésinore specifike né
kété Aneks.
2. Pér zonat (regjionet) qé ndodhen jashté kontinentit t& Europés, Shtetet Anétare (MS) mund t&
pércaktojné sisteme koordinative referencé t& pérshtatshme.
Kodet gjeodezike dhe parametrat e nevojshém pér pérshkrimin e kétyre sistemeve koordinative referencé dhe té
cilat lejojné veprimet e konvertimit dhe transformimit duhet t& dokumentohet dhe duhet té krijohet njé identifikues,
sipas EN ISO 19111 dhe ISO 19127.

1.4 Paragqitja

Sistemet koordinative referencé té pérdorura né shérbimin e shikimit té rrjetit
Pér shfagjen e grupeve t& t& dhénave hapésinore népérmjet shérbimit t& shikimit t& rrjetit si¢ specifikohet né
rregulloren nr. 976/2009, s& paku sistemet koordinative referencé pér koordinatat gjeodezike dy-dimensionale
(gjérésia, gjatésia) do té jené t& disponueshme.

1.5 Identifikuesit pér sistemet koordinative referencé

Identifikuesit e sistemeve koordinative referencé
1. Parametrat dhe identifikuesit e sistemit koordinativ referencé do t& menaxhohen né njé ose disa regjistra té
pérbashkét pér sistemet koordinative referencé.
2. Vetdm identifikuesit g8 pérmbajné njé regjistér t& pérbashkét do té pérdoren pér referimin tek sistemet
koordinative referencé té listuara né kété seksion.
3. Identifikuesit e listuar né tabelén 2 do té pérdoren pér referimin tek sistemet koordinative referencé té
pérdorura né njé grup t& dhénash.

Kéto udhézuese teknike propozojné pérdorimin e http URI-té té& ofruara nga Open Geospatial Consortium si
identifikues t& sistemit koordinativ referencé (shiko identifikuesit pér CRS-t& standard mé poshté). Kéto jané té
bazuara dhe t& drejtojné tek pérkufizimi né regjistrin e parametrave gjeodezik EPSG (http:/www.epsg-registry.org/).

Shénim: Identifikuesit e CRS mund t& pérdoren prsh né:

- Kodimin e té dhénave,
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- Metadatat e grupeve dhe shérbimeve té t& dhénave, dhe
- Kérkesat pér shérbimet e rrjetit t&¢ INSPIRE.

Tabela 2. http URI-té pér sistemet koordinative té referencés standarde:

Sistemi koordinativ referencé Shkurtimi Identifikuesi http URI
. . . http://mww.epsg-

Korniza Referuese Gjeodezike ;

. . KRGJSH_2010 registry.org/export htm?gml=urn:ogc:def:crs
Shgqiptare. ETRS89/ Abania 2010 \EPSC::6870
Kartezian 3D né ETRS89 ETRS89-XYZ http://www.opengis.net/def/crs/EPSG/0/4936
gggggme SDne ETRS8Omb | prpsgo.GRSSoR http:/)/ www.opengis.net/def/crs/EPSG/0/4937
Gjeodezike 2D né ETRS89 mbi
- | ETRS89-GRSS0 http:// www.opengis.net/deflcrs/ EPSG/0/4258
Projelsion LABAZD n¢ ETRS89 | prpggo 1 aABA http:// www.opengis.net/def/crs/EPSG/0/3035
mbi GRS80
Projeksion LCC 2D né ETRS89 . .
mbi GRSS0 ETRS89-LCC http:// www.opengis.net/def/crs/EPSG/0/3034
Projeksion TM 2D né ETRS89 mbi
GRS80, zona 34N (18°W deri ETRS89-TM34N http:// www.opengis.net/def/crs/EPSG/0/3046
24°W)
Lartési né EVRS EVRS http:// www.opengis.net/def/crs/EPSG/0/5730
3D t& kombinuara: Gjeodezike 2D
né ETRS89 mbi GRSS0, dhe ETRS89-GRS80-EVRS http:// www.opengis.net/def/crs/EPSG/0/7409
lartésité EVRS

C. SISTEMET REFERENCE TE PERKOHSHME

Sistemet referencé té pérkohshme
1. Sistemi referencé standard i pérkohshém ireferuar tek pika 5 e pjesés B t& Aneksit tek Rregullorja e Komisionit
(EC) nr. 1205/2008 () do t& pérdoret, pérveg rastit kur jané caktuar sisteme koordinative referencé té
pérkohshme t& tjera pér tema té t& dhénave hapésinore specifike né Aneksin II.

Shénim 1: Pika 5 e pjesés B e Aneksit t& Rregullores sé¢ Komisionit (EC) nr. 1205/2008 (IR-t& e metadatave t&
INSPIRE) thekson gé sistemi standard referencé do t& jets kalendari Gregorian, me datat e shprehura ng pérputhje me
ISO 8601.

Shénim 2: ISO 8601 Elementét e t¢ dhénave dhe formatet e shkémbimit — Shkémbimi i informacionit — Pasqyrimi i
datés dhé orés éshté njé standard ndérkombétar q& mbulon shkémbimin e té dhénave té lidhura datén dhe orén. Qéllimi
1 kétij standardi &shté qé té sigurojé njé metodé té qarté dhe t& miré-pércaktuar pér pasqyrimin e datés dhe orés, né
ményré qé t& shmangen keqinterpretimet e pasqyrimeve numerike t& datés dhe orés, veganérisht kur t& dhénat
transmetohen ndérmjet shteteve me konventa t& ndryshme pér shkrimin numerik té datés dhe orés. Standardi organizon
té dhénat né ményré q¢ termi mé i madh i pérkohshém (viti) shfaget fillimisht né t& dhéna varg dhe vazhdon deri te
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termi mé i vogél (sekondi). Ajo gjithashtu ofron njé metodé t& standardizuar pér komunikimin e informacionit t&
bazuar né kohé ndérmjet zonave kohore duke duke 1 dhéné njé spostim te Kohés Universale t& Koordinuar (UTC).

Shembull: 1997 (viti 1997);, 1997-07-16 (16 Korrik 1997); 1997-07-16T 19:20:30+01:00 (16 Korrik 1997, 199t 20min
30%k, zona kohore UTC+1).

D. NIJESITE E MATJEVE

Kérkesa dhe rregulla té tjera
2. Té gjitha vlerat e matjeve duhet t& shprehen népérmjet njésive SI ose jo-SI t& pranuara pér pérdorim me
Sistemin Ndérkombétar t& Njésive, pérvec kur specifikohet ndryshe pér tema apo tipe specifike t& t& dhénave
hapésinore.
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3.1.6. CILESIA E TE DHENAVE.

Ky kapitull pérfshin njé pérshkrim mbi cilésing e t& dhénave té elementéve dhe nén elementéve si dhe cilésiné e matjes
sé t& dhénave, qé duhen pérdorur pér té vlerésuar dhe dokumentuar cilésing e t& dhénave pér data setet qé lidhen me
té dhénat hapésinore t& temés Parcelat Kadastrale.

Kérkesé

Saktésia e materialeve hartografike, té cilat lidhen me tipologjiné e temés Parcelat Kadastrale, duhet té
plotésojné saktésiné ekzistuese té krijimit té kétyre materialeve, deri né momentin e krijimit dhe pércaktimit ¢
saktésisé sé Hartés pér Kadastrén Multifunksionale. Ndérsa harta bazé pér elementét e rinj gé do krijohen, do

té jeté produkti hartografik qé do té krijohet nga projekti i Fotografimit Ajror i vitit 2015.

Cilésia e té dhénave té elementéve, nén-elementéve dhe matjeve duhet t& pérdoret pér té:

e Specifikuar kérkesat apo rekomandimet lidhur me cilésing e té dhénave té rezultateve t& aplikueshme pér
data setet q& lidhen me t& dhénat hapésinore pér temén Parcelat Kadastrale.

e Vlerésuar dhe dokumentuar cilésing e elemenentéve t& metadatave té t& dhénave té dataseteve.

Né tabelén e méposhtme paragiten t& gjithé kérkesat pér cilésing e t& dhénave t& elementéve dhe nén elementéve &
pérmenden né kété standard. Informacioni i cilésisé sé t& dhénave vlerésohet né nivelin e objekteve hapésinore, llojet
e objekteve hapésinore, setet e té dhénave dhe serité e seteve.

Rekomandim:
Ku éshte e pamundur pér té shprehur vierésimin e njé elementi té cilésisé sé t& dhénave né ményré sasiore,
vierésimi i elementit duhet t¢ shprehet me njé deklaraté tekstuale si rezultat pérshkrues i cilésisé sé t¢ dhénave.

3.1.6.1. ELEMENTET E CILESISE SE TE DHENAVE:
Elementi i Nén-elementi i
Pjesa cilesise & cilésisé sé té Pérkufizimi Sferf‘ & .
dhénave dlicnave vlerésimit
3.1.6.1.1 | Kompletuar Pérjashtimi Te d].q?én?t © IMUNguara nga Objekt hapésinor
grupi i t& dhénave, si¢
pérshkruhen nga sfera
Lidhja e Koncepti I L N 3 Lloji i objektit
B-1.6.1.2 | géndrueshm géndrueshmérisé Respeltimi i regullave teskemes hapésinor; objekti
rigd konceptuale o
€nse hapésinor
Lidhjae Fusha B § . Lloji i objektit
peli6il.3 qéndrueshm géndrueshmérisé Respektlml ! vlere}ve & hapésinor; objekti
e territoreve té vlerés o
érisé hapésinor
1614 Sak_te_sla Sakte§1 absolute Afrimi me \{.lerat e koordl{lat?ve & Objekt hapésinor
pozicional ose e jashtme raportuara té pranuara si té vérteta
5 ose t€ vérteta
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Rekomandim:

Perjashtimi duhet té vierésohet dhe té dokumentohet duke pérdorur normén e artikujve té tepért & pércaktuara

né tabelat e méposhime.

KOPLETUAR — PERJASHTIMI. (COMPLETENESS — OMISSION)

Emri

Norma e artikujve té tepért

Emri alternativ

Cilésia e t& dhénave t& elementéve Kompletuar
Cilésia e t& dhénave t& nén-elementéve Pérjashtimi
Cilésia e t& dhénave t& matjeve themelore Shkalla e gabimit

Numri i artikujve t& hequr né setet e t& dhénave né lidhje me

Perlufizim numrin e artikujve gé duhet té ishin té pranishém.
Pérshkrim -

Fusha vlerésimit Objekte hapésinore

Fusha raportimit Objekte hapésinore

Parametér -

Cilésia e t& dhénave t& llojeve t& vlerave

Real, pérqindje, raport

Cilésia e t& dhénave t8 strukturés té vlerave

Burimi reference

ISO/DIS 19157 Geographic information — Data quality

Shembull -
Masa identifikuese 7
3.1.6.1:2. LOGIKA E QENDRUESHMERISE — KONCEPTI I QENDRUESHMERISE. (LOGICAL CONSISTENCY —

CONCEPTUAL CONSISTENCY)

Rekomandim:

Pér testet né géndrueshméring konceptuale, rekomandohet pér té pérdorur cilésiné e té dhénave té nén elementéve
t¢ ‘Logjika e gendrueshmérisé— Koncepti i géndrueshmérisé’ dhe masat e ‘Numri i artikujve jo né pérputhje me
rregullat e skemés konceptuale’ dhe ‘Numvri i mbivendosjeve t& paviefshme té sipérfageve’ té pércaktuara né

tabelat e mé poshté:

Emri

Numri i artikujve jo né pérputhje me rregullat ¢ skemés
konceptuale

Emri alternativ

Cilésia e t& dhénave t& elementéve

Logjika e géndrueshmérisé

Cilésia e t& dhénave t8 nén-elementéve

Koncepti i géndrueshmérisé

Cilésia e t& dhénave t& matjeve themelore

Numri i gabimit

Peérkufizim

Numérimin e t& gjithé artikujve né setet e t& dhénave té cilat
nuk jané né pérputhje me rregullat e skemés konceptuale.
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Pérshkrim

Nése skema konceptuale né ményré t& qarté ose té padyshimté
pérshkruan rregullat, kéto rregulla do t& ndigen. Shkeljet kundér
rregullave t& tilla mund té jeng, pér shembull, vendosja e
pavlefshme e tipologjive brenda njé tolerancé té caktuar,
dublikimi i elementéve dhe mbivendosjet té pavlefshme té& tyre.

Fusha vlerésimit

Objektet hapésinore, llojet e objekteve hapésinore

Fusha raportimit

Setet e t& dhénave

Parametér

Cilésia e t& dhénave t8 llojeve t& vlerave

Integer

Cilésia e t& dhénave t8 strukturés té vlerave

Burimi reference

ISO/DIS 19157 Geographic information — Data quality

Shembull -
Masa identifikuese 10
3.16.1.3. LOGIIKA E QENDRUESHMERISE — FUSHA E QENDRUESHMERISE. (LOGICAL CONSISTENCY —
DOMAIN CONSISTENCY)
Rekomandim:

Pér testet mbi fushén e qéndrueshmérisé, rekomandohet pér t& pérdorur cilésiné e té dhénave té nén elementéve

té ‘Logjika e géndrueshmérisé— Fusha e géndrueshmérisé’ dhe masat e Numri i artikujve jo né pérputhje me

fushen e tyre t& vierave’ dhe ‘Shkalla e pérputhjes sé vierave pér fushat’sic éshté specifikuar né tabelén e

méposhitme:

Emri

Numri i artikujve jo né pérputhje me fushén e tyre té
vlerave

Emri alternativ

Cilésia e t& dhénave t& elementéve

Logjika e géndrueshmérisé

Cilésia e t& dhénave t& nén-elementéve

Fusha e géndrueshmérisé

Cilésia e t&¢ dhénave t& matjeve themelore

Numri 1 gabimit

Pérkufizim

Numérimi i t& gjithé artikujve né setin e t& dhénave qé nuk jang
né pérputhje me fushén e tyre té vlerave

Pérshkrim

Fusha vlerésimit

Objektet hapésinore, llojet e objekteve hapésinore

Fusha raportimit

Setet e t& dhénave

Parametér

Cilésia e t& dhénave t& llojeve t& vlerave

Integer
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3.16.1.4
ACCURACY)

Rekomandim:

SAKTESIA E POZICIONIMIT — SAKTESIA ABSOLUTE APO E JASHTME. (ABSOLUTE OR EXTERNAL

Saktesia absolute ose e jashtme duhet té vierésohet dhe dokumentohet duke pérdorur emértimin e matjes( nga
ISO/DIS 19157) sig specifikohet né tabelat méposhté.

Emri

Gabimi mesatar kuadratik njési né planimetri

Emri alternativ

Cilésia e t& dhénave t& elementéve

Saktésia e pozicionimit.

Cilésia e t& dhénave t& nén-elementéve

Saktésia e jashtme apo absolute.

Cilésia e t& dhénave té matjeve themelore

Jo e aplikueshme

Pérkufizim

Rrezja e rrethit nga pika e dhéng, né té cilén vlera e verteté
shmanget me probabilitet P

Pérshkrim

Fusha vlerésimit

Objekt hapésinor

Fusha raportimit

Objekt hapésinor, setet e t& dhenave.

Parametér

Cilésia e t& dhénave t& llojeve té vlerave

Cilésia e t& dhénave t& strukturés té vlerave

Burimi reference

ISO/DIS 19157 Geographic information — Data quality

Shembull -
Masa identifikuese 28
Pjesa Elementi dhe nén-elementi Em”(at) Rezultati(et) Gjendja
i cilésisé sé t& dhénave :nea o objektive
st Shkalla e artikujve| Pér parcelat dhe zonat
B.1.6.1.1 |Kompletuar — Pérjashtimi i 0% kadastrale (nése ka)
» o Vlera mesatare e
31614 |Sektésiapozicionale w pasigurive Min. 16 cm Né zonat urbane
 —Sakiésia pozicionale(1D,
absolute e jashtme 2D)
. . Vlera mesatare e Ne +
B.1.614 |Sakiesia pozmlonaslek . pasigurive Min 40 cm ruiazlg/ri)au' Score
. —oakigsia pozicionale(1D, Bl
absolute e jashtme 2D)
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3.1.6.1.5. REKOMANDIME NE CILESINE E TE DHENAVE

Saktésia e hartés kadastrale

1. Saktésia e hedhjes né hartén kadastrale té parcelave dhe ndértesave, pércaktohet népérmjet llogaritjes sé vlerés sé:
e  Gabimit absolut né pércaktimin e pozicionit té pikés detaje (AL).

e Gabimit né pércaktimin e distancés midis dy pikave detaje (L).

2. Me “Gabim absolut né pércaktimin e pozicionit t& pikés detaje”, do t& kuptojmé madhésing:

AL = JE=K7 +( — %

Ku:
Xo, Yo — jané koordinatat e pikés né hartén kadastrale;
X, Y - jané koordinatat e s& nj&jtés pike, t& cilat jané pércaktuar népérmjet matjeve dhe llogaritjeve gjeodezike

gjaté kontrollit t& ushtruar né terren.
3. Me “Gabim né pércaktimin e distancés midis dy pikave detaje”, do té kuptojmé madhésing:

dL=L-Lo
Ku:
Lo — éshté distanca né hartén kadastrale midis dy pikave detaje, té zgjedhura rastésisht né té njéjtin objekt ose
nga objekte fginje.

L — &shté distanca e matur gjaté kontrollit né terren midis t& njéjtave pika té zgjedhura né hartén kadastrale.

4. Vlerat e lejuara pér AL dhe JL né qendrat e banuara jang:
a) Pér pikat kufitare t& parcelave dhe t& planimetrisé sé ndértesave me themele, té pércaktuara me matje

gjeodezike:
AL <= 16cm dhe L <= 10cm

5. Vlerat e lejuara pér AL dhe L jashté qendrave t& banuara jang:
a) Pér pikat kufitare t& parcelave dhe planeve t& ndértesave masive me themele, t& pércaktuara me matje

gjeodezike:
AL < =40cm dhe 0L <= 30cm
Ndryshimi i lejuar né pércaktimin e sipérfaqes sé parcelés

Ndryshimi i lejuar né pércaktimin e sipérfages sé parcelés qé pérftohet si diferencé midis sipérfages sé parcelés né
hartén kadastrale dhe sipérfaqes t& sé njéjtés parcelé té ripércaktuar nga kontrolli né terren, llogaritet me formulén:

AS=208LNS

Ku: JL — &shté gabimi né pércaktimin e distancés midis dy pikave detaje
S — éshté sipérfaqja e parcelés kadastrale e shprehur né m?.
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4. ANEKSE

4.1.

BASE
3132

3133

3134

3.1.3.5

3136

ANEKSE

Emri I elementit Anglisht

CadastralBoundary

BasicPropertyUnit

CadastralZoningLevelValu
e

CadastralParcel

CadastralZoning

GeographicalName
Identifier

AdministrativeUnits

KATALOGU I TIPOLOGIJISE

Emri I elementit Shqip

KufijtéKadastralg

NjésiaBazéEZonés

VleraENivelitTéZonésKad
astrale

ParcelatKadastrale

ZonatKadastrale

EmértimetGjeografike

Identifikues

KufijtéENjésive Administra
tive

Package

CadastralParcels

CadastralParcels
CadastralParcels

CadastralParcels

CadastralParcels

GeographicalName

Generic Conceptual
Model
AdministrativeUnit
s

Stereotypes

«featureType»

«featureType»
«codelist»

«featureType»

«featureType»

«featureType»
imported
«dataType»
imported
«featureType»
imported
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4.2. TE DHENAT E IMPORTUARA

A, Identifikues — (Identifier) - DataType

Kodilshtetit
Pérkufizim

Paketa
Referenca
Pérshkrim

Njé objekt identifikues i jashtém &shté njé identifikues unik i objektit t& publikuar
nga autoriteti pérgjegjés, 1 cili mund t& pérdoret nga aplikacionet e jashtme t&
referimit t& objektit hapésinor.

Base Type

INSPIRE Generic Conceptual Model, version 3.4 [DS-D2.5]

B.  Emértimet Gjeografike — (GeographicalName) - Feature Type

EmertimetGjeografike
Peérkufizim
Paketa
Referenca
Pérshkrim

Emértimi i sakté 1 vendosur njé elementi né realitet.
Geographical Names
INSPIRE Data specification on Geographical Names [DS-D2.8.1.3]

C.  Kufijté E Njésive Administrative — (AdministrativeUnits) -FeatureType

Kufijté ENjésiveAdministrative

Pérkufizim

Paketa
Referenca
Pérshkrim

Njésia administrative, kunjé shtet anétar ka dhe / ose ushtron té drejtat juridiksionale,
pér qeverisjen lokale, rajonale dhe kombétare.

AdministrativeUnits
INSPIRE Data specification on Administrative Units [DS-D2.8.1.4]
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4.3. KODI EPSG PER KRGISH 2010

s e cei st Rasicietom of Detailed Report on Projected

7 Oil and Gas Producers .
{ EPSG geodetic parsimaters Coordinate Reference Systems
’ data set version  8.5.4 Search Criteria: 6870
#1  Code: 0870 Name: ETRS89 / Albania 2010
Alhania alternative identifier : KRGISH-2010
Base GeogCRS: ETRSS9

Geodetic Datum: European Terrestrial Reference System 1989 Abbr Orientation
Ellipsoid: GRS 1980 1 Northing X north
2 Easting ¥ cast
CS remarks: Used in projected and engincering coordinate reference systems.
Semi-major axis fa) = 378137 metre
Inverse flattening (1) = 298 257222101 Mty Pecfpction:. ARem 2010
Projection Method: Transverse Mercator
Prime Meridian. Greenwich
’ cter Name er Value Init of .

Datum origin Fixed to the stable part of the Eurasian continental plate and Duasametst Lalu, Uniz of Measure

consistent with ITRS at the cpoch 1989.0. Latitude of natural origin 9 o 0" N
Datum remarks: The distinction in usage between ETRFS9 and ETRSS9 is Longitude of natural origin 20° 0 0" E

canﬁ!scd;:‘lhlhoug‘;:’ 7nn;::|¢ r‘um:cp(lﬂlly different in Senlo Tockor skl g ' o

0 ition.

practice are for the realisal Falas ensting 500000 metre
CRS scope: Large and medium scale topographic mapping. cadastral False northing 0 metre

and engincering survey.
CRS remarks. Planimetric component of Albanian Geodetic Reference Framework

(KRGISH) 2010.

Projection remarks: Planimetric component of Albanian Geodetic Reference Framework
(KRGISH) 2010.

CRS info. source. State Authority for Geospatial Information (ASIG). Data source: OGP Revision date: 18-Scp-14  Change id: 2014.008 2014.065
CRS area of use. 3212 Albania - onshore.

EPSG geodesy parameters. Version: 854  of I8 September 2014 Projected Coordinate Reference Systems (detailed) Printed on: 28-Oct-14 Page 1 of |
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